@@ 1
 
 
 
 
 
 
 
 
 
 
SanFran con0 is now available
@@

@@ 2
 




Press RETURN to get started.


SanFran>
@@

@@ 3
Password:
@@

@@ 4
SanFran#
@@

@@ 5
Exec commands:
  bfe              For manual emergency modes setting
  clear            Reset functions
  clock            Manage the system clock
  configure        Enter configuration mode
  connect          Open a terminal connection
  copy             Copy a config file to or from a tftp server
  debug            Debugging functions (see also 'undebug')
  disable          Turn off privileged commands
  disconnect       Disconnect an existing network connection
  enable           Turn on privileged commands
  erase            Erase flash or configuration memory
  exit             Exit from the EXEC
  help             Description of the interactive help system
  lat              Open a lat connection
  lock             Lock the terminal
  login            Log in as a particular user
  logout           Exit from the EXEC
  mbranch          Trace multicast route down tree branch
  mrbranch         Trace reverse multicast route up tree branch
  name-connection  Name an existing network connection
  no               Disable debugging functions
  pad              Open a X.29 PAD connection
  ping             Send echo messages
  ppp              Start IETF Point-to-Point Protocol (PPP)
  reload           Halt and perform a cold restart
  resume           Resume an active network connection
  rlogin           Open an rlogin connection
  rsh              Execute a remote command
  send             Send a message to other tty lines
  setup            Run the SETUP command facility
  show             Show running system information
  slip             Start Serial-line IP (SLIP)
  start-chat       Start a chat-script on a line
  systat           Display information about terminal lines
  telnet           Open a telnet connection
  terminal         Set terminal line parameters
  test             Test subsystems, memory, and interfaces
  tn3270           Open a tn3270 connection
  traceroute       Trace route to destination
  tunnel           Open a tunnel connection
  undebug          Disable debugging functions (see also 'debug')
  verify           Verify checksum of a Flash file
  where            List active connections
  which-route      Do OSI route table lookup and display results
  write            Write running configuration to memory, network, or terminal
  x3               Set X.3 parameters on PAD
  xremote          Enter XRemote mode
SanFran#
@@

@@ 6
 






SanFran con0 is now available





Press RETURN to get started.










SanFran>enable
Password:
@@

@@ 7
Cisco Internetwork Operating System Software
IOS (tm) 3000 Software (IGS-J-L), Version 11.1(11), RELEASE SOFTWARE (fc1)
Copyright (c) 1986-1996 by cisco Systems, Inc.
Compiled Mon 11-Mar-96 19:34 by tamb
Image text-base: 0x0302E6A8, data-base: 0x00001000

ROM: System Bootstrap, Version 5.2(8a), RELEASE SOFTWARE
ROM: 3000 Bootstrap Software (IGS-RXBOOT), Version 5.2(8a), RELEASE SOFTWARE (f
c1)

SanFran uptime is 1 week, 1 day, 18 hours, 56 minutes
System restarted by power-on
System image file is "flash:igs-j-l.103-10", booted via flash
@@

@@ 8
 
cisco 2500 (68030) processor (revision L) with 6144K/2048K bytes of memory.
Processor board serial number 02975066
SuperLAT software copyright 1990 by Meridian Technology Corp).
TN3270 Emulation software (copyright 1994 by TGV Inc).
X.25 software, Version 2.0, NET2, BFE and GOSIP compliant.
Bridging software.
Basic Rate ISDN software, Version 1.0.
1 Ethernet/IEEE 802.3 interface.
2 Serial network interfaces.
1 ISDN Basic Rate interface.
32K bytes of non-volatile configuration memory.
8192K bytes of processor board System flash (Read ONLY)

Configuration register is 0x2102
 
SanFran#
@@

@@ 9
SanFran#
@@
@@ 10
CPU utilization for five seconds: 2%/2%; one minute: 5%; five minutes: 5%
 PID Q T       PC Runtime (ms)    Invoked   uSecs   Stacks  TTY Process
   1 M *        0          680        117    5811 1126/2000   0 Exec
   2 L E  3040184     23182032     221024  104884  918/1000   0 Check heaps
   3 M E  30676AE        35800    5901120       6  632/1000   0 Timers
   4 L E  3096BFE           24         56     428  766/1000   0 ARP Input
   5 L E  30C06B2            0          1       0  924/1000   0 Probe Input
   6 M E  30C024A            0          1       0  962/1000   0 RARP Input
   7 H E  30B294C       154936     283490     546 1610/2000   0 IP Input
   8 M E  30D9192         1608     161219       9  728/1000   0 TCP Timer
   9 L E  30DAE6E           16         17     941  686/1000   0 TCP Protocols
  10 M E  30BD382            0          1       0  796/1000   0 BOOTP Server
  11 M E  3118FFC        38668     117832     328  830/1000   0 CDP Protocol
  13 L T  318A9A2           56      12658       4  930/1000   0 IP Cache Ager
  14 M E  322B58E           40          4   10000 1724/2000   0 SNMP Traps
  15 M E  3036610          360        206    1747  680/1000   0 Net Background
  16 L E  30618D0           44         84     523  868/1000   0 Logger
  17 M P  3040EB2       335288     759477     441  686/1000   0 TTY Background
  18 H E  30368C2        39016     209504     186  372/500    0 Net Input
  19 M P  3036544       304348      12658   24043  736/1000   0 Per-minute Jobs
  20 M E  31AEC56         3824      12243     312  840/1000   0 OSPF Hello
  21 M E  31795C0         1028      12679      81  924/1000   0 IP-RT Background
  22 M E  31AE864         1184        695    1703  928/1500   0 OSPF Router
@@
@@ 11
 PID Q T       PC Runtime (ms)    Invoked   uSecs   Stacks  TTY Process
  --More--
SanFran#
@@

@@ 12
SanFran#show processes
@@

@@ 13
SanFran#
@@

@@ 14
               Head  FreeList    Total(b)     Used(b)     Free(b)  Largest(b)
Processor     5FE24     2E958     5894620      662644     5231976     5221884
      I/O    600000     2F628     2097152      397268     1699884     1699348

          Processor memory

 Address  Bytes Prev.    Next     Ref  PrevF   NextF   Alloc PC  What
5FE24        24 0        5FE60      1                  311F522   *Init*
5FE60      2508 5FE24    60850      1                  3050D18   TTY data
60850      2000 5FE60    61044      1                  3052E36   TTY Input Buf
61044       512 60850    61268      1                  3052E66   TTY Output Buf
61268      2000 61044    61A5C      1                  30410A2   *Init*
61A5C      2000 61268    62250      1                  3079594   OSPF Router
62250       104 61A5C    622DC      1                  352F234   Router Init
622DC       104 62250    62368      1                  352F234   Router Init
62368       104 622DC    623F4      1                  352F234   Router Init
623F4       104 62368    62480      1                  352F234   Router Init
62480       104 623F4    6250C      1                  352F234   Router Init
6250C        60 62480    6256C      1                  3067580   Router Init
6256C        60 6250C    625CC      1                  3067580   Router Init
625CC        60 6256C    6262C      1                  3067580   Router Init
6262C        60 625CC    6268C      1                  3067580   Router Init
6268C        24 6262C    626C8      1                  30A9392   Router Init
626C8        52 6268C    62720      1                  30A9392   Router Init
62720        96 626C8    627A4      2                  31FDFFC   IP-EIGRP Router

 Address  Bytes Prev.    Next     Ref  PrevF   NextF   Alloc PC  What
627A4       520 62720    629D0      0  0       0       305262A   (coalesced)
629D0        28 627A4    62A10      1                  30412A2   *Sched*
62A10        64 629D0    62A74      1                  3181840   IP Input
62A74       100 62A10    62AFC      1                  3119488   CDP Protocol
62AFC        24 62A74    62B38      1                  3089376   *Init*
62B38      2508 62AFC    63528      1                  303BAE2   *Init*
63528      3440 62B38    642BC      1                  3040286   Reg Service
642BC      2040 63528    64AD8      1                  3040286   Reg Function
64AD8      1152 642BC    64F7C      1                  304A07C   Registry
64F7C      1152 64AD8    65420      1                  304A07C   Registry
65420      1152 64F7C    658C4      1                  304A07C   Registry
658C4      1152 65420    65D68      1                  304A07C   Registry
65D68       720 658C4    6605C      1                  304A07C   Registry
6605C      1152 65D68    66500      1                  304A07C   Registry
66500      1152 6605C    669A4      1                  304A07C   Registry
669A4      1152 66500    66E48      1                  304A07C   Registry
66E48      1152 669A4    672EC      1                  304A07C   Registry
672EC      1152 66E48    67790      1                  304A07C   Registry
67790      1152 672EC    67C34      1                  304A07C   Registry
67C34      1152 67790    680D8      1                  304A07C   Registry
680D8      1152 67C34    6857C      1                  304A07C   Registry
6857C      3440 680D8    69310      1                  3040286   Reg Service
@@

@@ 15
 

          I/O memory

 Address  Bytes Prev.    Next     Ref  PrevF   NextF   Alloc PC  What
600000      264 0        60012C     1                  302F62E   *Packet Data*
60012C      264 600000   600258     1                  302F62E   *Packet Data*
600258      264 60012C   600384     1                  302F62E   *Packet Data*
600384      264 600258   6004B0     1                  302F62E   *Packet Data*
6004B0      264 600384   6005DC     1                  302F62E   *Packet Data*
6005DC      264 6004B0   600708     1                  302F62E   *Packet Data*
600708      264 6005DC   600834     1                  302F62E   *Packet Data*
600834      264 600708   600960     1                  302F62E   *Packet Data*
600960      264 600834   600A8C     1                  302F62E   *Packet Data*
600A8C      264 600960   600BB8     1                  302F62E   *Packet Data*
600BB8      264 600A8C   600CE4     1                  302F62E   *Packet Data*
600CE4      264 600BB8   600E10     1                  302F62E   *Packet Data*
600E10      264 600CE4   600F3C     1                  302F62E   *Packet Data*
600F3C      264 600E10   601068     1                  302F62E   *Packet Data*
601068      264 600F3C   601194     1                  302F62E   *Packet Data*
601194      264 601068   6012C0     1                  302F62E   *Packet Data*
6012C0      264 601194   6013EC     1                  302F62E   *Packet Data*
6013EC      264 6012C0   601518     1                  302F62E   *Packet Data*
@@

@@ 16
BRI0 is administratively down, line protocol is down
  Hardware is BRI
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec, rely 255/255, load 1/255
  Encapsulation HDLC, loopback not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Output queue 0/40, 0 drops; input queue 0/75, 0 drops
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets, 0 restarts
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
 --More--
@@

@@ 17
Ethernet0 is up, line protocol is up
  Hardware is Lance, address is 0000.0c8d.c30d (bia 0000.0c8d.c30d)
  Internet address is 172.16.128.1 255.255.255.0
  MTU 1500 bytes, BW 10000 Kbit, DLY 1000 usec, rely 255/255, load 1/255
  Encapsulation ARPA, loopback not set, keepalive set (10 sec)
  ARP type: ARPA, ARP Timeout 4:00:00
  Last input 0:00:04, output 0:00:00, output hang never
  Last clearing of "show interface" counters never
  Output queue 0/40, 0 drops; input queue 0/75, 0 drops
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     85565 packets input, 13504437 bytes, 0 no buffer
     Received 85527 broadcasts, 0 runts, 0 giants
     13 input errors, 13 CRC, 4 frame, 0 overrun, 0 ignored, 0 abort
     0 input packets with dribble condition detected
     191795 packets output, 16578873 bytes, 0 underruns
     5 output errors, 1492 collisions, 9 interface resets, 0 restarts
     0 output buffer failures, 0 output buffers swapped out
 --More--
@@

@@ 18
Serial0 is up, line protocol is up
  Hardware is HD64570
  Internet address is 172.16.65.2 255.255.255.0
  MTU 1500 bytes, BW 1544 Kbit, DLY 20000 usec, rely 255/255, load 1/255
  Encapsulation HDLC, loopback not set, keepalive set (10 sec)
  Last input 0:00:06, output 0:00:01, output hang never
  Last clearing of "show interface" counters never
  Output queue 0/40, 0 drops; input queue 0/75, 0 drops
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     212236 packets input, 13370212 bytes, 0 no buffer
     Received 99219 broadcasts, 0 runts, 0 giants
     134 input errors, 1 CRC, 0 frame, 0 overrun, 6 ignored, 1 abort
     204364 packets output, 12853535 bytes, 0 underruns
     0 output errors, 0 collisions, 143 interface resets, 0 restarts
     0 output buffer failures, 0 output buffers swapped out
     106 carrier transitions
     DCD=up  DSR=up  DTR=up  RTS=up  CTS=up
 --More--
@@

@@ 19
Serial1 is up, line protocol is up
  Hardware is HD64570
  Internet address is 172.16.67.1 255.255.255.0
  MTU 1500 bytes, BW 1544 Kbit, DLY 20000 usec, rely 255/255, load 1/255
  Encapsulation HDLC, loopback not set, keepalive set (10 sec)
  Last input 0:00:00, output 0:00:02, output hang never
  Last clearing of "show interface" counters never
  Output queue 0/40, 0 drops; input queue 0/75, 0 drops
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     223335 packets input, 14250542 bytes, 0 no buffer
     Received 110467 broadcasts, 0 runts, 0 giants
     2 input errors, 1 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     202503 packets output, 12876815 bytes, 0 underruns
     0 output errors, 0 collisions, 4 interface resets, 0 restarts
     0 output buffer failures, 0 output buffers swapped out
     96 carrier transitions
     DCD=up  DSR=up  DTR=up  RTS=up  CTS=up
 --More--
@@

@@ 20
Global values:
  Internet Protocol routing is enabled
BRI0 is administratively down, line protocol is down
Ethernet0 is up, line protocol is up
  Internet address is 172.16.128.1 255.255.255.0
Serial0 is up, line protocol is up
  Internet address is 172.16.65.2 255.255.255.0
Serial1 is up, line protocol is up
  Internet address is 172.16.67.1 255.255.255.0
SanFran#
@@

@@ 21
CPU utilization for five seconds: 12%/1%; one minute: 5%; five minutes: 5%
 PID Q T       PC Runtime (ms)    Invoked   uSecs   Stacks  TTY Process
   1 M *        0          612        104    5884 1136/2000   2 Exec
   2 L E  3040184     23197148     221168  104884  918/1000   0 Check heaps
   3 M E  30676AE        35808    5901275       6  632/1000   0 Timers
   4 L E  3096BFE           24         56     428  766/1000   0 ARP Input
   5 L E  30C06B2            0          1       0  924/1000   0 Probe Input
   6 M E  30C024A            0          1       0  962/1000   0 RARP Input
   7 H E  30B294C       154964     283612     546 1610/2000   0 IP Input
   8 M E  30D9192         1608     161319       9  728/1000   0 TCP Timer
   9 L E  30DAE6E           16         17     941  686/1000   0 TCP Protocols
  10 M E  30BD382            0          1       0  796/1000   0 BOOTP Server
  11 M E  3118FFC        38712     117899     328  830/1000   0 CDP Protocol
  13 L T  318A9A2           56      12666       4  930/1000   0 IP Cache Ager
  14 M E  322B58E           40          4   10000 1724/2000   0 SNMP Traps
  15 M E  3036610          360        206    1747  680/1000   0 Net Background
  16 L E  30618D0           44         84     523  868/1000   0 Logger
  17 M P  3040EB2       335508     759980     441  686/1000   0 TTY Background
  18 H E  30368C2        39080     209645     186  372/500    0 Net Input
  19 M P  3036544       304564      12667   24043  736/1000   0 Per-minute Jobs
  20 M E  31AEC56         3844      12343     311  840/1000   0 OSPF Hello
  21 M E  31795C0         1028      12687      81  924/1000   0 IP-RT Background
  22 M E  31AE864         1192        700    1702  928/1500   0 OSPF Router
@@

@@ 22
SanFran#
@@
@@ 23
 






SanFran con0 is now available





Press RETURN to get started.
@@

@@SCRL 020301
SanFran>______________________
@@SCRL

@@SCRL 020302
SanFran#_______________________
@@SCRL

@@SCRL 020303
SanFran#_______________________
@@SCRL

@@SCRL 020304
SanFran>________________________
@@SCRL

@@SCRL 020401
SanFran#________________________
@@SCRL

@@SCRL 020403
SanFran#________________________
@@SCRL

@@SCRL 020405
SanFran#__________________________
@@SCRL

@@SCRL 020407
SanFran#_____________________________
@@SCRL

@@SCRL 020408
SanFran#_______________________________
@@SCRL
