@@QUES 040101 T/F Q,4,436,339,272   
Do you think the following statement is true or false?

It also defines the area ID for this interface.
|
1
|

|
That's right.
|
In fact, it does.
|
The statement is true.

@@QUES 040102 Y/N Q,21,440,222,252
Do you think the SanFran router is an ABR?
|
1
|

|
You're right.
|
In fact, it is.
|
The answer is Yes.

@@QUES 040103 Y/N Q,184,382,256,278
Do you think you need to be in privileged mode in order to configure the London router?
|
1
|

|
You're right.
|
In fact, you do.
|
The answer is Yes.

@@QUES 040104 SXY Q,323,437,289,318
Which of the following do you think you do next?
|
Choose an option.
|
You press @UCTRL+Z@u to exit configuration mode
You specify the address range for area 1 for summarization
You type @Rexit@r
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040201 SFB Q,390,387,228,197
See if you can supply the command to log on to the Dublin router using Telnet.

|
Type your answer.
|

|
%008dublin, telnet dublin, telnet 172.16.66.2, telnet 172.16.67.2
|
That's right.
|
Yes, but the word used here is "".
|
Try again.
|

|

|

|

|
That's not the word required here. Try again.
|
The answer is "dublin".
|
The answer is now shown.

@@QUES 040202 T/F Q,381,430,234,287
Do you think the following statement is true or false?

You can configure the router in User mode.
|
2
|

|
That's right.
|
Actually, you need to be in Privileged mode.
|
The statement is false.

@@QUES 040203 SFB Q,400,344,218,217
See if you can supply the command to enter into Configuration mode on the Dublin router.

|
Type your answer.
|

|
config,configure,conf
|
That's right.
|

|
Yes, but the word used here is "".
|
Try again.
|

|

|

|
That's not the word required here. Try again.
|
The answer is "config".
|
The answer is now shown.

@@QUES 040204 SFB Q,372,412,241,210
See if you can supply the command to enable OSPF routing on this router using a process ID of 59.

|
Type your answer.
|

|
router ospf 59
|
That's right.
|
Yes, but the word used here is "".
|
Try again.
|

|

|

|

|
That's not the word required here. Try again.
|
The answer is "router ospf 59".
|
The answer is now shown.

@@QUES 040205 SYF Q,263,455,359,285
Which of the following commands configures the network with the address 172.16.66.0 on area 0 for OSPF?
|
Choose an option.
|
%010router 172.16.66.0 0.0.0.255 area 0
%010network 172.16.66.0 0.0.0.255 area 0
%010network area 0 172.16.66.0 0.0.0.255
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040206 SFB Q,42,438,256,240
See if you can complete the line of code to configure the third network on the Dublin router. (Its address is 172.16.192.0 and it is in area 2.)

|
Type your answer.
|

|
area 2
|
That's right.
|
Yes, but the word used here is "".
|
Try again.
|

|

|

|

|
That's not the word required here. Try again.
|
The answer is "area 2".
|
The answer is now shown.

@@QUES 040207 SDF Q,325,437,295,333
Try to decide which part of the command goes in which blank to complete the command that specifies the address range for area 2.

|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
range
area
|
2
|
That's right.
|
In fact, it's the other way around.
|
Incorrect.
|
Incorrect.
|
The full statement is now shown.

@@QUES 040208 T/F Q,52,425,296,318
Do you think the following statement is true or false?

This command configures route summarization between area 0 and area 2.
|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 040209 SXY Q,355,420,263,267
What key(s) do you press to exit Configuration mode?
|
Choose an option.
|
ESC
CTRL+Z
ALT+X
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040210 SFB Q,393,396,222,213
Can you supply the command to log into the Sydney router using its address 172.16.65.1 ?

|
Type your answer.
|

|
%008telnet 172.16.65.1,172.16.65.1
|
That's right.
|
telnet sydney, sydney
|
Yes, but using its address the command would by "telnet 172.16.65.1".
|
Try again.
|

|

|

|
That's not the word required here. Try again.
|
The answer is "telnet 172.16.65.1".
|
The answer is now shown.
@@QUES 040211 SYF Q,354,419,272,319
Which of the following commands would you use to enable OSPF routing on the Sydney router?
|
Choose an option.
|
%010router ospf
%010ospf router 59
%010router ospf 59
%010ospf 59
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040212 SFB Q,363,329,245,191
See if you can complete the command to configure the first network.

|
Type your answer.
|

|
network,net,netw,netwo,networ
|
That's right.
|
Yes, but the word used here is "".
|
Try again.
|

|

|

|

|
That's not the word required here. Try again.
|
The answer is "network".
|
The answer is now shown.

@@QUES 040213 SFB Q,383,366,225,201
See if you can supply the command to save the configuration in NVRAM.

|
Type your answer.
|

|
copy runn start,copy running-config startup-config,copy run start
|
That's right.
|
Yes, but the word used here is "".
|
Try again.
|

|

|

|

|
That's not the word required here. Try again.
|
The answer is "copy runn start".
|
The answer is now shown.

@@QUES 040301 FIB Q,329,438,275,205
How many interfaces do you think the SanFran router has in the backbone area? _____
|
Type your answer.
|

|
2,two
|
That's right.
|

|
Try again.
|

|

|

|

|
That's not the answer required here. Try again.
|
The answer is "two".
|
The answer is now shown.

@@QUES 040302 DTF Q,351,457,278,339
Try to decide which option goes in which blank.

The SPF algorithm has executed in area 4  _  times and in the backbone area  _  times.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
%010six
%010three
|
2
|
That's right.
|
In fact, it's the other way around.
|
Incorrect.
|
Incorrect.
|
The full statement is now shown.

@@QUES 040303 FIB Q,321,282,286,203
How many addresses do you think the router has identified as belonging to itself?  ______
|
Type your answer.
|

|
three,3
|
That's right.
|
Try again.
|

|

|

|

|

|
That's not the answer required here. Try again.
|
The answer is "three".
|
The answer is now shown.

@@QUES 040304 SXY Q,376,406,237,303
How many networks do you think OSPF is routing for?
|
Choose an option.
|
Two
Three
Four
Five
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040305 Y/N Q,388,315,225,254
Do you think that this update was acknowledged?
|
1
|

|
You're right.
|
In fact, it was.
|
The answer is Yes.

@@QUES 040401 SFB Q,311,428,301,220
See if you can complete the command to display general information about the OSPF routing process on the Sydney router.

|
Type your answer.
|
The routing protocol in use is OSPF.
|
ospf
|
That's right.
|

|

|

|

|

|

|
That's not the word required here. Try again.
|
The answer is "ospf".
|
The answer is now shown.

@@QUES 040402 SFB Q,312,359,297,209
Now see if you can complete the command to display the current state of the routing table for this router.

|
Type your answer.
|

|
route
|
That's right.
|

|

|

|

|

|

|
That's not the word required here. Try again.
|
The answer is "route".
|
The answer is now shown.



@@QUES 040403 SFB Q,346,419,267,220
See if you can complete the command to display the parameters and current state of the active routing process.

|
Type your answer.
|

|
protocol,prot,proto
|
That's right.
|

|

|

|

|

|

|
That's not the word required here. Try again.
|
The answer is "protocol".
|
The answer is now shown.

@@QUES 040404 SFB Q,356,308,228,193
Now type the command to turn on OSPF debugging.
|
Type your answer.
|

|
%007debug ip ospf events,de ip ospf ev,de ip os ev
|
That's right.
|

|

|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "debug ip ospf events".
|
The answer is now shown.

@@QUES 040405 SFB Q,404,450,213,193
What command do you think would let you see border routers?
|
Type your answer.
|

|
%007show ip ospf border-routers
|
That's right.
|

|

|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "show ip ospf border-routers".
|
The answer is now shown.

@@QUES 040101t T/F Q,144,381,309,309
Is the following statement true or false?

The command you use to specify the address range configures route summarization on the router.
|
1
|
10
|
Correct.
|
Incorrect. The statement is true.

@@QUES 040102t Y/N Q,0,0,269,268
If your company has only one network address, can you divide your network into different areas?
|
1
|
10
|
Correct.
|
Incorrect. The answer is Yes.

@@QUES 040103t SXY Q,139,409,391,340
Which of the following commands defines the address 172.16.65.0 as an OSPF network in area 0?
|
Choose an option.
|
%010@Rnetwork 172.16.65.0 area 0@r
%010@Rinterface area 0 172.16.65.0 0.0.0.255@r
%010@Rnetwork 172.16.65.0 0.0.0.255 area 0@r
%010@Rrange 172.16.65.0 0.0.0.255 area 0@r
|
3
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 040104t SXY Q,130,399,357,320
Which of the following commands would you use to specify the address range for area 4?
|
Choose an option.
|
%010@Rrange area 4 172.16.128.0 255.255.255.0@r
%010@Rarea 4 range 172.16.128.0 255.255.128.0@r
%010@Rnetwork area 4 172.16.128.0@r
%010@Rarea 4 172.16.128.0 255.255.255.0@r
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 040301t SXY Q,137,383,366,305
Which of the following commands would you use to view the current state of the routing table?
|
Choose an option.
|
%010@Rshow IP Routing Table@r
%010@Rshow IP Route@r
%010@Rshow IP Protocol@r
%010@Rshow IP OSPF@r
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 040302t SXY Q,153,383,308,301
Which of the following commands would you use to find out which routing protocol was in operation on a router?
|
Choose an option.
|
%010@Rshow IP Protocol@r
%010@Rshow IP Route@r
%010@Rshow IP Update@r
|
1
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 040303t SXY Q,0,0,273,302
Which of the following commands could tell you how many times the SPF has executed on a router?
|
Choose an option.
|
%010@Rshow IP Protocol@r
%010@Rshow IP Route@r
%010@Rshow IP OSPF@r
|
3
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.
|

|

|
