@@QUES 020101 MXY Q,286,453,268,350
For which of the following routing protocols do you think the IP implementation of Enhanced E-IGRP can redistribute routes?

|
Choose each appropriate item.
|
OSPF
IP RIP
IS-IS
EGP
BGP
|

|
1,2,3,4,5
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. All the options are correct and are now highlighted.
|
All the options are correct and are now highlighted.

@@QUES 020102 T/F Q,229,445,293,324
Do you think the following statement is true or false?

A router that is sending updates for several different routing protocols is very demanding of bandwidth.

|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.

@@QUES 020103 SXY Q,253,454,263,290
To which routers do you think a router running E-IGRP sends updates?

|
Choose an option.
|
All routers
Adjacent routers
Affected routers
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020104 T/F Q,8,452,253,320
Do you think the following statement is true or false?

Enhanced IGRP routers and IGRP routers can easily exchange routing information.

|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 020105 T/F Q,4,452,253,345
Do you think the following statement is true or false?

To achieve minimal disruption you should begin by adding Enhanced IGRP at the core of the network and then work outwards to the periphery.
|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.

@@QUES 020106 XYF Q,246,448,314,330
See if you can choose the correct option to fill in the blank.

The routers then have both an IGRP and an E-IGRP process active, _ .

|
Choose an option to fill the blank.
|
%010sharing the same AS number
%010using different AS numbers
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020201 T/F Q,6,432,291,299
Do you think the following statement is true or false?

In order to configure the routers you must be in Privileged mode.

|
1
|

|
That's right.
|
In fact, you must.
|
The statement is true.

@@QUES 020202 SXY Q,35,422,279,292
Which of the following key presses do you think you use to exit configuration mode?

|
Choose an option.
|
£UAlt+X£u
£UCtrl+Z£u
£UEsc£u
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020203 Y/N Q,82,412,257,271
Do you think you must be in Configuration mode in order to configure the London router?

|
1
|

|
You're right.
|
In fact, you must.
|
The answer is Yes.

@@QUES 020204 SXY Q,117,434,276,346
Which of the following do you think you do next?

|
Choose an option.
|
You type exit to return to the SanFran router
You press Ctrl+Z to exit Configuration mode
You enter £Rcopy runn start£r to save the configuration in NVRAM
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020301 SFB Q,388,438,231,194
See if you can supply the command to log on to the Dublin router using Telnet.

|
Type your answer.
|

|
%007dublin,%007telnet dublin,%007telnet 172.16.66.2,%007telnet 172.16.67.2
|
That's right.
|
Yes, but the command used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "dublin".
|
The answer is now shown.

@@QUES 020302 SFB Q,377,352,233,212
See if you can supply the command to enter into Configuration mode on the Dublin router.

|
Type your answer.
|

|
%007config, configure
|
That's right.
|
Yes, but the command used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "config".
|
The answer is now shown.

@@QUES 020303 SFB Q,341,447,287,213
See if you can supply the command to enable Enhanced IGRP routing on this router using an AS number of 109.

|
Type your answer.
|

|
%007router eigrp 109
|
That's right.
|
Yes, but the commandd used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "router eigrp 109".
|
The answer is now shown.

@@QUES 020304 SYF Q,342,439,281,309
Which of the following commands define the networks with which the Dublin router interfaces?
|
Choose an option.
|
%010router 172.16.0.0
%010network 172.16.0.0
%010network area 0 172.16.0.0
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020305 SXY Q,43,441,313,288
How do you log out of the Dublin router?
|
Choose an option.
|
Type £Rexit£r
Press £UCtrl+Z£u
Press £UEsc£u
Type £Rtelnet SanFran£r
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020306 SFB Q,326,442,293,196
See if you can supply the command to log into the Sydney router using its address 172.16.65.1.

|
Type your answer.
|

|
%007telnet 172.16.65.1
|
That's right.
|
telnet sydney, sydney
|
Yes, but using its address the command would by "telnet 172.16.65.1".
|
Try again.
|

|

|

|
That's not the command required here. Try again.
|
The answer is "telnet 172.16.65.1".
|
The answer is now shown.

@@QUES 020307 SYF Q,306,455,307,320
Which of the following commands would you use to enable Enhanced IGRP routing on the Sydney router?
|
Choose an option.
|
%010router e-igrp
%010eigrp router 109
%010router eigrp 109
%010eigrp 109
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020308 SFB Q,334,283,297,208
See if you can complete the command to define the networks with which the Sydney router interfaces.

|
Type your answer.
|

|
%007network,%007net
|
That's right.
|
Yes, but the command used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "network".
|
The answer is now shown.

@@QUES 020309 SFB Q,334,439,277,192
See if you can supply the command to save the configuration in NVRAM.

|
Type your answer.
|

|
%007copy runn start,%007copy running-config startup-config
|
That's right.
|
Yes, but the command used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "copy runn start".
|
The answer is now shown.

@@QUES 020101t MXY Q,145,414,377,350
Which of the following statements is/are true?

|
Choose each appropriate item.
|
You can use Enhanced IGRP to integrate several existing networks that are using different routing protocols
The IP implementation of Enhanced IGRP supports variable length subnet masks (VLSMs)
Enhanced IGRP is very demanding of bandwidth
|
1,2
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 020102t MXY Q,119,415,401,350
Which of the following statements is/are true?

|
Choose each appropriate item.
|
Enhanced IGRP uses a single metric to determine the best path to a destination
Enhanced IGRP routers use a metric structure similar to that used by IGRP routers
Enhanced IGRP routers and IGRP routers cannot exchange routing information
|
2
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The only correct option is now highlighted.
|
You have not made any correct choices. The only correct option is now highlighted.

@@QUES 020103t SXY Q,0,0,350,350
In which of the following cases is route redistribution between routers automatic?

|
Choose an option.
|
When the two routers are in the same autonomous system
When the two routers are in different autonomous systems
|
1
|
10
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020104t MXY Q,0,0,350,350
Which of the following network level routing protocols does Enhanced IGRP support?

|
Choose each appropriate item.
|
AppleTalk RTMP
IPX RIP
IP RIP
|
1,2,3
|
21
|
Correct.
|
7 per correct decision
|
Partly right. All the options are correct and are now highlighted.
|
You have not made any correct choices. All the options are correct and are now highlighted.

@@QUES 020201t SXY Q,0,0,350,350
Once an Enhanced IGRP process is started which of the following commands is used to define the networks with which a router running Enhanced IGRP interfaces?

|
Choose an option.
|
%010router eigrp 172.16.0.0
%010network 172.16.0.0
%010eigrp 172.16.0.0
|
2
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020202t MXY Q,0,0,350,350
Which of the following statements is/are true?

|
Choose each appropriate item.
|
You must be in Privileged mode in order to configure a router
You must be in Configuration mode in order to configure a router
You can configure routers remotely using Telnet
|
1,2,3
|
21
|
Correct.
|
7 per correct decision
|
Partly right. All the options are correct and are now highlighted.
|
You have not made any correct choices. All the options are correct and are now highlighted.
|
|
|
|
|
|

