@@QUES 030101 T/F Q,158,438,303,340
Do you think the following statement is true or false?

You use the Passive-Interface command to prevent routing protocol updates from being generated on the interface.

|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 030102 XYF Q,241,447,324,332
See if you can choose the correct option to fill in the blank.

You use  _______________  to filter routing updates on one or more interfaces.

|
Choose an option to fill the blank.
|
%010the Distribute-List command
Access Lists
Masks
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030103 SXY Q,243,446,305,332
What do you think happens if no interface is specified?

|
Choose an option.
|
You are prompted to specify an interface
The default interface is selected
The access list is applied to all incoming updates
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 030104 T/F Q,216,446,299,300
Do you think the following statement is true or false?

As a result, network 10.0.0.0 is hidden.

|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 030105 XYF Q,154,442,279,350
See if you can choose the correct option to fill in the blank.

The  ________  keyword allows traffic matching the parameters to be forwarded.

|
Choose an option to fill the blank.
|
ŁUPermitŁu
ŁUConnectedŁu
ŁUForwardŁu
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030106 T/F Q,244,447,293,306
Do you think the following statement is true or false?

The Distribute-List command is used with access lists to redistribute routing information.

|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 030107 T/F Q,149,440,296,316
Do you think the following statement is true or false?

This configuration redistributes routing information only from network 10.0.0.0.

|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.

@@QUES 030108 XYF Q,137,419,307,350
See if you can choose the correct option to fill in the blank.

You define a static route using the  _________  command.

|
Choose an option to fill the blank.
|
IP Route
Show IP Route
Static Route
Define Static Route
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030109 SXY Q,199,313,280,282
Where does it redistribute them to?

|
Choose an option.
|
IGRP
OSPF
RIP
Enhanced IGRP
|

|
4
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 030201 MXY Q,263,444,304,350
What benefits do you think route summarization provides?

|
Choose each appropriate item.
|
It reduces the load on the router
It reduces the perceived complexity of the network
It prevents routing updates from being generated on the interface
|

|
1,2
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 030202 Y/N Q,163,299,267,240
Do you think you can turn off automatic route summarization?

|
1
|

|
You're right.
|
In fact, the answer is Yes.
|
The answer is Yes.

@@QUES 030203 XYF Q,148,433,276,321
See if you can choose the correct option to fill in the blank.

In this configuration routes will be  ___________  summarized at the Serial 0 interface.

|
Choose an option to fill the blank.
|
%010manually
%010automatically
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030301 SFB Q,289,348,319,196
See if you can complete the command to display general information about the Enhanced IGRP routing process.

|
Type your answer.
|
The routing protocol in use is Enhanced IGRP.
|
%008eigrp
|
That's right.
|

|
Yes, but the command used here is "".
|

|
Try again.
|

|

|
That's not the command required here. Try again.
|
The answer is "eigrp".
|
The answer is now shown.

@@QUES 030302 SFB Q,340,368,262,209
Now see if you can complete the command to display the current state of the routing table for this router.

|
Type your answer.
|

|
%008route
|
That's right.
|

|
Yes, but the command used here is "".
|

|
Try again.
|

|

|
That's not the command required here. Try again.
|
The answer is "route".
|
The answer is now shown.

@@QUES 030303 SFB Q,293,360,317,191
See if you can complete the command to display the parameters and current state of the active routing process.

|
Type your answer.
|

|
%008protocol
|
That's right.
|

|
Yes, but the command used here is "".
|

|
Try again.
|

|

|
That's not the command required here. Try again.
|
The answer is "protocol".
|
The answer is now shown.

@@QUES 030304 SFB Q,340,352,271,177
Now type the command to turn on Enhanced IGRP debugging.

|
Type your answer.
|

|
%008debug ip-eigrp events
|
That's right.
|

|
Yes, but the command used here is "".
|

|
Try again.
|

|

|
That's not the command required here. Try again.
|
The answer is "debug ip-eigrp events".
|
The answer is now shown.

@@QUES 030101t MXY Q,145,414,359,350
What are the methods that can be used to minimize routing updates?

|
Choose each appropriate item.
|
Filtering routing updates with access lists
Using redistribution with a distribute list to minimize advertised routes
Eliminating the routing protocol Network command for an interface with an address from a separate network
|
1,2,3
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 030102t T/F Q,137,371,350,271
Redistribution means that certain routes are not advertised in some parts of the network.

|
2
|
10
|
Correct.
|
Incorrect. The statement is false.

@@QUES 030103t XYF Q,0,0,350,350
The  ____________  list specifies the networks from which updates may be received and from which they will be suppressed by the router.

|
Choose an option to fill the blank.
|
%010distribute
%010static
%010access
|
3
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030104t DTF Q,147,391,309,315
To redistribute routing updates you use the  _  command with  ________________ .

|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
Distribute-List
Access Lists
|
1
|
Correct.
|
10
|
Incorrect. It's the other way around.
|
0
|
Incorrect.
|
0
|
Incorrect.
|
0
|
The full statement is now shown.

@@QUES 030105t T/F Q,161,385,311,296
A network can be hidden from routers using interface filtering or redistribution filtering.

|
1
|
10
|
Correct.
|
Incorrect. The statement is true. 

@@QUES 030201t Y/N Q,175,393,273,299
Does Enhanced IGRP have to be manually configured for route summarization?

|
2
|
10
|
Correct.
|
Incorrect. The answer is No.

@@QUES 030202t FIB Q,128,340,372,206
The _______________________ command is used to turn off automatic route summarization.

|
Type the missing command.
|
20
|
%007No Auto-Summary
|
That's right.
|

|
Yes but the word used here "".
|

|

|

|

|
Incorrect.
|
The command used here is "No Auto-Summary".
|
The full statement is now shown.

@@QUES 030203t SXY Q,147,393,329,328
Which command specifies summary routes on a particular interface?

|
Choose an option.
|
IP Summary-Address EIGRP
Auto-Summary
EIGRP Summary-Address
|
1
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 030204t T/F Q,180,395,287,302
Without route summarization each router in a network must retain a route to every subnet in the network.

|
1
|
10
|
Correct.
|
Incorrect. The statement is true.
|
|
|
|
|
|
|
