@@QUES 030101 T/F Q,161,358,268,319
Do you think the following statement is true or false?

All servers and routers keep a complete list of the services available throughout the network.
|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 030102 XYF Q,135,437,336,310
See if you can choose the correct option to fill the blank.

Adding, finding and removing, services on an IPX network is done  _____________ .
|
Choose an option to fill the blank.
|
%010statically
%010dynamically
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030103 MXY Q,90,433,414,347
See if you can identify the correct statement(s)?
|
Choose each appropriate item.
|
A GNS request is a broadcast that is issued by a client using IPX SAP
GNS requests a specific service from a server
The nearest available server offering the required service responds with another SAP
A GNS response allocates a server to the client
|

|
1,2,3,4
|
That's right.
|
Partly right. In fact, all options are correct and are now highlighted.
|
You have not made any correct choices. In fact, all options are correct and are now highlighted.
|
All options are correct and are now highlighted.

@@QUES 030104 XYF Q,8,396,270,353
See if you can choose the correct option to fill the blank.

________  should be the first to respond to GNS requests.
|
Choose an option to fill the blank.
|
Routers
Local NetWare servers
Remote NetWare servers
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030105 Y/N Q,129,330,334,268
Do you think that the allocation of available servers in an IPX network can be implemented using a round-robin strategy?
|
1
|

|
You're right.
|
In fact, you can.
|
The answer is Yes.

@@QUES 030106 XYF Q,301,455,325,353
See if you can choose the correct option to fill the blank.

A Cisco router will advertise the complete SAP table  ____________ .
|
Choose an option to fill the blank.
|
%010at regular intervals
%010at every topology change
%010only on request
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030107 T/F Q,124,370,343,324
Do you think the following statement is true or false?

When selecting a server for a GNS response, no consideration is given to the metrics associated with the route to the server.
|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.

@@QUES 030201 XYF Q,169,380,267,336
See if you can decide which words fill the blank.

This type of flow control is called  __________________ .
|
Choose an option to fill the blank.
|
%010start-to-end flow control
%010end-user flow control
%010end-to-end flow control
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030202 T/F Q,135,359,320,299
Do you think the following statement is true or false?

SPX enhances the IPX protocol by supervising data sent across the network.
|
1
|

|
That's right.
|
In fact, it's true.
|
The statement is true.

@@QUES 030203 T/F Q,341,377,288,323
Do you think the following statement is true or false?

SPX requests verification from the destination that the data transmitted was successfully received.
|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 030204 XYF Q,153,433,286,368
See if you can choose the correct option to fill the blank.

SPX attaches a  ____________  to each segment transmitted as a means of verifying error free transmission.
|
Choose an option to fill the blank.
|
%010flag
%010checksum
%010header
%010trailer
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030205 SXY Q,91,397,409,367
Can you identify what action SPX takes when no replies to acknowledgment requests for such a series of packets are  received within a specified time?
|
Choose an option.
|
SPX only retransmits those packets not acknowledged
SPX retransmits all packets in the series
SPX immediately ends transmission and informs the operator that the connection is down
SPX stops and waits for the destination to request retransmission of the packets unsuccessfully received
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 030206 XYF Q,115,387,367,350
See if you can choose the correct option to fill the blank.

SPX spoofing allows clients and servers to create their own  _______  keepalive packets.
|
Choose an option to fill the blank.
|
%010watchdog
%010update
%010connection
%010virtual
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030207 MXY Q,111,411,365,350
See if you can identify the accurate statement(s) about User Datagram Protocol (UDP).
|
Choose each appropriate item.
|
UDP is connection-oriented
UDP provides transport services
UDP does not acknowledge data receipt
Datagram delivery is accomplished by assigning a port address
|

|
2,3,4
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 030208 XYF Q,159,381,276,314
See if you can decide which words fill the blank.

A port address is a  ______________ .
|
Choose an option to fill the blank.
|
%010virtual circuit connection
%010pointer to a local process
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030301 FIB Q,167,438,268,241
See if you can complete the following statement.

The NetWare shell runs on  _______  or workstations.
|
Type the missing word.
|
Remember NetWare's client/server approach.
|
%007clients
|
That's right.
|

|

|

|

|

|

|
That's not the word required here. Try again.
|
The missing word is "clients".
|
The full statement is now shown.

@@QUES 030302 SXY Q,255,454,367,405
Try to select the action taken by the NetWare shell when it monitors an application I/O request that can only be satisfied by an access to the network.
|
Choose an option.
|
The NetWare shell passes the request to local I/O resources
The NetWare shell immediately packages the request and sends it to lower layer software for processing
The NetWare shell polls the network for an appropriate server before passing the request to lower layer software
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 030303 Y/N Q,140,435,304,276
Do you think client applications are aware of any network access required for completion of an application call?
|
2
|

|
You're right.
|
In fact, they are not.
|
The answer is No.

@@QUES 030304 SXY Q,120,353,350,325
Can you identify which layer of the OSI model describes the functionality of the RPC?
|
Choose an option.
|
%010transport layer
%010application layer
%010presentation layer
%010session layer
%010network layer
|

|
4
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 030305 T/F Q,150,390,297,313
Do you think the following statement is true or false?

RPC does not allow local applications to call functions on other networks.
|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.

@@QUES 030306 MXY Q,126,437,336,335
Identify the true statement(s) about NetWare RPC servers.
|
Choose each appropriate item.
|
RPC servers are usually specialized service providers
RPC servers execute function calls and put the results in reply packets
RPC reply packets are returned to the calling operating system or client
|

|
1,2,3
|
That's right.
|
Partly right. In fact, all options are correct and are now highlighted.
|
You have not made any correct choices. In fact, all options are correct and are now highlighted.
|
All options are correct and are now highlighted.

@@QUES 030307 DTF Q,118,376,371,363
Try to decide which option goes in which blank.

NetWare  __________  software running on a workstation uses NCP function calls to provide transparent file and printer access to the service  __________ .
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
%010server
%010client
|
4
|
That's right.
|
Incorrect.
|
Incorrect.
|
That's not correct.
|
The full statement is now shown.

@@QUES 030308 T/F Q,148,387,306,320
Do you think the following statement is true or false?

NetWare Message Handling Service (MHS) is a message delivery system that provides electronic mail transport.
|
1
|

|
That's right.
|
In fact, it's true.
|
The statement is true.

@@QUES 030309 DTF Q,118,435,359,340
Try to decide which option goes in which blank.

____________  provides message delivery among users on the same file server.

____________  provides network-wide message delivery.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
Global MHS
Basic MHS
|
2
|
That's right.
|
In fact, it's the other way around.
|
Incorrect.
|
Incorrect.
|
The full statements are now shown.

@@QUES 030310 MXY Q,98,433,398,395
Identify the true statement(s) about NetWare MHS.
|
Choose each appropriate item.
|
Basic MHS does not support full-name user addressing
Basic MHS supports third party message applications
Users can be imported from the NetWare bindery on installation
Basic MHS is easily upgraded to Global MHS
NetWare MHS is not suitable for electronic mail applications in environments with limited connectivity requirements
|

|
2,3,4
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 030311 T/F Q,253,358,237,313
Do you think the following statement is true or false?

Btrieve is a key-indexed record management system.
|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 030312 MXY Q,93,424,410,362
Identify the true statement(s) about NetWare Btrieve?
|
Choose each appropriate item.
|
Btrieve is client-based
Btrieve automatically maintains file indexes as records are inserted, updated, and deleted
Btrieve maintains consistent file structues
Btrieve has fixed-size I/O cache buffers
Btrieve allows concurrent access to records in multiprocess environments
|

|
2,3,4,5
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 030313 DTF Q,107,426,382,370
Try to decide which option goes in which blank.

A Btrieve application running on a  ___________  can access data on the local server or on a remote server.

A Btrieve application running on a  ___________  can access local, remote, or local and remote data.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
%010workstation
%010server
|
2
|
That's right.
|
In fact, it's the other way around.
|
Incorrect.
|
Incorrect.
|
The full statements are now shown.

@@QUES 030314 Y/N Q,152,332,298,289
Do you think NLM modules are designed as easily attachable add-ons to the existing NetWare system?
|
1
|

|
You're right.
|
In fact, they are.
|
The answer is Yes.

@@QUES 030315 DTF Q,9,451,263,362
Try to decide which option goes in which blank.

The  __________  packets are encapsulated within  ______packets for transport across the IBM network.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
LU 6.2
NetWare
|
2
|
That's right.
|
In fact, it's the other way around.
|
Incorrect.
|
Incorrect.
|
The full statement is now shown.

@@QUES 030316 XYF Q,303,449,321,395
See if you can choose the correct option to fill in the blank.

NetWare's NetBIOS emulation software allows  ____________  within the NetWare system to run applications that support IBM's NetBIOS calls.
|
Choose an option to fill the blank.
|
%010routers
%010servers
%010workstations
%010the network administrator
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030101t MXY Q,120,442,389,406
Identify the true statement(s) about the operation of the client/server relationship in IPX networks.
|
Choose each appropriate item.
|
All servers can advertise their services using SAP advertisements
All routers and servers keep a complete list of the services available throughout the network
SAP services are identified by name
GNS packets are used to synchronize the list of available servers
A GNS response allocates a server to a client
|
1,2,5
|
35
|
Correct.
|
7
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 030102t SXY Q,133,428,368,365
What action does a client take when it requires a specific service?
|
Choose an option.
|
It sends a unicast packet to a known server
It broadcasts a GNS request
It polls it's nearest router for the address of an available server
It examines SAP updates for servers offering the required service
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 030103t XYF Q,132,427,373,372
By default, a Cisco router operating on an IPX segment responds to a GNS request with  ______________  in the SAP table.
|
Choose an option to fill the blank.
|
%010the most recently known server
%010the next available server
%010a randomly chosen server
%010the longest known server
|
1
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030104t T/F Q,177,386,280,284
Routers give clients the address of the next available server when a round-robin strategy is in operation.
|
1
|
10
|
Correct.
|
Incorrect. The statement is true.

@@QUES 030105t MXY Q,153,414,322,335
Identify the metrics used by a router when choosing a server for a GNS response.
|
Choose each appropriate item.
|
%010cost
%010tick value
%010hop count
%010bandwidth
%010load
|
2,3
|
35
|
Correct.
|
7
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 030201t MXY Q,144,425,345,373
Identify the true statement(s) about NetWare's SPX protocol.
|
Choose each appropriate item.
|
SPX is a sequenced packet protocol
SPX is connection-oriented
SPX supplements the datagram service offered by NetWare's IPX protocol
NetWare's SPX is equivalent to a session layer protocol in the OSI model
|
1,2,3
|
28
|
Correct.
|
7
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 030202t DTF Q,145,414,342,348
_______  verifies and acknowledges successful packet delivery to any network destination.

_______  simply accepts and transports packets across a network without verification of successful receipt.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
UDP
SPX
|
2
|
Correct.
|
10
|
The correct statements are now shown.
|
0
|
Incorrect.
|
0
|
Incorrect.
|
0
|
The full statement is now shown.

@@QUES 030203t T/F Q,168,376,294,275
UDP is a reliable, connection-oriented transport protocol.
|
2
|
10
|
Correct.
|
Incorrect. The statement is false.

@@QUES 030204t FIB Q,166,343,297,208
SPX's verification process involves calculating a  _________  value from the data before transmission.
|
Type the missing word.
|
20
|
%007checksum,check sum,check-sum
|
Correct.
|

|

|

|

|

|

|

|
Incorrect. The missing word is "checksum".
|
The full statement is now shown.

@@QUES 030205t DTF Q,156,389,317,301
_______  datagrams are encapsulated inside  ________  headers for transport across an IP based internetwork.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
IPX/SPX
UDP/IP
|
1
|
Correct.
|
10
|
Incorrect. It's the other way around.
|
0
|
Incorrect.
|
0
|
Incorrect.
|
0
|
The full statement is now shown.

@@QUES 030206t SXY Q,101,435,432,393
What action does SPX take when a number of packet retransmissions fails to return a positive acknowledgment?
|
Choose an option.
|
SPX assumes the connection has failed and warns the operator
SPX continues retransmitting packets until connection failure is confirmed
SPX continues retransmitting until a keepalive timer times out
SPX simply stops retransmitting and takes no further action
|
1
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 030207t DTF Q,0,0,395,299
SPX watchdog spoofing allows a  _________  to act for a  _________  by sending watchdog packets to a NetWare server to keep the session between client and server active.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
NetWare client
%010router
|
2
|
Correct.
|
10
|
Incorrect. It's the other way around.
|
0
|
Incorrect.
|
0
|
Incorrect.
|
0
|
The full statement is now shown.

@@QUES 030301t MXY Q,0,0,442,387
Identify the true statement(s) about the NetWare shell.
|
Choose each appropriate item.
|
The NetWare shell consists of a number of Virtual Loadable Modules (VLMs)
The NetWare shell blocks application I/O calls that require network access
The NetWare shell functions to keep client applications  unaware of any network access required for completion of application calls
Application calls that do not require network access are sent to local resources by the NetWare shell
|
1,3,4
|
28
|
Correct.
|
7
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 030302t MXY Q,0,0,279,324
Select the type(s) of software that handle RPC local function calls.
|
Choose each appropriate item.
|
%010redirector
%010shell
%010virtual file system interface
|
1,2,3
|
21
|
Correct.
|
7
|
Partly right. In fact, all options are correct and are now highlighted.
|
You have not made any correct choices. In fact, all options are correct and are now highlighted.

@@QUES 030303t T/F Q,0,0,299,307
RPC servers are usually specialized service providers that can only handle a single RPC call at any one time.
|
2
|
10
|
Correct.
|
Incorrect. The statement is false.

@@QUES 030304t XYF Q,0,0,350,350
The NetWare Core Protocol (NCP) is a series of  _____________________  designed to satisfy workstation application requests.
|
Choose an option to fill the blank.
|
VLMs
%010server routines
%010interrupt handling routines
%010function calls
%010application monitoring routines
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030305t MXY Q,0,0,274,366
Identify the service(s) provided by NetWare Core Protocols (NCPs).
|
Choose each appropriate item.
|
%010file access
%010printer access
%010name management
%010accounting
%010security
%010file synchronization
|
1,2,3,4,5,6
|
36
|
Correct.
|
6
|
Partly right. In fact, all options are correct and are now highlighted.
|
You have not made any correct choices. In fact, all options are correct and are now highlighted.

@@QUES 030306t FIB Q,133,354,268,247
Which NetWare message delivery protocol would be used to provide electronic mail transport?

_____________
|
Type your answer.
|
20
|
%007MHS,Message Handling Service,Basic MHS,Global MHS
|
Correct.
|

|

|

|

|

|

|

|
Incorrect.
|
The answer is now shown.

@@QUES 030307t T/F Q,0,0,269,285
Basic MHS allows full-name user addressing and supports third party message applications.
|
1
|
10
|
Correct.
|
Incorrect. The statement is true.

@@QUES 030308t FIB Q,0,0,243,212
NetWare Btrieve is Novell's  _________  indexed record management system.
|
Type the missing word.
|
20
|
%007key
|
Correct.
|

|

|

|

|

|

|

|
Incorrect. The missing word is "key".
|
The full statement is now shown.

@@QUES 030309t FIB Q,0,0,255,204
LU 6.2 allows NetWare nodes to exchange information across an  ________  network.
|
Type the missing word.
|
20
|
%007IBM
|
Correct.
|

|

|

|

|

|

|

|
Incorrect. The missing word is "IBM".
|
The full statement is now shown.

@@QUES 030310t T/F Q,0,0,290,294
A NetWare Loadable Module (NLM) is a program that you can load and unload from server memory only when the server is not running.
|
2
|
10
|
Correct.
|
Incorrect. The statement is false.
|
|
|
|
|
|
|
