@@ 1
Ethernet0 is up, line protocol is up
  Hardware is Lance, address is 0000.0c8d.c30d (bia 0000.0c8d.c30d)
  Internet address is 172.16.128.1/24
  MTU 1500 bytes, BW 10000 Kbit, DLY 1000 usec, rely 255/255, load 1/255
  Encapsulation ARPA, loopback not set, keepalive set (10 sec)
  ARP type: ARPA, ARP Timeout 4:00:00
  Last input 0:00:06, output 0:00:02, output hang never
  Last clearing of "show interface" counters never
  Output queue 0/40, 0 drops; input queue 0/75, 0 drops
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
      33104 packets input, 5306937 bytes, 0 no buffer
      Received 33075 broadcasts, 0 runts, 0 giants
      0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
      0 input packets with dribble condition detected
      37109 packets output, 3444689 bytes, 0 underruns
      483 output errors, 416 collisions, 3 interface resets, 0 restarts
      0 output buffer failures, 0 output buffers swapped out
@@

@@ 2
Serial0 is up, line protocol is up
  Hardware is HD64570
  Internet address is 172.16.65.2/24
  MTU 1500 bytes, BW 1544 Kbit, DLY 20000 usec, rely 255/255, load 1/255
  Encapsulation HDLC, loopback not set, keepalive set (10 sec)
  Last input 0:00:00, output 0:00:02, output hang never
  Last clearing "show interface" counters never
  Output queue 0/40, 0 drops; input queue 0/75, 0 drops
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     38666 packets input, 2232727 bytes, 0 no buffer
     Received 37515 broadcasts, 0 runts, 0 giants
     0 input errors, 0CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     38754 packets output, 2279229 bytes, 0 underruns
     0 output errors, 0 collisions, 1 interface resets, 0 restarts
     0 output buffer failures, 0 output buffers swapped out
     4 carrier transitions
     DCD=up DSR=up DTR=up RTS=up CTS=up
@@

@@ 3
  Hardware is HD64570
  Internet address is 172.16.67.2/24
  MTU 1500 bytes, BW 1544 Kbit, DLY 20000 usec, rely 255/255, load 1/255
  Encapsulation HDLC, loopback not set, keepalive set (10 sec)
  Last input 00:00:01, output 00:00:00, output hang never
  Last clearing of "show interface" counters never
  Ouput queue: 0/40, 0 drops; input queue 0/75, 0 drops
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
    46225 packets input, 2723381 bytes, 0 no buffer
    Received 42727 broadcasts, 0 runts, 0 giants
    0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
    40650 packets output, 2437686 bytes, 0 underruns
    0 output errors, 0 collisions, 1 interface resets, 0 restarts
    0 output buffer failures, 0 output buffers swapped out
    34 carrier transitions
    DCD=up DSR=up DTR=up RTS=up CTS=up
@@

@@ 4
Capability Codes: R - Router, T - Trans Bridge, B - Source Route Bridge
                  S - Switch, H - Host, I - IGMP

Device ID       Local Intrfce      Holdtme    Capability  Platform  Port ID
Sydney             Ser 0           125          R         2500      Ser 0
Dublin             Ser 1           175          R         2500      Ser 1
@@

@@ 5
SanFran#dublin
Trying dublin (172.16.67.2)... Open
@@

@@ 6
 

User Access Verification

Password:
@@

@@ 7
Dublin>
@@

@@ 8
BRIO is administratively down, line protocol is down
  Hardware is BRI
  MTU 1500 bytes, BW 64 Kbit, DLY 20000 usec, rely 255/255, load 1/255
  Encapsulation HDLC, loopback not set
  Last input never, output never, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0 (size/max/drops); Total output drops: 0
  Output queue: 0/64/0 (size/max/drops)
     Conversations 0/0 (active/max active)
     Reserved Conversations 0/0 (allocated/max allocated)
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     0 packets input, 0 bytes, 0 no buffer
     Received 0 broadcasts, 0 runts, 0 giants
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 packets output, 0 bytes, 0 underruns
     0 output errors, 0 collisions, 0 interface resets
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
@@

@@ 9
Serial0 is up, line protocol is up
  Hardware is HD64570
  Internet address is 172.16.66.2/24
  MTU 1500 bytes, BW 1544 Kbit, DLY 20000 usec, rely 255/255, load 1/255
  Encapsulation HDLC, loopback not set, keepalive set (10 sec)
  Last input 00:00:05, output 00:00:01, output hang never
  Last clearing of "show interface" counters never
  Output queue 0/40, 0 drops; input queue 0/75, 0 drops
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute ouput rate 0 bits/sec, 0 packets/sec
     10202 packets input, 592685 bytes, 0 no buffer
     Received 8035 broadcasts, 0 runts, 0 giants
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     10209 packets output, 591789 bytes, 0 underruns
     0 output errors, 0 collisions, 2 interface resets
     0 output buffer failures, 0 output buffers swapped out
     0 carrier transitions
     DCD=up DSR=up DTR=up RTS=up CTS=up
@@

@@ 10
Serial1 is up, line protocol is up
  Hardware is HD64570
  Internet address is 172.16.67.2/24
  MTU 1500 bytes, BW 1544 Kbit, DLY 20000 usec, rely 255/255, load 1/255
  Encapsulation HDLC, loopback not set, keepalive set (10 sec)
  Last input 00:00:00, output 00:00:09, output hang never
  Last clearing of "show interface" counters never
  Input queue: 0/75/0 (size/max/drops); Total output drops: 0
  Ouput queue: 0/64/0 (size/threshold/drops)
    Conversations 0/1 (active/max active)
    Reserved Conversations 0/0 (allocated/max allocated)
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
    10925 packets input, 720206 bytes, 0 no buffer
    Received 10517 broadcasts, 0 runts, 0 giants
    0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
    10433 packets output, 651566 bytes, 0 underruns
    0 output errors, 0 collisions, 1 interface resets
    0 output buffer failures, 0 output buffers swapped out
    0 carrier transitions
    DCD=up DSR=up DTR=up RTS=up CTS=up
@@

@@ 11
Serial1 is up, line protocol is up
@@

@@ 12
 
[Connection to 172.16.67.2 closed by foreign host]
SanFran#
@@

@@ 13
Ethernet 0 is up line protocol is down
  Hardware is Lance, address is 0000.0c92.9048 (bia 0000.Oc92.9048)
  Internet address is 131. 108. 192. 1/24
  MTU 1500 bytes, BW 10000 Kbit, DLY 1000 usec. rely 128/255, load 1/255
  Encapsulation ARPA, loopback not set, keepalive set (10 sec)
  ARP type:  ARPA, ARP Timeout 04:00:00
  Last input 01:54:48, output 00:00:05, output hang never
  Last clearing of "show interface" counter never
  Output queue 0/40, 0 drops; input queue 0/75, 0 drops
  5 minute input rate 0 bits/sec, 0 packets/sec
  5 minute output rate 0 bits/sec, 0 packets/sec
     983 packets input, 148372 bytes, 0 no buffer
     Received 983 broadcasts, 0 runts, 0 gaints
     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
     0 input packets with dribble condition detected
     1243 packets output, 93188 bytes, 0 underruns
     695 output errors, 16 collisions, 2 interface resets
     0 babbles, 0 late collision, 13 deferred
     695 lost carrier. 0 no carrier
@@

@@SCRL 040201
 



SanFran>enable
Password
SanFran# ____________________
@@SCRL

@@SCRL 040202
SanFran# ________________________
@@SCRL

@@SCRL 040205
Dublin> ____________________
@@SCRL

@@SCRL 040206
Dublin> __________
@@SCRL
