@@QUES 020101 T/F Q,74,450,240,305
Do you think the following statement is true or false?

The network number identifies a physical network.
|
1
|

|
That's right.
|
In fact, it does.
|
The statement is true.

@@QUES 020102 T/F Q,121,433,346,316
Do you think the following statement is true or false?

A network must have a number that is unique throughout the entire IPX internetwork.
|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 020103 SXY Q,114,298,372,277
What part of the IPX address 4A.0000.0c00.23FE do you think is the node address?
|
Choose an option.
|
4A.0000.0c00.23FE
4A.0000.0C00
0000.0C00.23FE
23FE
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020201 XYF Q,122,380,347,345
See if you can choose the correct option to fill the blank.

A frame is an information unit whose source and destination is a  __________  layer entity.
|
Choose an option to fill the blank.
|
%010transport
%010network
%010physical
%010data link
|

|
4
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020202 T/F Q,128,365,337,314
Do you think the following statement is true or false?

Ethernet version 2 can be used for networks that handle both TCP/IP and IPX traffic.
|
1
|

|
That's right.
|
In fact, it can.
|
The statement is true.

@@QUES 020203 Y/N Q,157,390,270,294
Do you think that Cisco routers can support SAP, SNAP, and LLC frame encapsulation formats?
|
1
|

|
You're right.
|
In fact, they can.
|
The answer is Yes.

@@QUES 020204 Y/N Q,77,449,281,256
Do you think that FDDI has a raw frame format similar to Ethernet's?
|
1
|

|
You're right.
|
In fact, it does.
|
The answer is Yes.

@@QUES 020301 Y/N Q,142,437,309,264
Do you think that packet fragmentation is performed by Novell IPX.
|
2
|

|
You're right.
|
In fact, it isn't.
|
The answer is No.

@@QUES 020302 SXY Q,127,367,334,331
What information do you think is contained in the transport control field?
|
Choose an option.
|
An indication of the number of routers a packet has passed through
An indication of the network layer protocols used
A list of packets received and sent
A time log of transmitted packets
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020303 T/F Q,343,379,280,323
Do you think the following statement is true or false?

When this field is zero, the sending and receiving nodes are assumed to be on the same network segment.
|
1
|

|
That's right.
|
In fact, they are.
|
The statement is true.

@@QUES 020401 T/F Q,397,378,226,317
Do you think the following statement is true or false?

This enables IPX routing on those interfaces.
|
1
|

|
That's right.
|
In fact, it does.
|
The statement is true.

@@QUES 020402 Y/N Q,157,349,280,273
Do you think that a single interface can support multiple networks?
|
1
|

|
You're right.
|
In fact, it can.
|
The answer is Yes.

@@QUES 020403 XYF Q,141,437,318,323
See if you can choose the correct option to fill the blank.

When assigning multiple networks to a single interface, all encapsulation types for the networks should be  _________ .
|
Choose an option to fill the blank.
|
%010identical
%010different
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020404 SXY Q,166,329,263,294
How many IPX networks do you think that the administrator can configure on the Ethernet cable?
|
Choose an option.
|
One
Four
Any amount required
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020405 MXY Q,327,381,302,329
What do you think the number segment of the command may refer to?
|
Choose each appropriate item.
|
%010number of subinterfaces being assigned
%010port card number
%010connector card number
%010interface card number
|

|
2,3,4
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 020406 T/F Q,130,396,322,330
Do you think the following statement is true or false?

Once you have specified the subinterface, the second step is identical to that for enabling IPX on a single network.
|
1
|

|
That's right.
|
In fact, it is.
|
The statement is true.

@@QUES 020407 SXY Q,97,438,397,298
If you specify a configuration parameter such as an update timer on a particular subinterface, to which of the following do you think the parameter will apply?
|
Choose an option.
|
To that subinterface only
To that subinterface and all subsequent subinterfaces on the same main interface
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020101t XYF Q,141,383,353,289
In IPX addressing the  _____  address is normally used to identify a particular interface.
|
Choose an option to fill the blank.
|
%010node
%010network
MAC
|
3
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020102t T/F Q,176,396,285,311
IPX addressing uses the Address Resolution Protocol to map the logical address to the MAC address.
|
2
|
10
|
Correct.
|
Incorrect. The statement is false.

@@QUES 020103t MXY Q,138,402,360,327
Which of the following are valid IPX addresses?
|
Choose each appropriate item.
|
0000.0A01.57AB
0000006C.0000.0F93.AB71
8A.002.0AB.DE9
7B.0001.0G21.BC42
|
2,4
|
28
|
Correct.
|
7
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 020104t SXY Q,179,394,271,307
In IPX addressing, how many bits does the network number contain?
|
Choose an option.
|
80
48
32
8
|
3
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020201t SXY Q,170,414,296,344
Which Novell encapsulation technique now allows encapsulation of IPX in the standard 802.3 frame format?
|
Choose an option.
|
Subnet Access Protocol
Service Access Point
Novell-Ether
Address Resolution Protocol
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020202t XYF Q,172,403,295,328
The Cisco keyword for Ethernet 802.3 is  ___________  .
|
Choose an option to fill the blank.
|
ARPA
Novell-Ether
SAP
SNAP
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020203t SXY Q,133,414,363,350
Which of the following is true about the Ethernet and FDDI raw encapsulation formats?
|
Choose an option.
|
The 802.2 LLC header follows the MAC header
The 802.2 LLC header is not included
The 802.2 LLC header precedes the MAC header
|
2
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020204t XYF Q,191,406,256,328
The  ________________  encapsulation type is used on serial interfaces.
|
Choose an option to fill the blank.
|
ARPA
HDLC
SAP
SNAP
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020205t MXY Q,162,414,302,350
Which Cisco keyword frame encapsulation types do Ethernet, FDDI and Token-Ring have in common?
|
Choose each appropriate item.
|
ARPA
HDLC
SAP
SNAP
|
3,4
|
28
|
Correct.
|
7
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 020301t XYF Q,0,0,288,347
In Novell IPX routing, when the value of the  _______  field reaches 16 the packet is discarded.
|
Choose an option to fill the blank.
|
%010transport control
%010packet type
%010packet length
%010checksum
|
1
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020302t SXY Q,166,420,294,363
In an IPX packet, what information is contained in the packet type field?
|
Choose an option.
|
The encapsulation method used on the packet
The source of the packet
The size of the packet
Which upper layer protocol will receive the packet's information
|
4
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020303t SXY Q,150,414,325,350
What information is contained in the data section of the IPX packet?
|
Choose an option.
|
The services offered or required by the packet
Higher level protocol units
The encapsulation type of the packet
Information about IPX routing paths
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020401t SXY Q,147,404,342,322
When enabling IPX on individual interfaces, the encapsulation type chosen for a network should be the same as which of the following?
|
Choose an option.
|
That used by any other networks on the interface
That used by clients and servers on the network
|
2
|
10
|
Correct.
|
Incorrect. The correct option is now highlighted.


@@QUES 020402t SXY Q,99,443,442,401
The sales, marketing, product development, and finance department networks have been configured as subinterfaces on the company Ethernet line, and you want to lengthen the interval between routing updates across all departments.

Which interfaces should be configured with this information?
|
Choose an option.
|
The Ethernet line only
The first network assigned as a subinterface
Those with the same encapsulation type
All the networks
|
4
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|

|

|

|

