@@QUES 030101 XYF Q,320,375,302,316
See if you can choose the correct option to fill in the blank.

Route summarization  _  the amount of routing protocol traffic.
|
Choose an option to fill the blank.
|
%010increases
%010reduces
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030102 T/F Q,161,397,270,318
Do you think the following statement is true or false?

Route summarization is automatically configured in OSPF.
|
2
|

|
That's right.
|
Actually, it must be manually configured.
|
The statement is false.

@@QUES 030103 T/F Q,134,397,320,328
Do you think the following statement is true or false?

If you develop a large-scale internetwork of privately addressed IP nodes you will have unlimited access to the Internet.
|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.

@@QUES 030104 T/F Q,121,356,337,328
Do you think the following statement is true or false?

If route summarization is being used, routes that change within an area do not need to be changed in the backbone or in other areas.
|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 030105 XYF Q,145,332,293,293
See if you can choose the correct option to fill in the blank.

These are called  _  routes.
|
Choose an option to fill the blank.
|
%010inter area
%010intra-area
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030201 SXY Q,154,403,290,341
What do you think the default value for OSPF metrics is based on?
|
Choose an option.
|
Delay
Bandwidth
Path length
Reliability
Load
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 030202 XYF Q,314,451,306,353
See if you can choose the correct option to fill in the blank.

By default a faster medium will be assigned a metric value  _  the metric value of an FDDI link.
|
Choose an option to fill the blank.
|
%010less than
%010equal to
%010greater than
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030203 Y/N Q,308,447,315,284
Do you think the internal route metric is added to the external route metric when you are using the external type 2 metric?
|
2
|

|
You're right.
|
In fact, the answer is No.
|
The answer is No.

@@QUES 030204 XYF Q,126,401,342,339
See if you can choose the correct option to fill in the blank.

If the ABRs inject only the default route into the area, the traffic goes to the ABR that is closest to the  _  of the traffic.
|
Choose an option to fill the blank.
|
%010source
%010destination
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030205 SXY Q,270,448,357,347
Why do you think you would want the traffic to leave the area as soon as possible?
|
Choose an option.
|
The backbone typically has higher bandwidth lines available
The area cannot handle too much traffic at once
The traffic is not destined for the area so there is no point in keeping it in the area
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 030206 T/F Q,170,390,248,324
Do you think the following statement is true or false?

Internetwork topologies are generally designed so that there are no redundant routes.
|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.



@@QUES 030101t MXY Q,0,0,322,396
Which of the following statements about route summarization is/are true?
|
Choose each appropriate item.
|
Route summarization in an OSPF internetwork occurs between each area and the backbone area
Route summarization is automatically configured in OSPF
Route summarization is disabled by default in OSPF routers
OSPF route summarization occurs in the ABRs
|
1,3,4
|
28
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 030102t SXY Q,0,0,312,340
Which of the following is the more wasteful of address space?
|
Choose an option.
|
Using bit-wise subnetting and variable-length subnetwork masks (VLSMs) in combination
Creating a backbone and multiple areas and assigning a separate network address for each
|
2
|
10
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 030103t MXY Q,0,0,376,369
Which of the following statements is/are true?
|
Choose each appropriate item.
|
If you develop a large-scale internetwork of privately addressed IP nodes you will have limited access to the Internet
All nodes on the network in the DMZ must have public-assigned IP addresses
Using a private addressing scheme affords your internetwork limited flexibility and scalability
|
1,2
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 030104t XYF Q,0,0,321,356
If an explicit route to a given IP network or subnetwork cannot be found, the router will forward the packet to a destination specified by the  _  route.

|
Choose an option to fill the blank.
|
%010external
%010intra-area
%010inter area
%010default
|
4
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030201t Y/N Q,0,0,324,275
Can you configure the area so the traffic leaves it as late as possible if the ABRs inject only default routes into the area?
|
2
|
10
|
Correct.
|
Incorrect. The answer is No.

@@QUES 030202t MXY Q,145,414,356,350
Which of the following statements is/are true?
|
Choose each appropriate item.
|
The default value for OSPF metrics is based on load
The metric for a route is the sum of the metrics for all the links in the route
When route summarization is enabled, OSPF uses the metric of the worst route in the summary
|
2
|
21
|
Correct.
|
7 per correct decision
|
Incorrect. The only correct option is now highlighted.
|
You have not made any correct choices. The correct option is now highlighted.



@@QUES 030203t DTF Q,0,0,347,289
Given an OSPF environment with both FDDI and ATM, you must manually configure link metric values so that the  _  link has a higher value than the  _  link.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
FDDI
ATM
|
1
|
Correct.
|
10
|
Incorrect. It's the other way around.
|
0
|
Incorrect.
|
0
|
Incorrect.
|
0
|
The full statement is now shown.

@@QUES 030204t SXY Q,0,0,337,326
Assume that an OSPF area has two ABRs. You want traffic that is not destined for the area to leave the area as soon as possible.

Which of the following will the ABRs have to inject into the area?
|
Choose an option.
|
Default routes only
Summaries
|
1
|
10
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 030205t MXY Q,0,0,355,364
Which of the following statements is/are true?
|
Choose each appropriate item.
|
Internetwork topologies are generally designed to avoid redundant routes
If equal-cost paths exist between nodes, Cisco routers automatically load balance in an OSPF environment
Cisco routers can use up to four equal-cost paths for a given destination
|
2,3
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
