@@QUES 020101 Y/N Q,143,364,312,241
Would you expect that all hosts on an internetwork require unique addresses?
|
1
|

|
That's right.
|
In fact, the answer is Yes.
|
The answer is Yes.

@@QUES 020102 MXY Q,141,420,326,350
Try to identify the valid IP/address(es).

|
Choose one or more items.
|
132.1324.87.175
132.132.87
132.132.87.175
132.132.87.0
|

|
3,4
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 020103 DTF Q,291,403,314,354
Try to decide which option goes in which blank.

The node address component  _____  between hosts on a given network, but  _____  between hosts on different networks.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
%010must be unique
%010can be the same
|
1
|
That's right.
|
In fact it's the other way around.
|
You've filled the first blank correctly, but not the second.
|
You've filled the second blank correctly, but not the first.
|
The full statement is now shown.

@@QUES 020104 Y/N Q,157,320,294,239
Do you think you can use the address 00000000 on a class A network?
|
2
|

|
You're right.
|
In fact, the answer is No.
|
The answer is No.

@@QUES 020105 SXY Q,165,383,290,286
How many possible class B network addresses do you think there are?

|
Choose an option.
|
127
16,384
64
65,536
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020106 XYF Q,151,321,291,242
The ____ address component of a class C address is the last octet.

|
Choose an option.
|
%010network
%010node
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020107 Y/N Q,162,338,279,236
Do you think interfaces can have more than one IP address?
|
1
|

|
You're right.
|
In fact, they can.
|
The answer is Yes.

@@QUES 020108 Y/N Q,169,407,284,250
Do you think routing tables contain host information?
|
2
|

|
You're right.
|
In fact, they don't.
|
The answer is No.

@@QUES 020201 MXY Q,124,387,350,277
Which of the following forms of addresses are acceptable to IP applications such as Telnet?

|
Choose each appropriate item.
|
Host names
IP addresses
Hardware addresses
|

|
1,2
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 020202 DTF Q,120,458,357,288
Try to decide which option goes in which blank.

When a user specifies a  ______  in a command, it must be translated into the appropriate ______.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
host name
IP address
|
1
|
That's right.
|
In fact, it's the other way around.
|
You've filled the first blank correctly, but not the second.
|
You've filled the second blank correctly, but not the first.
|
The full statement is now shown.

@@QUES 020203 SXY Q,243,309,273,285
What type of network do you think uses host tables?

|
Choose an option.
|
Large networks
Small to medium sized networks
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020204 Y/N Q,208,332,279,254
Do you think it's possible to locate a node address in a network table?
|
2
|

|
You're right.
|
In fact, you can't.
|
The answer is No.

@@QUES 020205 XYF Q,343,433,269,295
See if you can choose the correct option to fill the blank.

DNS divides the Internet into  ___________ .
|
Choose an option to fill the blank.
|
%010domains
%010subnets
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020206 Y/N Q,161,351,290,244
Do you think that there are separate top-level domains for each country?
|
1
|

|
You're right.
|
In fact, the answer is Yes.
|
The answer is Yes.

@@QUES 020207 XYF Q,144,320,283,268
Unlike ____ , NIS does not provide name translation for the entire Internet.
|
Choose an option to fill the blank.
|
DNS
%010host tables
%010network tables
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020208 XYF Q,319,402,310,350
See if you can choose the correct option to fill the blank.

To obtain Internet access, an IP address must be obtained from _ .
|
Choose an option to fill the blank.
|
%010the Internet Society
%010a registration authority
%010a telephone company
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020209 SXY Q,128,412,330,284
How do you think IP addresses and domain names are maintained by an organization after registration?

|
Choose an option.
|
On a DNS server
On a network server
On a disk
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020101t SXY Q,179,383,293,301
To which class of IP address does the address 224.0.0.5 belong?
|
Choose an option from the list.
|
A
B
C
D
E
|
4
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020102t SXY Q,163,381,301,283
How many octets make up the network component of a class B IP address?
|
Choose an option from the list.
|
1
2
3
4
|
2
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020103t SXY Q,161,379,320,302
Identify the class to which the IP address 27.34.200.19 belongs.
|
Choose an option from the list.
|
A
B
C
D
E
|
1
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020104t SXY Q,174,394,289,311
Which class of IP address is used by ICMP router discovery packets?
|
Choose an option from the list.
|
A
B
C
D
E
|
4
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020105t MXY Q,145,414,350,350
Identify the true statement(s).
|
Choose one or more items.
|
Class D IP addresses are used for multicast traffic
Class C IP addresses use two octets to identify a node within a network
The most significant bits in Class B IP addresses are always 10
|
1,3
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 020106t SXY Q,198,392,279,290
Identify which of the following is a network address.
|
Choose an option.
|
130.113.0.0
128.63.2.100
10.2.1.1
|
1
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020201t MXY Q,145,414,350,350
Which of the following commands will open a remote terminal session with a remote host?
|
Choose one or more items.
|
Telnet 132.132.87.175
Telnet 132.132.87.175 ^Bhostname^b
%010^Bhostname^b
Telnet ^Bhostname^b
|
1,3,4
|
28
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 020202t MXY Q,151,396,329,315
You can map names to IP addresses using which of the following?
|
Choose one or more items.
|
Host tables and network tables
DNS
MIL
NIS
|
1,2,4
|
28
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 020203t SXY Q,162,387,309,304
Which name translation scheme is used on the Internet?
|
Choose an option from the list.
|
Host tables
Network tables
DNS
NIS
|
3
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
|
|
|
|
|
|

