@@QUES 040101 Y/N Q,143,391,317,285
Do you think that you need to implement a corporate-wide policy to provide an effective traffic queuing plan?

|
1
|

|
You're right.
|
In fact, the answer is Yes.
|
The answer is Yes.

@@QUES 040102 T/F Q,138,418,316,350
Do you think the following statement is true or false?

You can configure priority, custom, and weighted fair queuing on a Cisco router, and you can assign different queue types to each interface.

|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.

@@QUES 040103 XYF Q,127,417,341,350
See if you can choose the correct option to fill the blank.

When there is a limited amount of bandwidth available, priority queuing consumes  __________________  of the available bandwidth.

|
Choose an option to fill the blank.
|
%010a small part
%010half
%010a large part
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 040104 Y/N Q,139,312,314,266
Do you think you have to first define access lists with weighted fair queuing?

|
2
|

|
You're right.
|
In fact, the answer is No.
|
The answer is No.

@@QUES 040201 T/F Q,14,355,239,311
Do you think the following statement is true or false?

If a priority queue fills up, packets are dropped.

|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 040202 SXY Q,287,420,302,337
Which of the following commands do you think assigns previously unassigned traffic to a queue?

|
Choose an option.
|
Priority-List Interface default
Priority-List Default
Priority-List Queue
Priority-List Queue Default
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040203 XYF Q,291,434,321,372
See if you can choose the correct option to fill the blank.

You use the  _____________________  command to assign a priority list number to an interface.

|
Choose an option to fill the blank.
|
Priority-List Interface
Priority-List
Priority-Queue
Priority-Group
|

|
4
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 040301 Y/N Q,4,278,355,266
Do you think that a protocol can monopolize the entire bandwidth, risking the loss of lower priority packets?

|
2
|

|
You're right.
|
In fact, the answer is No.
|
The answer is No.

@@QUES 040302 SXY Q,145,399,303,321
How do you think the system operates queues 1 to 16?

|
Choose an option.
|
The system promotes packets from queue 16 up to queue 1 where they wait to be serviced
The system services packets by cycling through the queues sequentially
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040303 SXY Q,88,371,291,304
When do you think the system queue is emptied?

|
Choose an option.
|
Before any of the other queues
At regular intervals during the operation of the other queues
After the other queues
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040304 XYF Q,272,436,343,372
See if you can choose the correct option to fill the blank.

You use the  _  command to specify the queue to which previously unassigned traffic will be directed.

|
Choose an option to fill the blank.
|
Queue-List
Queue-List Default
Queue-List Group
Queue-List Queue
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 040305 XYF Q,19,420,313,370
See if you can choose the correct option to fill the blank.

Byte-count-number specifies the  __  number of bytes that the system allows to be delivered from a given queue during a particular cycle.

|
Choose an option to fill the blank.
|
%010maximum
%010minimum
%010default
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 040306 SXY Q,292,407,320,307
Which of the following commands do you think you use to assign a queue list to an interface?

|
Choose an option.
|
Queue-List Interface
Queue-List List
Custom-Queue-List
Queue-List custom
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040401 XYF Q,248,449,266,329
See if you can choose the correct option to fill the blank.

The exact order of the packets is determined by the occurrence of the  _  bit in each packet.

|
Choose an option to fill the blank.
|
%010first
%010last
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 040402 T/F Q,160,425,293,350
Do you think the following statement is true or false?

The packets constituting a given message are placed in a holding queue before transmission.

|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 040403 Y/N Q,148,369,285,245
Do you think that file transfers are demanding on bandwidth resources?

|
1
|

|
You're right.
|
In fact, the answer is Yes.
|
The answer is Yes.

@@QUES 040404 Y/N Q,5,343,271,262
Do you think that control-message conversations continue to enqueue data?
|
1
|

|
You're right.
|
In fact, the answer is Yes.
|
The answer is Yes.

@@QUES 040405 XYF Q,6,431,350,368
See if you can choose the correct option to fill the blank.

You use the  _  command to display detailed queuing information for a given interface.

|
Choose an option to fill the blank.
|
Show Queue
Show Queue Interface
Show Interface
Show Interface Queue
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 040101t MXY Q,0,0,395,351
Identify the true statement(s).

|
Choose each appropriate item.
|
Queuing is useful over congested serial lines
Queuing is fast and efficient since it requires buffering in the router
There are different types of queuing strategies but you can assign only one queue type to a given interface
|
1,3
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 040102t XYF Q,0,0,295,304
Using a  _  queuing strategy ensures that each traffic type gets to use some portion of the link.

|
Choose an option to fill the blank.
|
%010priority
%010custom
|
2
|
10
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 040103t MXY Q,0,0,350,412
Identify the true statement(s) comparing and contrasting priority and custom queuing strategies.

|
Choose each appropriate item.
|
Custom queuing is more powerful than priority queuing when you need to prioritize a mission-critical protocol
Priority queuing guarantees that one type of traffic will get through at the expense of all others
Priority queuing makes maximum use of low-bandwidth links for a few selected protocols.
|
2,3
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 040104t T/F Q,0,0,324,314
When you use the weighted fair queuing strategy the low-bandwidth traffic shares the transmission service proportionally according to assigned weights.

|
2
|
10
|
Correct.
|
Incorrect. The statement is false.

@@QUES 040201t SXY Q,0,0,396,350
When you implement priority routing on a Cisco router, which of the following commands is used to establish queuing priorities based on protocol type?

|
Choose an option.
|
Priority-List
Priority-List Queue
Priority-List Protocol
Priority-Protocol
|
3
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 040202t XYF Q,0,0,376,350
When you implement priority queuing on a Cisco router, you use the  __  command to set the priority of all traffic arriving at a given interface.

|
Choose an option to fill the blank.
|
Priority-List Default
Priority-Group Interface
Priority-List Group
Priority-List Interface
|
4
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.
|
The full statement is now shown.

@@QUES 040203t XYF Q,0,0,421,350
When you implement priority queuing on a Cisco router, you use the  _  command to assign previously unassigned traffic to a queue.

|
Choose an option to fill the blank.
|
Priority-List Interface
Priority-List Default
Priority-Group
Priority-Group Default
|
2
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.
|
The full statement is now shown.

@@QUES 040204t XYF Q,0,0,383,350
When you implement priority queuing on a Cisco router, you use the  _  command to define the maximum number of packets in each priority queue.

|
Choose an option to fill the blank.
|
Priority-List Queue-Limit
Priority-List Queue
Priority-List Queue Default
Priority-Group Limit
|
1
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.
|
The full statement is now shown.

@@QUES 040205t SXY Q,0,0,411,350
When you are implementing priority queuing on a Cisco router, which of the following commands do you use to assign a priority list number to an interface?

|
Choose an option.
|
Priority-List
Priority-List Number
Priority-List Interface
Priority-Group
|
4
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.

@@QUES 040206t T/F Q,0,0,270,287
With priority queuing, the high priority queue is always emptied before the others.

|
1
|
10
|
Correct.
|
Incorrect. The statement is true.

@@QUES 040301t T/F Q,0,0,344,298
Custom queuing assigns different amounts of queue space to each protocol and handles the queues in round-robin fashion.

|
1
|
10
|
Correct.
|
Incorrect. The statement is true.

@@QUES 040302t SXY Q,0,0,352,350
When you implement custom queuing on a Cisco router, which of the following commands do you use to establish the priority of traffic arriving on an interface?

|
Choose an option.
|
Queue-List Protocol
Queue-List Queue
Queue-List Interface
Queue-List Default
|
3
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.

@@QUES 040303t XYF Q,0,0,376,356
When you implement custom queuing on a Cisco router, you use the  _  command to limit the length of a particular queue.

|
Choose an option to fill the blank.
|
Queue-List Default
Queue-List Queue
Custom-Queue-List
Queue-List List
|
2
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.
|
The full statement is now shown.

@@QUES 040304t SXY Q,0,0,376,350
When you implement custom queuing on a Cisco router, which of the following commands do you use to define the minimum byte count transferred from a given queue?

|
Choose an option.
|
Queue-List Byte-Count
Queue-List Count
Custom-Queue Byte-Count
Queue-List Queue Byte-Count
|
4
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.

@@QUES 040305t XYF Q,0,0,379,350
When you implement custom queuing on a Cisco router, you use the  _  command to assign a queue list to an interface.

|
Choose an option to fill the blank.
|
Custom-Queue
Custom-Queue-List
Custom-Queue-Number
Queue-List Custom-Queue
|
2
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.
|
The full statement is now shown.

@@QUES 040401t MXY Q,0,0,436,381
Identify the true statement(s) about weighted fair queuing.

|
Choose each appropriate item.
|
A conversation index is used by the fair queue algorithm to determine whether traffic represents low or high volume conversation
As packets are switched through a router they arrive in a precise order at the outgoing interface as indicated by the last bit in each packet
Cisco's implementation of weighted fair queuing divides traffic into conversations based on packet header addressing
|
1,3
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 040402t XYF Q,0,0,374,332
You use the  _  command to manually enable fair queuing on an interface.

|
Choose an option to fill the blank.
|
Fair-Queue List
Fair-Queue
Fair-Queue Discard
Fair-Queue Interface
|
2
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.
|
The full statement is now shown.

@@QUES 040403t SXY Q,0,0,336,350
Which of the following commands do you use to display detailed queuing information for a given interface?

|
Choose an option.
|
Fair-Queue Interface
Show Interface
Show Queue
Show Queuing Interface
|
3
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.

@@QUES 040404t XYF Q,0,0,336,350
You use the  _  command to display the status of a given interface and whether queuing is enabled.

|
Choose an option to fill the blank.
|
Show Queue
Show Queuing Fair
Show Queuing Interface
Show Interface
|
4
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.
|
The full statement is now shown.


