@@QUES 030101 T/F Q,11,342,322,311
Do you think the following statement is true or false?

You can use AutoInstall to configure the first router on the network independently.

|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.

@@QUES 030102 Y/N Q,144,399,299,302
Do you think that the TFTP server can provide a host name for the address presented by the new router?

|
1
|

|
You're right.
|
In fact, the answer is Yes.
|
The answer is Yes.

@@QUES 030103 XYF Q,97,380,290,350
See if you can choose the correct option to fill in the blank.

First the  _  determines an IP address from an existing preconfigured router.

|
Choose an option to fill the blank.
|
%010new router
TFTP server
%010existing router
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030104 SXY Q,8,343,365,330
What do you think happens if the TFTP server fails to provide the new router with a host name?

|
Choose an option.
|
The AutoInstall process starts over
The new router sends a request for IP address-to-host name resolution to a DNS server
The AutoInstall process provides the new router with a temporary host name
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 030105 XYF Q,274,421,318,366
See if you can choose the correct option to fill in the blank.

The IP helper-address command defines the address of the  __________________________________ .

|
Choose an option to fill the blank.
|
%010existing router's serial port
%010new router's first Ethernet port
TFTP server
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030106 SXY Q,272,407,338,317
What do you think happens if the router finds no configuration file?

|
Choose an option.
|
The IOS generates an error message
The router enters setup mode
The router prompts you to supply the address of a remote system holding a valid configuration file
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 030107 SXY Q,318,441,299,321
Which of the following do you think you are prompted for next?

|
Choose an option.
|
More Global Parameters
Network Interface Parameters
Router Bootup Parameters
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 030108 XYF Q,8,455,314,306
See if you can choose the correct option to fill in the blank.

If you enter Yes the configuration file is executed and saved in  ________ .

|
Choose an option to fill the blank.
|
ROM
Flash memory
NVRAM
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030201 T/F Q,208,439,402,274
Do you think the following statement is true or false?

The startup configuration file is stored in RAM and is accessed when the router is running.

|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.

@@QUES 030202 SXY Q,12,431,314,350
Which of the following do you think is the full command that displays a router's startup configuration?

|
Choose an option.
|
Startup
Show Startup
Show Startup-Config
Startup Config
|

|
3
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The correct command is now highlighted.

@@QUES 030203 XYF Q,298,434,310,330
See if you can choose the correct option to fill in the blank.

A Cisco router's running configuration file is stored in  ______ .

|
Choose an option to fill the blank.
|
RAM
NVRAM
ROM
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030204 Y/N Q,265,438,348,273
When administrators want to make changes and test configuration files, do you think they first change the startup configuration file?

|
2
|

|
You're right.
|
In fact, the answer is No.
|
The answer is No.

@@QUES 030205 XYF Q,37,433,291,383
See if you can choose the correct option to fill in the blank.

You use the Privileged mode  ______________  command to enter Global Configuration mode.

|
Choose an option to fill the blank.
|
Configure
Terminal Configure
Enable Configure
Connect
|

|
1
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The full statement is now shown.

@@QUES 030206 Y/N Q,43,422,272,273
Do you think you can configure a router from a virtual terminal?

|
1
|

|
You're right.
|
In fact, the answer is Yes.
|
The answer is Yes.

@@QUES 030207 MXY Q,24,439,321,321
From which of the following do you think you can load an operating system image?

|
Choose each appropriate item.
|
NVRAM
ROM
Flash memory
A TFTP server
|

|
2,3,4
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 030208 T/F Q,15,433,309,338
Do you think the following statement is true or false?

Flash memory is not vulnerable to network failures that can occur when you load system images from servers.

|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 030209 XYF Q,284,434,323,370
See if you can choose the correct option to fill in the blank.

You can use the  __________________  command to learn the name of the system image file.

|
Choose an option to fill the blank.
|
Show Processes
Show Memory
Show Running-Config
Show Flash
|

|
4
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The full statement is now shown.

@@QUES 030210 SXY Q,312,414,292,331
Which of the following commands do you think you use to copy the system image to a tftp server?

|
Choose an option.
|
Copy Flash TFTP
Copy TFTP Flash
Copy TFTP
|

|
1
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The correct command is now highlighted.

@@QUES 030301 SXY Q,296,431,298,322
Which command do you think you use to examine the results of configuration changes that you make?

|
Choose an option.
|
Show Processes
Show Startup-Config
Show Memory
Show Running-Config
|

|
4
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The correct command is now highlighted.

@@QUES 030302 SXY Q,145,380,320,314
Which of the following commands do you think you use to store the current router configuration on a network tftp server?

|
Choose an option.
|
Copy Startup-Config TFTP
Copy Flash TFTP
Copy Running-Config TFTP
|

|
3
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The correct command is now highlighted.

@@QUES 030303 T/F Q,154,398,304,330
Do you think the following statement is true or false?

You enter the IP address of the router interface to which you are copying the configuration file.

|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.

@@QUES 030304 XYF Q,232,439,368,322
See if you can choose the correct option to fill in the blank.

You can erase the current contents of NVRAM using the  _______________________  command.

|
Choose an option to fill the blank.
|
Erase Startup-Config
Erase Running-Config
|

|
1
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The full statement is now shown.

@@QUES 030305 SXY Q,280,327,298,306
Which of the following commands do you think you use to start the process of setting a terminal password from Global Configuration mode?

|
Choose an option.
|
Terminal
Password
Line
|

|
3
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The correct command is now highlighted.

@@QUES 030306 XYF Q,24,423,320,350
See if you can choose the correct option to fill in the blank.

You can find out more information about using the hostname command by typing ______________ .

|
Choose an option to fill the blank.
|
Hostname Router
Hostname?
Hostname ?
|

|
3
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The full statement is now shown.

@@QUES 030307 SXY Q,32,439,290,338
Say you want to change the router's name to SanJose.

Which of the following commands do you think you use?

|
Choose an option.
|
Hostname SanJose
Hostname ? SanJose
Hostname router SanJose
|

|
1
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The correct command is now highlighted.


@@QUES 030401 SFB Q,383,444,246,197
See if you can enter the command that displays the router's running configuration.

|
Type your answer.
|

|
%007show running-config,sh runn,show run,show running
|
That's right.
|
Yes, but the word used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "show running-config".
|
The answer is now shown.

@@QUES 030402 SFB Q,355,444,274,197
See if you can type the command that displays the router's startup configuration file.

|
Type your answer.
|

|
%007show startup-config,sh start,show startup,show start
|
That's right.
|
Yes, but the word used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "show startup-config".
|
The answer is now shown.

@@QUES 030403 SFB Q,357,444,272,197
See if you can enter the command that allows you to access Global Configuration mode.

|
Type your answer.
|

|
%007configure terminal,config term
|
That's right.
|
Yes, but the command used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "configure terminal".
|
The answer is now shown.

@@QUES 030404 SFB Q,350,444,274,256
In this case you are renaming the router Vienna.

See if you can type the command that changes the router's name from London to Vienna.

|
Type your answer.
|

|
%007hostname Vienna,ho Vienna,host Vienna
|
That's right.
|
Yes, but the word used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "hostname vienna".
|
The answer is now shown.

@@QUES 030405 SXY Q,317,454,309,288
Which of the following key combinations do you use to exit configuration Mode?

|
Choose an option.
|
ŁUCtrl+PŁu
ŁUCtrl+XŁu
ŁUCtrl+EŁu
ŁUCtrl+ZŁu
|

|
4
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 030406 XYF Q,318,456,308,327
See if you can choose the correct option to fill in the blank.

You acknowledge the message and return to the Privileged mode prompt by pressing __________.
|
Choose an option to fill the blank.
|
ŁUEnterŁu
ŁUCtrl+ZŁu
ŁUEsc+XŁu
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030407 SFB Q,353,449,274,197
See if you can enter the command that will display the updated configuration information.

|
Type your answer.
|

|
%007show running-config,sh runn,sho runn,show running
|
That's right.
|
Yes, but the word used here is "".
|
Try again.
|
%007show startup-config
|
You have altered the router's running configuration, not the startup configuration file. Try again.
|

|

|
That's not the command required here. Try again.
|
The answer is "show running-config".
|
The answer is now shown.

@@QUES 030101t MXY Q,0,0,329,393
Which of the following statements about the Cisco AutoInstall feature is true?

|
Choose each appropriate item.
|
A new router must be connected to an existing router on either a WAN or a LAN link
The existing router acts as a SLARP, BOOTP or RARP server
The existing router provides a host name for the IP address presented by the new router
|
1
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The correct option is now highlighted.
|
You have not made any correct choices. The correct option is now highlighted.

@@QUES 030102t T/F Q,0,0,354,288
A new router can AutoInstall from an existing router over a LAN or a WAN interface.

|
1
|
10
|
Correct.
|
Incorrect. The statement is true.

@@QUES 030103t XYF Q,0,0,426,333
If, during initialization, a router does not locate a valid configuration file, it enters  _  mode.

|
Choose an option to fill the blank.
|
%010router configuration
%010setup
ROM monitor
Global Configuration
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 030104t MXY Q,0,0,333,335
Which of the following parameters do you configure in setup mode using the system configuration dialog?

|
Choose each appropriate item.
|
Global parameters
Network interface parameters
Router bootstrap parameters
|
1,2
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 030105t SXY Q,0,0,407,391
During initial router configuration the setup command facility prompts you to accept or reject the configuration command script you have just created.

What happens if you accept the script?

|
Choose an option.
|
The configuration file is executed but the file is not saved
The configuration file is saved but it does not execute immediately
The configuration file is executed and saved in NVRAM
|
3
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 030201t XYF Q,0,0,435,339
To display the router configuration file stored in NVRAM, you use the  _____________________  command.

|
Choose an option to fill the blank.
|
Show Running-Config
Config Term
Show Memory
Show Startup-Config
|
4
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.
|
The full statement is now shown.

@@QUES 030202t T/F Q,0,0,364,318
The default method of providing configuration information for a router is to type in commands from  a terminal console.

|
1
|
10
|
Correct.
|
Incorrect. The statement is true.

@@QUES 030203t MXY Q,0,0,418,406
Which of the following statements about router configuration is true?

|
Choose each appropriate item.
|
You can load an operating system image from NVRAM
In case of both network failure and corrupted flash memory you can specify that a system image is loaded from ROM
You can create a backup of the operating system image by copying it to a network server
You can access Interface Configuration mode from Router Configuration mode
|
2,3
|
28
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 030204t SXY Q,0,0,331,369
Which of the following commands do you use to back up an operating system image file to a tftp server?

|
Choose an option.
|
Copy TFTP Flash
Copy TFTP
Copy Flash TFTP
Copy Flash
|
3
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.

@@QUES 030301t MXY Q,0,0,350,350
From which of the following sources can you load router configuration information?

|
Choose each appropriate item.
|
A TFTP server
RAM
NVRAM
Flash memory
|
1,3
|
28
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 030302t XYF Q,0,0,316,351
You can merge additional router configuration information from a TFTP server using the  _  command.

|
Choose an option to fill the blank.
|
Copy TFTP Flash
Copy Flash TFTP
Copy Running-Config TFTP
Copy TFTP Startup-Config
|
4
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.
|
The full statement is now shown.

@@QUES 030303t SXY Q,0,0,350,350
Which of the following commands do you use to delete a router's startup configuration?

|
Choose an option.
|
Exit Startup
Quit Startup-Config
Erase Startup-Config
Del Startup-Config
|
3
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.

@@QUES 030304t SXY Q,0,0,310,374
Say you are configuring a password for the router's console terminal.

Which of the following commands do you use as the first step?

|
Choose an option.
|
Line
Line Console 0
Line Terminal
Line Terminal 0
|
2
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.

@@QUES 030305t XYF Q,0,0,303,350
You use the  ____________________  command to change a router's name.

|
Choose an option to fill the blank.
|
Config Term
Hostname
Config Router
Rename
|
2
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.
|
The full statement is now shown.
