@@QUES 010101 MXY Q,193,414,237,332
With which of the following internetworking protocols do you think NetWare might share  physical channels?

|
Choose each appropriate item.
|
TCP/IP
DECnet
AppleTalk
|

|
1,2,3
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. All of the options are correct and are now highlighted.
|
The correct options are highlighted.

@@QUES 010102 MXY Q,138,432,313,319
Which services do you think can be provided by the entire NetWare system?

|
Choose each appropriate item.
|
File sharing
Printer sharing
Electronic mail transfer
Database access
|

|
1,2,3,4
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 010103 Y/N Q,151,421,277,305
Do you think that NetWare clients and servers can be represented by all kinds of computer system, from PCs to mainframes?

|
1
|

|
You're right.
|
In fact, they can.
|
The answer is Yes.

@@QUES 010104 Y/N Q,149,406,289,281
Do you think that in the client-server system, remote network access is transparent to the user?

|
1
|

|
You're right.
|
In fact, it is.
|
The answer is Yes.

@@QUES 010105 Y/N Q,34,431,257,280
Do you think that the Novell/IPX protocol stack maps directly onto the OSI model?

|
2
|

|
You're right.
|
In fact, it doesn't.
|
The answer is No.

@@QUES 010106 SXY Q,15,449,305,382
With reference to the graphic shown, which protocol do you think is used by servers and routers for advertising their services and network addresses?

|
Choose an option.
|
NCP
SAP
SPX
IPX
RIP
NLSP
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.



@@QUES 010201 Y/N Q,32,443,250,276
Do you think that Novell IPX requires an acknowledgement of each packet sent?

|
2
|

|
You're right.
|
In fact, it doesn't.
|
The answer is No.

@@QUES 010202 MXY Q,170,447,253,323
What do you think are the IPX RIP metrics used for making decisions on optimal routes?

|
Choose each appropriate item.
|
%010ticks
%010bandwidth
%010delay
%010hop count
|

|
1,4
|
That's right.
|
Partly right. RIP uses both hop count and ticks. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 010203 XYF Q,345,444,277,377
See if you can choose the correct option to fill the blank.

Servers running SAP identify themselves and advertise their services by broadcasting a service identification _________ .

|
Choose an option to fill the blank.
|
%010packet
%010application
%010update table
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 010204 T/F Q,335,447,284,332
Do you think the following statement is true or false?

Under a connection-oriented protocol, a virtual circuit must be established to enable data transfer.

|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 010205 T/F Q,200,352,246,328
Do you think the following statement is true or false?

The NetWare Core Protocol provides client-to-server connections and applications.

|
1
|

|
That's right.
|
In fact, it does.
|
The statement is true.

@@QUES 010301 MXY Q,14,436,259,313
To which of the following layers or sublayers do you think that IEEE 802.3 corresponds?

|
Choose each appropriate item.
|
Physical
Media access control
Logical link control
|

|
1,2
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 010302 Y/N Q,171,429,254,282
Do you think that Token Ring specifies both IEEE sublayers of the OSI data-link layer?

|
2
|

|
You're right.
|
In fact, it doesn't.
|
The answer is No.

@@QUES 010303 SXY Q,66,407,350,350
Which MAC protocol has a four- part standard comprising Physical Media Dependent, Physical, Media Access Control and Station Management sections roughly corresponding to the OSI physical and data-link layers?

|
Choose an option.
|
Ethernet/IEEE 802.3
ARCnet
Token Ring/IEEE 802.5
FDDI
PPP
|

|
4
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010101t XYF Q,0,0,346,315
NetBIOS is usually known as  _________  layer interface specification.

|
Choose an option to fill the blank.
|
%010an application
%010a presentation
%010a session
%010a transport
|
3
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 010102t MXY Q,0,0,263,378
To which of the OSI layers does SAP approximately correspond?

|
Choose each appropriate item.
|
%010application
%010presentation
%010session
%010transport
%010network
%010data-link
%010physical
|
1,2,3
|
35
|
Correct.
|
5 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 010103t XYF Q,0,0,316,265
The NetWare Core Protocol corresponds to the  _______  layers of the OSI model.
|
Choose an option to fill the blank.
|
%010upper
%010lower
|
1
|
10
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 010201t SXY Q,0,0,317,331
Which protocol provides client-to-server connections and applications?

|
Choose an option.
|
Service Advertisement Protocol
Novell Link Services Protocol
Sequenced Packet Exchange
NetWare Core Protocol
|
4
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 010202t DTF Q,156,380,317,278
________  is a connection-oriented protocol and  ________  is a connectionless protocol.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
IPX
SPX
|
2
|
Correct.
|
10
|
Incorrect. It's the other way around.
|
0
|
Incorrect.
|
0
|
Incorrect.
|
0
|
The full statement is now shown.

@@QUES 010203t XYF Q,184,396,263,314
The Sequenced Packet Exchange is a  ________  layer protocol.

|
Choose an option to fill the blank.
|
%010network
%010transport
%010data-link
%010physical
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 010204t XYF Q,172,402,294,326
IPX can use Novell's  ___  to route packets through an internetwork.

|
Choose an option to fill the blank.
|
RIP
NCP
OSPF
IGRP
|
1
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 010301t MXY Q,0,0,303,342
Which media access control protocols do not map onto the logical link control sublayer of the OSI data-link layer?

|
Choose each appropriate item.
|
IEEE 802.3
FDDI
Token Ring
ARCnet
PPP
|
1,2,3
|
25
|
Correct.
|
5 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 010302t MXY Q,176,410,284,337
Apart from Token ring, which media access protocol(s) use(s) a token-passing media access method.

|
Choose each appropriate item.
|
ARCnet
Ethernet
FDDI
PPP
|
1,3
|
28
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 010303t XYF Q,145,414,340,350
The  ________  protocol utilises the High Level Data Link protocol and the Logical Link Control protocol at the data link layer.

|
Choose an option to fill the blank.
|
Ethernet
ARCnet
FDDI
Token Ring
PPP
|
5
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 010304t SXY Q,145,430,348,383
Which MAC protocol has a four-part standard comprising Physical Media Dependent, Physical, Media Access Control, and Station Management sections roughly corresponding to the OSI physical and data-link?

|
Choose an option.
|
Ethernet/IEEE 802.3
ARCnet
Token Ring/IEE 802.5
FDDI
PPP
|
4
|
20
|
That's right.
|
That's not it. The correct option is now highlighted.
|
|
|
|
|
|
|
