Classful networks use routing protocols that can only understand the NIC classification of network addresses, with common standard prefixes /8, /16, /24.

Classless networks use routing protocols that allow the specification of arbitrary network prefixes to determine the network portion of an address.

