@@QUES 020101 SXY Q,340,435,271,320
What do you think you type to enter Privileged mode?

|
Choose an option.
|
Privileged
Enable
Exec
User
|

|
2
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The correct command is now highlighted.

@@QUES 020102 Y/N Q,16,431,306,301
When you use help to check the syntax of a command, do you think you add a space between the command and the question mark?

|
1
|

|
You're right.
|
In fact, you do.
|
The answer is Yes.

@@QUES 020103 Y/N Q,329,322,275,256
Do you think that enhanced editing mode is automatically enabled?

|
1
|

|
You're right.
|
In fact, it is.
|
The answer is Yes.


@@QUES 020104 SXY Q,89,431,256,320
Which of the following do you think you use to recall?

|
Choose an option.
|
ŁUCtrl+AŁu
ŁUCtrl+BŁu
ŁUCtrl+PŁu
ŁUCtrl+EscŁu
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020201 Y/N Q,338,438,276,286
Do you think you can examine the router's configurable components from user EXEC mode?

|
1
|

|
You're right.
|
In fact, you can.
|
The answer is Yes.

@@QUES 020202 SXY Q,18,368,256,343
What do you think Runtime represents?

|
Choose an option.
|
How long the router has been up
The CPU time the process has left to run
The CPU time the process has used
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.


@@QUES 020301 SFB Q,335,429,233,203
See if you can type the command that allows you to access privileged mode.

|
Type your answer.
|
You are effectively 'switching on' privileged mode.
|
%007enable,en,ena,enab,enabl
|
That's right.
|
%007e
|
Yes, you can abbreviate the command, but using a single character is not enough in this case. The shortest acceptable abbreviation of the enable command here is en.
|
Try again.
|

|

|

|
That's not the command required here. Try again.
|
The answer is "enable".
|
The answer is now shown.

@@QUES 020302 SYF Q,374,446,241,272
Which of the following do you think you type to see a list of Privileged mode commands?
|
Choose an option.
|
?
??
%010priv?
|

|
1
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The correct command is now shown.

@@QUES 020303 SFB Q,358,440,267,193
See if you can type the command to exit back to User mode.

|
Type your answer.
|
Having enabled privileged mode you now want to leave it.
|
%007disable,disab,disabl,disa
|
That's right.
|
%007d,di,dis
|
Yes, you can abbreviate the command, but using less than four characters is not enough in this case. The shortest acceptable abbreviation of the disable command here is disa.
|
Try again.
|

|

|

|
That's not the command required here. Try again.
|
The answer is "disable".
|
The answer is now shown.

@@QUES 020304 SFB Q,365,451,264,197
See if you can type the command that logs you out of the router.

|
Type your answer.
|
There are a couple of options.
|
%007logout,logo
|
That's right.
|
Yes, but the command used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "logout".
|
The answer is now shown.



@@QUES 020401 SFB Q,357,435,266,187
See if you can type the command that displays the version of the Cisco IOS.
|
Type your answer.
|

|
%007show version,sh ver,show ver,show vers,show versi,show versio,sh vers,sh versi,sh versio,sh version,sho ver,sho vers,sho versi,sho versio,sho version
|
That's right.
|
Yes, but the command used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "show version".
|
The answer is now shown.

@@QUES 020402 SXY Q,320,439,309,361
What do you think this configuration register setting means?
|
Choose an option.
|
The router should attempt to load a Cisco IOS from a tftp server
The router should attempt to load a Cisco IOS from a network management station
The router should attempt to load a Cisco IOS from flash memory
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 020403 SFB Q,367,437,261,198
See if you can type the command that shows the processes that are running on the router.

|
Type your answer.
|
You want to show router processes.
|
%007show processes,sh proc,sh proce,sh proces,sh process,sh processe,sh processes,sho proc,sho proce,sho proces,sho process,sho processe,sho processes,show proc,show proce,show proces,show process,show processe
|
That's right.
|
%007sh p,sh pr,sh pro
|
Yes, you can abbreviate the command, but using only these characters are not enough in this case. The shortest acceptable abbreviation of the show processes command is s proc.
|
Try again.
|

|

|

|
That's not the command required here. Try again.
|
The answer is "show processes".
|
The answer is now shown.

@@QUES 020404 XYF Q,39,440,313,350
See if you can choose the correct option to fill in the blank.

You press __________ to recall the most recent command.
|
Choose an option to fill the blank.
|
ŁUCtrl+AŁu
ŁUEsc+BŁu
ŁUCtrl+PŁu
ŁUCtrl+BŁu
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020405 SFB Q,353,435,266,193
See if you can type the command that shows statistics about memory.

|
Type your answer.
|
You want to examine the memory management system.
|
%007show memory,sh me,show mem,sho me,sho mem,sh mem
|
That's right.
|
Yes, but the command used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "show memory".
|
The answer is now shown.

@@QUES 020406 SXY Q,50,433,295,312
Which of the following commands do you think you type to get back to the router prompt?
|
Choose an option.
|
%010logout
%010q
%010exit
%010show prompt
|

|
2
|
That's right.
|
That's not it. The correct command is now highlighted.
|
The correct command is now highlighted.

@@QUES 020407 SFB Q,352,436,267,197
See if you can type the command that shows information about the router's hardware interfaces.

|
Type your answer.
|

|
%007show interfaces,sh in,show in,show int,sho int,sho in
|
That's right.
|
Yes, but the word used here is "".
|
Try again.
|

|

|

|

|
That's not the command required here. Try again.
|
The answer is "show interfaces".
|
The answer is now shown.

@@QUES 020408 SFB Q,337,438,281,195
See if you can supply the command that shows what protocols are running on the router.

|
Type your answer.
|
You want to show the router's protocols.
|
%007show protocols,sh prot,sho prot,show prot
|
That's right.
|
%007sh pr,sh pro
|
Yes, you can abbreviate the command, but these characters is not enough in this case. The shortest acceptable abbreviation of the show protocols command is sh prot.
|
Try again.
|

|

|

|
That's not the command required here. Try again.
|
The answer is "show protocols".
|
The answer is now shown.



@@QUES 020101t XYF Q,0,0,410,350
When you are navigating a command line that extends beyond a single line on the screen, you can press  _________  to return directly to the start of the line.

|
Choose an option to fill the blank.
|
ŁUCtrl+PŁu
ŁUCtrl+BŁu
ŁUCtrl+AŁu
ŁUEsc+BŁu
|
3
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 020102t T/F Q,0,0,373,338
When you are working with the Cisco IOS context-sensitive help, you use command syntax help to discover which keywords and arguments are required to complete a command.

|
1
|
10
|
Correct.
|
Incorrect. The statement is true.

@@QUES 020103t SXY Q,0,0,324,350
Which of the following key combinations do you type to recall the previous Cisco IOS command line entry?

|
Choose an option.
|
ŁUCtrl+PŁu
ŁUCtrl+BŁu
ŁUCtrl+FŁu
ŁUCtrl+AŁu
|
1
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 020104t MXY Q,0,0,304,350
Which of the following commands can you type to exit the user interface and log out of the router?

|
Choose each appropriate item.
|
Bye
Logout
Quit
End
|
2,3
|
28
|
Correct.
|
7 per correct decision
|
Partly right. The correct commands are now highlighted.
|
You have not made any correct choices. The correct commands are now highlighted.

@@QUES 020201t MXY Q,0,0,350,350
Which of the following Cisco IOS commands displays the operating system version?

|
Choose each appropriate item.
|
Show Version
Show Memory
Show Flash
Show Processes
|
1
|
28
|
Correct.
|
7
|
Partly right. The correct command is now highlighted.
|
Incorrect. The correct command is now highlighted.

@@QUES 020202t SXY Q,0,0,318,350
Which Cisco IOS command displays the value of the configuration register?

|
Choose an option.
|
Show Running-Config
Show Version
Show Buffers
Show Interfaces
|
2
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.

@@QUES 020203t T/F Q,0,0,350,292
The show interfaces command displays the burnt in address (BIA) of a router's Ethernet interface.

|
1
|
10
|
Correct.
|
Incorrect. The statement is true.

@@QUES 020204t XYF Q,0,0,403,340
The routing table being used by IP on a router can be examined using the  _  command.

|
Choose an option to fill the blank.
|
Show IP Protocol
Show IP Route
Show Interfaces
Show IP Interface
|
2
|
20
|
Correct.
|
Incorrect. The correct command is now highlighted.
|
The full statement is now shown.



@@QUES 020205t DTF Q,0,0,374,358
The  _  command shows how much memory is available to specific programs.

The  _  command is used to show how the management system allocates memory for different purposes within the router.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
Show Memory
Show Buffers
|
3
|
Correct.
|
10
|
Incorrect.
|
0
|
Incorrect.
|
0
|
Incorrect.
|
0
|
The correct statements are now shown.
