@@QUES 040101 SXY Q,265,451,237,316
Which protocol do you think is used to locate an unused IP address on the network?
|
Choose an option.
|
ARP
RARP
ICMP
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040102 XYF Q,179,413,270,326
See if you can choose the correct option to fill in the blank.

An interface can have  _  IP address(es).
|
Choose an option to fill the blank.
|
%010multiple
%010only one
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 040103 SXY Q,161,401,277,309
Which of the following commands do you think is used to copy the running configuration to NVRAM?
|
Choose an option.
|
Copy Running-Config
Copy Config
Copy Running-Config Startup-Config
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040104 Y/N Q,129,390,336,297
Do you think you can use hostnames to connect to another router using the configuration entered in the system dialog?
|
2
|

|
You're right.
|
In fact, you can't.
|
The answer is No.

@@QUES 040105 Y/N Q,236,454,291,290
Do you think it's possible to reach an address outside your router subnet using Telnet with an IP address?
|
2
|

|
You're right.
|
In fact, you can't.
|
The answer is No.

@@QUES 040106 SXY Q,142,311,310,296
What protocol do you think Ping uses to determine if packets are being routed?
|
Choose an option.
|
ARP
ICMP
IP
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040107 T/F Q,287,422,291,331
Do you think the following statement is true or false?

The Trace command uses error messages generated by routers to establish the path taken by a packet.
|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 040108 Y/N Q,193,372,256,268
Do you think Cisco IOS uses ARP and RARP to resolve network addresses?
|
1
|

|
You're right.
|
In fact, it does.
|
The answer is Yes.

@@QUES 040109 SXY Q,283,428,263,298
What do you think a static ARP cache contains?
|
Choose an option.
|
An IP address only
A hostname
An IP address associated with a hardware address
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040110 T/F Q,163,403,271,308
Do you think the following statement is true or false?

The HP Probe protocol is used to resolve serial data-link addresses.
|
2
|

|
That's right.
|
Actually, it doesn't.
|
The statement is false.

@@QUES 040111 SXY Q,301,427,310,303
If an IP address does not have a domain name, which of the following domains will it be allocated?
|
Choose an option.
|
The default domain
Any domain in the list of domains
It will not be allocated any domain
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 040201 SYF Q,361,458,260,313
See if you can select the correct command to display the local router's interfaces.
|
Choose an option.
|
%010show ip route
%010show config
%010show interface
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 040202 SFB Q,355,357,270,209
See if you can type the command used to display information about other routers on the network.

|
Type your answer.
|

|
%008show cdp neighbors,sh cd nei,sho cdp nei,sho cdp neigh
|
That's right.
|

|
Yes, but the command used here is "show cdp neighbors".
|

|
Try again.
|

|

|
That's not the word required here. Try again.
|
The answer is "show cdp neighbors".
|
The answer is now shown.

@@QUES 040203 MXY Q,61,444,303,291
See if you can identify the interface(s) directly connected to the SanFran router.
|
Choose each appropriate item.
|
Ethernet0 Dublin
Serial0 Sydney
Serial1 Dublin
Serial1 Sydney
|

|
2,3
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 040204 MXY Q,52,434,289,308
See if you can identify the different commands you can use to log in to the Dublin router.
|
Choose each appropriate item.
|
%010telnet dublin
172.16.67.2
%010telnet 172.16.67.2
%010dublin
|

|
1,3,4
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 040205 SFB Q,349,342,268,195
See if you can enter the command to view the interfaces on the Dublin router.

|
Type your answer.
|

|
%008show interface,%008sh int,%008sho inter,%008sho int
|
That's right.
|

|
Yes, but the command used here is "".
|

|
Try again.
|

|

|
That's not the command required here. Try again.
|
The answer is "show interface", "sh int", "sho inter", "sho int".
|
The answer is now shown.

@@QUES 040206 SFB Q,352,368,264,175
See if you can type the command to log out of the Dublin router.

|
Type your answer.
|

|
%007exit
|
That's right.
|

|
Yes, but the command used here is "exit".
|

|
Try again.
|

|

|
That's not the word required here. Try again.
|
The answer is "exit".
|
The answer is now shown.

@@QUES 040101t MXY Q,0,0,361,350
How can a new router find an initial IP address or a valid configuration file when it first boots?
|
Choose each appropriate item.
|
From a BOOTP server if one exists on the network
If you select the System Configuration Dialog
From a DNS server if one exists on the network
|
1,3
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 040102t MXY Q,173,388,316,307
To configure the router manually, which of the following methods can you use?
|
Choose each appropriate item.
|
Autoinstall
Configuration mode
The Configuration System Dialog
|
2,3
|
21
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 040103t MXY Q,150,403,342,341
Which of the following does the System Configuration Dialog allow you to configure?
|
Choose each appropriate item.
|
Router interfaces
Routing protocols
Routing tables
Host names
Passwords
|
1,2,4,5
|
25
|
Correct.
|
5 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 040104t SXY Q,180,403,262,323
Which of the following describes a running configuration?
|
Choose an option.
|
A configuration file stored in NVRAM
A configuration file stored in Flash memory
A configuration file stored in RAM
|
3
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 040105t DTF Q,145,385,350,294
Complete the Copy command to save a running configuration to NVRAM.

copy  _ -config _ -config
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
%010startup
%010running
|
2
|
Correct.
|
10
|
Incorrect. It's the other way around.
|
0
|
Incorrect.
|
0
|
Incorrect.
|
0
|
The full statement is now shown.

@@QUES 040106t T/F Q,148,379,343,295
Is the following statement true or false?

You need to specify ARP cache entries when dynamic address resolution is available.
|
2
|
10
|
Correct.
|
Incorrect. The statement is false.

@@QUES 040107t SXY Q,151,377,323,285
The command Clear ARP-Cache removes which type of entry from the ARP cache?
|
Choose an option.
|
Static entries
Non-static entries
|
2
|
10
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 040108t SXY Q,167,390,306,303
What is the maximum number of hosts you can have acting as name servers?
|
Choose an option.
|
2
3
4
6
|
4
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 040109t FIB Q,154,343,306,229
Enter the command to test connectivity to the London router using the IP address 172.16.66.1.

________________
|
Type your answer.
|
15
|
%008ping 172.16.66.1
|
Correct.
|

|

|

|

|

|

|
That's not the command used here.
|
The command used here is "ping 172.16.66.1".
|
The answer is now shown.

@@QUES 040110t FIB Q,148,356,343,249
Enter the command to find the route an IP packet takes from SanFran to Dublin using either the hostname Dublin, or the IP address 172.16.67.2.

________________
|
Type your answer.
|
15
|
%008trace Dublin,%008trace dublin,%008trace DUBLIN,%008trace 172.16.67.2
|
That's right.
|

|

|

|

|

|

|
Incorrect.
|
The command used here is "trace dublin" or "trace 172.16.67.2".
|
The answer is now shown.
|
|
|
|
|
|
|

