@@QUES 010101 MXY Q,101,426,393,343
See if you can identify why RIP only maintains a single table entry for any specific destination.
|
Choose each appropriate item.
|
Because it uses hop count as its sole metric
Because it only records the route advertised by its nearest neighbor
For any specific destination it maintains information on the optimal route only
|

|
1,3
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are highlighted.

@@QUES 010102 SXY Q,359,448,268,370
What do you think the RIP routing update timer is used for?
|
Choose an option.
|
It is used to set the interval between periodic update messages
It is used to set the time to live of routed packets
It is used to record the number of messages a particular router receives in a specific timespan
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010103 SXY Q,132,355,334,286
What do you think happens to an invalid route when the route flush timer expires?
|
Choose an option.
|
The route is removed from the routing table
The route is marked as valid again
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010104 XYF Q,173,398,256,331
See if you can choose the correct option to fill the blank.

The value for the route invalid timer must be  _  than that for the route flush timer.
|
Choose an option to fill the blank.
|
%010less
%010greater
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 010105 XYF Q,303,453,324,317
See if you can choose the correct option to fill the blank.

Regular routing update messages contain  _  of the sender's routing table.
|
Choose an option to fill the blank.
|
%010all
%010part
|

|
1
|
That's right.
|
That's not it.  Regular routing updates actually contain all of the sender's routing table.
|
The full statement is now shown.

@@QUES 010106 SXY Q,150,453,299,353
What information do you think the version number field specifies?
|
Choose an option.
|
The serial number of the router
The version of the packet to be sent
The version of the packet format being used
The RIP version being implemented
|

|
4
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010107 SXY Q,347,450,279,316
What address family do you think is usually found when routing with RIP through the Internet?
|
Choose an option.
|
IP
X.25
IPX
DECnet
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010108 SXY Q,268,453,243,316
Which metric do you think is specified in the metric field?
|
Choose an option.
|
Hop count
Delay
Reliability
Bandwidth
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010109 SXY Q,126,361,337,328
What do you think Router 1's next step is?
|
Choose an option.
|
When it identifies the contradiction between its routing information and Router 2's it stops routing
It advertises and uses a two-hop path to Network A through Router 2
It ignores all further updates regarding Network A
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010110 T/F Q,140,392,314,320
Do you think the following statement is true or false?

When the hop count for a route exceeds 15, the route is marked unreachable.
|
1
|

|
That's right.
|
In fact, it is.
|
The statement is true.

@@QUES 010111 SXY Q,123,322,350,287
Which timer determines how long it is before the route is removed from the routing table?
|
Choose an option.
|
Route invalid timer
Route flush timer
Routing update timer
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010112 Y/N Q,115,322,356,270
Do you think that Router A will accept an update message regarding Network 1 from Router E while the hold-down timer is in place?
|
1
|

|
You're right.
|
In fact, it will.
|
The answer is Yes.

@@QUES 010113 T/F Q,148,417,291,320
Do you think the following statement is true or false?

Split horizons are useful for coping with large internetwork routing loops.
|
2
|

|
That's right.
|
Actually, they are useful for smaller two-node loops.
|
The statement is false.

@@QUES 010114 SXY Q,123,313,350,292
With RIP routing and its use of the hop count metric, what is the infinite cost likely to be?
|
Choose an option.
|
Any distance above the number of routers or hops in the internetwork
Any distance equaling 15 hops
Any distance above 15 hops
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010201 XYF Q,137,368,336,338
See if you can choose the correct option to fill the blank.

You type  _  at the User Exec mode prompt to put the router in Privileged mode.
|
Choose an option to fill the blank.
|
%010begin
%010start
%010privilege
%010enable
|

|
4
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 010202 Y/N Q,300,435,308,276
Do you think there is a command for checking which IP protocol are running?
|
1
|

|
You're right.
|
In fact, there is.
|
The answer is Yes.

@@QUES 010203 SXY Q,49,352,370,310
What do you think is the command to check which networks are available to the local router?
|
Choose an option.
|
%010show ip route
%010show ip table
%010show routes
%010show networks
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010204 T/F Q,348,389,264,297
Do you think the following statement is true or false?

To set up RIP you have to put the router in Configuration mode.
|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 010205 SXY Q,59,440,287,261
What do you think is the next step?
|
Choose an option.
|
Log onto other routers
Enable other networks
Turn on RIP on SanFran
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010206 DTF Q,5,437,337,319
Try to decide which option goes in which blank.

To turn on RIP routing you type  _  _  in Configuration mode.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
%010rip
%010router
|
2
|
That's right.
|
In fact, it's the other way around.
|
Incorrect.
|
Incorrect.
|
The full statement is now shown.

@@QUES 010207 SXY Q,25,438,273,321
What do you think is the correct command to enable this network?
|
Choose an option.
|
%010enable net 172.16.0.0
%010network 172.16.0.0
172.16.0.0 network
172.16.0.0
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
3
|
In fact you enter the IP address after the network command. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010208 XYF Q,9,435,315,350
See if you can choose the correct option to fill the blank.

To exit config mode you press  _ at the SanFran(config-router)# prompt.
|
Choose an option to fill the blank.
|
ŁUCtrl+EŁu
ŁUCtrl+XŁu
ŁUCtrl+ZŁu
ŁUEscŁu
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 010209 XYF Q,146,347,249,316
See if you can choose the correct option to fill the blank.

Now you need to get into  _  mode.
|
Choose an option to fill the blank.
|
Configuration
Privileged
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 010210 T/F Q,323,376,290,302
Do you think the following statement is true or false?

Next you need to enable the specific network that RIP will work on.
|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 010211 XYF Q,338,432,272,365
See if you can choose the correct option to fill the blank.

The command to turn off RIP debugging is  _  IP RIP.
|
Choose an option to fill the blank.
|
Undebug
Offdebug
Enddebug
Stpdebug
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 010212 MXY Q,13,355,295,306
What commands do you think can be used to test network connectivity?
|
Choose an option.
|
Ping
Trace
Show Run Config
Show IP Route
|

|
1,2
|
That's right.
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.
|
The correct options are now highlighted.

@@QUES 010301 SYF Q,336,329,285,262
Which of the following do you type to put the router in privileged mode?
|
Choose an option.
|
%010privilege
%010config
%010enable
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct command is now shown.

@@QUES 010302 Y/N Q,392,376,203,251
Can you enable RIP from Privileged mode?
|
2
|

|
You're right.
|
In fact, you must be in Configuration mode.
|
The answer is No.

@@QUES 010303 SYF Q,353,360,259,294
What do you enter to put the router into Configuration mode?
|
Choose an option.
|
%010start
%010enable
%010config
%010startconfig
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct command is now shown.

@@QUES 010304 SDF Q,354,452,269,302
Try to decide which command part goes in which blank to form the complete command to enable RIP on the Sydney router.

|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
%010router
%010rip
|
1
|
That's right.
|
In fact, it's the other way around.
|
Incorrect.
|
Incorrect.
|
The full statement is now shown.

@@QUES 010305 SFB Q,360,401,251,202
See if you can type the command to enable the associated network 172.16.0.0.
|
Type your answer.
|

|
%007network 172.16.0.0
|
That's right.
|

|
Yes, but the command used here is "network 172.16.0.0".
|

|
Try again.
|

|

|
That's not the answer required here. Try again.
|
The answer is "network 172.16.0.0".
|
The answer is now shown.

@@QUES 010306 SXY Q,302,405,317,301
Which of the following is the correct key combination to exit Configuration mode?
|
Choose an option.
|
ŁUCtrl+CŁu
ŁUCtrl+EŁu
ŁUCtrl+XŁu
ŁUCtrl+ZŁu
|

|
4
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 010307 SYF Q,345,398,281,311
Which command do you use to save the new configuration to NVRAM?
|
Choose an option.
|
%010start copy runn
%010runn copy start
%010copy runn start
%010copy run start
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct command is now shown.

@@QUES 010308 T/F Q,364,408,248,320
Do you think the following statement is true or false?

To return to your local router, all you have to do is type ŁRexitŁr.
|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 010309 SYF Q,320,456,310,386
You want to telnet to 172.16.68.2 in London from Sydney.

Remember that this destination doesn't have a host name entry on Sydney.

What do you type at the local router's Privileged mode prompt?
|
Choose an option.
|
%010telnet London
%010telnet 172.16.68.2
%010telnet Sydney
%010telnet 172.16.0.0
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct command is now shown.

@@QUES 010310 T/F Q,379,410,232,320
Do you think the following statement is true or false?

You have to change to Configuration mode first.
|
1
|

|
That's right.
|
In fact, the statement is true.
|
The statement is true.

@@QUES 010311 SFB Q,330,431,256,184
Try typing the command to set up RIP on the London router.
|
Type your answer.
|

|
%007router rip
|
That's right.
|

|
Yes, but the command used here is "router rip".
|

|
Try again.
|

|

|
That's not the command required here. Try again.
|
The answer is "router rip".
|
The answer is now shown.

@@QUES 010312 SFB Q,346,258,266,194
See if you can type the command to save the new configuration to NVRAM on London.
|
Type your answer.
|

|
%007copy runn start,%007copy ru st
|
That's right.
|

|
Yes, but the command used here is "copy runn start".
|
copy run start
|
Try again.
|

|

|
That's not the command required here. Try again.
|
The answer is "Copy Runn Start".
|
The answer is now shown.

@@QUES 010313 SFB Q,381,386,230,264
You have finished enabling RIP on the London router.

See if you can type the command that returns you to the SanFran router.
|
Type your answer.
|

|
%007exit,%007ex
|
That's right.
|

|
Yes, but the command used here is "exit".
|

|
Try again.
|

|

|
That's not the command required here. Try again.
|
The answer is "exit".
|
The answer is now shown.

@@QUES 010314 SYF Q,280,394,270,284
Which of the following commands is used to examine RIP updates?
|
Choose an option.
|
%010show ip route
%010debug ip rip
%010show ip protocol
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct command is now shown.

@@QUES 010315 SYF Q,370,385,252,262
Which of the following do you use to turn off RIP debugging?
|
Choose an option.
|
%010offdebug ip rip
%010undebug ip rip
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct command is now shown.

@@QUES 010316 SYF Q,323,420,292,333
To verify which routing protocol is enabled on the router, which of the following commands must you enter at the local router privileged prompt?
|
Choose an option.
|
%010show ip protocol
%010show protocol
%010show table
%010show ip route
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct command is now shown.

@@QUES 010317 SFB Q,338,435,268,213
See if you can type the command to test network connectivity and show the route taken by packets to a destination.
|
Type your answer.
|

|
%007trace,%007Trace,%007ping,%007Ping
|
That's right.
|

|
Yes, but the command used here is "Trace".
|

|
Try again.
|

|

|
That's not the command required here. Try again.
|
The answer is "Trace".
|
The answer is now shown.

@@QUES 010318 SYF Q,347,416,269,322
Which of the following is the correct format of the Ping command to test connectivity for the London Ethernet 172.16.1.1.
|
Choose an option.
|
%010ping London
%010ping 172.16.1.1
%010ping 172.16.1.0
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct command is now shown.

@@QUES 010101t SXY Q,0,0,337,318
Under the Routing Information Protocol, neighbors must be notified of an invalid route before which of the following expires?
|
Choose an option.
|
Routing update timer
Route invalid timer
Route flush timer
|
3
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.


@@QUES 010102t SXY Q,0,0,329,350
What is the maximum number of address family, address, and metric fields that can be contained in a single IP RIP packet?
|
Choose an option.
|
1
3
16
25
255
|
4
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.


@@QUES 010103t SXY Q,0,0,302,323
What is the typical initial value assigned to RIP's route invalid timer?
|
Choose an option.
|
30 seconds
90 seconds
170 seconds
270 seconds
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.


@@QUES 010104t DTF Q,0,0,386,324
In solving the count to infinity problem with RIP, the  _  method is useful for dealing with routing loops between adjacent routers, and the  _  method is useful for loops in large internetworks.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
%010poison reverse
%010split horizon
|
2
|
Correct.
|
10
|
Incorrect. It's the other way around.
|
0
|
Incorrect.
|
0
|
Incorrect.
|
0
|
The full statement is now shown.

@@QUES 010105t SXY Q,0,0,321,329
Which metric does RIP use to determine the optimal route to a destination?
|
Choose an option.
|
Delay
Hop count
Bandwidth
Reliability
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.


@@QUES 010201t SXY Q,0,0,298,311
Which command is used to save the new router configuration in NVRAM?
|
Choose an option.
|
Start Copy Runn
Copy Runn Start
Runn Copy Start
Copy Run Start
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 010202t SXY Q,0,0,322,326
If you want to monitor RIP routing tables, which of the following do you enter?
|
Choose an option.
|
%010debug ip rip
%010ping
%010trace
%010show ip route
|
4
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 010203t T/F Q,0,0,337,260
To exit configuration mode you must enter ŁUCtrl+XŁu at the configuration mode prompt.
|
2
|
10
|
Correct.
|
Incorrect. The statement is false.

@@QUES 010204t XYF Q,0,0,298,332
When configuring RIP, once RIP is turned on, you next  _  networks associated with the router.
|
Choose an option to fill the blank.
|
%010configure
%010enable
%010telnet to
%010exit
|
2
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.
