| Lab 5.3.7 Cable Tester - Length Estimated time: 45 min. Objectives: Demonstrate skill with a cable tester more advanced than a simple continuity/pin-out tester Use the Length features of the tester to check for opens and shorts with coax and UTP cable Background: In this lab, you will learn the Cable Length feature of the Fluke 620 LAN CableMeter (or its equivalent). Cable length tests can be very helpful in troubleshooting cabling problems with UTP and coaxial cable. You will learn how to use a cable tester to check the length of Ethernet cabling to verify that it is within the standards specified and that the wires inside are the same length (for UTP). You will test different cables including UTP and Coax to determine their length. The Cabling infrastructure (or cable plant) in a building is expected to last at least 10 years. Cabling related problems are one of the most common causes of network failure. The quality of cabling components used, the routing and installation of the cable and quality of the connector terminations will be the main factors in determining how trouble-free the cabling will be. Tools / Preparation: Prior to starting the lab, the teacher or lab assistant should have several correctly wired CAT 5 cables (both straight thru and crossover) and several Coaxial (thinnet) cables to test. Cables should be numbered to simplify the testing process and to maintain consistency. A cable tester should be available that can do cable length tests for UTP and coax. Work individually or in teams. The following resources will be required: CAT 5 straight or crossover cables of different colors. (some good and some bad) Coax (thinnet) cables of different lengths Cable Tester (Fluke 620 LAN CableMeter or similar) to test cable length Related Research Web Sites : Here are several web sites where you can get additional information on cabling standards: http://www.bicsi.org/techsem http://www.fluke.com/ Step 1. Set the Advanced Cable Tester for the Desired cable (UTP or COAX) These instructions pertain to the Fluke 620 LAN CableMeter. Turn the rotary switch selector on the tester to the LENGTH position. Press the SETUP button to enter the setup mode and observe the LCD screen on the tester. The first option should be CABLE: Press the UP or DOWN buttons until the desired cable type of UTP or COAX (thinnet) is selected. Press ENTER to accept that setting and go to the next one. Continue pressing the UP/DOWN arrows and pressing ENTER until the tester is set to the following cabling characteristics depending on the type of cable you will be testing.
Tester Option | Desired Setting - UTP | Desired Setting - COAX
CABLE: | UTP | COAX
WIRING: | 10BASET or EIA/TIA 4PR | 10BASE2 or RG58 (thinnet)
CATEGORY: | CAT 5 | N/A
WIRE SIZE | AWG 24 | N/A
CAL to CABLE? | NO | NO
BEEPING: | ON or OFF | ON or OFF
LCD CONTRAST | From 1 thru 10 (brightest) | From 1 thru 10 (brightest)
> Step 2. Setup the Cable to be Tested (UTP or COAX) For each UTP cable to be tested with the following tests, place the near end of the cable into the RJ45 jack labeled UTP/FTP on the tester. Place the RJ45-RJ45 female coupler on the far end of the cable and then insert the Cable Identifier into the other side of the coupler. The coupler and the cable identifier are accessories that come with the Fluke 620 LAN CableMeter. For coax cables, insert one end of the BNC connector into the jack labeled COAX on the tester. Coax cables should not be terminated. If tested with a terminating resistor (50 W), the display will be the resistance of the cable plus the terminating resistor. Step 3 – Perform Cable Length Test Function Using the tester Test function and a Cable ID Unit (for UTP), you can determine the functionality of the cable. Perform a Basic cable Test on each of the cables provided and fill in the following table based on the result for each CAT 5 cable tested. For each cable, write down the number and color, whether the cable is straight thru or crossover or coaxial, the tester screen test results and what you think the problem is. For UTP cables, press the down arrow or up arrow to see all pairs.
> Cable No. | Cable Color | How cable is wired (UTP or coax) | Tester Displayed Test Results (Note: refer to the Fluke manual for detailed description of test results) | Problem
> 1 |  |  |  |
2 |  |  |  |
3 |  |  |  |
4 |  |  |  |