Chapter 7: Novell IPX Commands:
debug ipx routing activity | Displays information about Routing Information Protocol (RIP) update packets.
debug ipx sap | Displays information about Service Advertising Protocol (SAP) update packets.
encapsulation novell-ether | Specifies that Novell's unique frame format is used on a network segment.
encapsulation sap | Specifies that Ethernet 802.2 frame format is used on a network segment. Cisco's keyword is sap.
interface | Configures an interface type and enters interface configuration mode.
ipx delay | Sets the tick count.
ipx ipxwan | Enables the IPXWAN protocol on a serial interface.
ipx maximum-paths | Sets the number of equal-cost paths the Cisco IOS software uses when forwarding packets.
ipx network | Enables Internetwork Packet Exchange (IPX) routing on a particular interface and optionally selects the type of encapsulation (framing).
ipx router | Specifies the routing protocol to use.
ipx routing | Enables IPX routing.
ipx sap-interval | Configures less frequent SAP updates over slow links.
ipx type-20-input-checks | Restricts the acceptance of IPX type 20 propagation packet broadcasts.
network | Assigns a NIC-based address to which the router is directly connected. Associates networks with an IGRP routing process. Enables Enhanced IGRP on a network in IPX router configuration mode.
ping | Sends ICMP echo request packets to another node on the network. Checks host reachability and network connectivity. Diagnoses basic network connectivity.
show ipx interface | Displays the status of the IPX interfaces configured in the Cisco IOS software and the parameters configured on each interface.
show ipx route | Displays the content of the IPX routing table.
show ipx servers | Displays the IPX server list.
show ipx traffic | Displays the number and type of packets.
show protocols | Displays the configured protocols.