Chapter 1-8 Commands
Chapter 1: The OSI Reference Model and Routing
ip address | Sets the logical network address of the interface.
network | Assigns a NIC-based address to which the router is directly connected. Associates networks with an IGRP routing process. Enables Enhanced IGRP on a network in IPX router configuration mode.
network-number | Specifies a directly connected network.
ping | Sends ICMP echo request packets to another node on the network. Checks host reachability and network connectivity. Diagnoses basic network connectivity.
protocol | Defines an IP routing protocol, which can be either RIP, Interior Gateway Routing Protocol (IGRP), Open Shortest Path First (OSPF), or Enhanced IGRP.
router rip | Selects RIP as the routing protocol.
term ip netmask-format | Specifies the format in which network masks are displayed in show command output.
Chapter 2: L AN Switching
show spantree | Displays spanning-tree information for a virtual local-area network (VLAN).
Chapter 3: VLANs
There are no commands from Chapter 3
Chapter 4: LAN Design
There are no commands from Chapter 4
Chapter 5: Routing Protocols: IGRP
metric holddown | Keeps new IGRP routing information from being used for a certain period of time.
network | Assigns a NIC-based address to which the router is directly connected. Associates networks with an IGRP routing process. Enables Enhanced IGRP on a network in IPX router configuration mode.
router igrp | Enables an IGRP routing process.
timers basic | Controls how often IGRP sends updates.
Chapter 6: ACLs
access-group | Applies access control lists (ACLs) to an interface.
access-list | Defines a standard IP ACL.
deny | Sets the conditions for a named IP ACL.
interface | Configures an interface type and enters interface configuration mode.
ip access-group | Controls access to an interface.
ip address | Sets the logical network address of the interface.
permit | Sets conditions for a named IP ACL.
show access-lists | Displays the contents of all current ACLs.
show ip interface | Lists a summary of an interface's IP information and status.
Chapter 7: Novell IPX
debug ipx routing activity | Displays information about Routing Information Protocol (RIP) update packets.
debug ipx sap | Displays information about Service Advertising Protocol (SAP) update packets.
encapsulation novell-ether | Specifies that Novell's unique frame format is used on a network segment.
encapsulation sap | Specifies that Ethernet 802.2 frame format is used on a network segment. Cisco's keyword is sap.
interface | Configures an interface type and enters interface configuration mode.
ipx delay | Sets the tick count.
ipx ipxwan | Enables the IPXWAN protocol on a serial interface.
ipx maximum-paths | Sets the number of equal-cost paths the Cisco IOS software uses when forwarding packets.
ipx network | Enables Internetwork Packet Exchange (IPX) routing on a particular interface and optionally selects the type of encapsulation (framing).
ipx router | Specifies the routing protocol to use.
ipx routing | Enables IPX routing.
ipx sap-interval | Configures less frequent SAP updates over slow links.
ipx type-20-input-checks | Restricts the acceptance of IPX type 20 propagation packet broadcasts.
network | Assigns a NIC-based address to which the router is directly connected. Associates networks with an IGRP routing process. Enables Enhanced IGRP on a network in IPX router configuration mode.
ping | Sends ICMP echo request packets to another node on the network. Checks host reachability and network connectivity. Diagnoses basic network connectivity.
show ipx interface | Displays the status of the IPX interfaces configured in the Cisco IOS software and the parameters configured on each interface.
show ipx route | Displays the content of the IPX routing table.
show ipx servers | Displays the IPX server list.
show ipx traffic | Displays the number and type of packets.
show protocols | Displays the configured protocols.
Chapter 8: Network Management
There are no commands for Chapter 8