Test parameters :: | 27/55
| The primary field test parameters are: Wire map Length Insertion loss Near-end crosstalk (NEXT) Power sum near-end crosstalk (PSNEXT) Equal-level far-end crosstalk (ELFEXT) Power sum equal-level far-end crosstalk (PSELFEXT) Return loss Propagation delay Delay skew NOTE - Other parameters such as longitudinal balance and longitudinal impedance, which may be of importance to specific networking applications, are under study.
Test parameters :: | 27/55