Work area telecommunications outlet/connector :: | 10/55
| 100 Ohm balanced twisted-pair telecommunications outlet/connector Requirements Each four-pair cable shall be terminated in an eight-position modular outlet at the work area. Telecommunications outlet/connectors for 100 Ohm UTP and ScTP cabling shall meet the requirements of ANSI/TIA/EIA-568-B.2 and the terminal marking and mounting requirements specified in ANSI/TIA/EIA-570-A. Pin/pair assignments shall be as shown below. The T568B pin/pair assignments may be used if necessary to accommodate certain 8-pin cabling systems. These illustrations depict the front view of the telecommunications outlet/connector.
Work area telecommunications outlet/connector :: | 10/55