Optical fiber telecommunications outlet connectors :: | 11/55
| Requirements Horizontal optical fiber cabling at the work area outlet shall be terminated to a duplex optical fiber outlet/connector meeting the requirements of ANSI/TIA/EIA-568-B.3. Recommendations To facilitate inter-office moves, consider the use of one style of duplex connector for the work area outlet. The 568SC connector was previously specified by ANSI/TIA/EIA-568-A and should continue to be considered for the work area outlet. Other connector styles, including those of a small form factor (SFF), may also be considered. Requirements Work area cords (all media types) The maximum work area cable (cord) length shall not exceed 5 m (16 ft). All cords used in the work area shall meet or exceed the performance requirements in ANSI/TIA/EIA-568-B.2 and ANSI/TIA/EIA-568-B.3.
Optical fiber telecommunications outlet connectors :: | 11/55