Cabling installation requirements :: | 18/55
| Requirements Cable and components shall be visually inspected for proper installation. Recommendations Cable stress, such as that caused by tension in suspended cable runs and tightly cinched bundles, should be minimized. Cable ties used to bundle cables should be applied loosely to allow the cable tie to slide around the cable bundle. The cable ties should not be cinched so tightly as to deform the cable sheath. Cable placement should not deform the cable sheath.
Cabling installation requirements :: | 18/55