Backbone cabling design recommendations :: | 46/55
| Backbone cabling design recommendations The intrabuilding backbone subsystem should be designed with sufficient spare capacity to service additional outlet/connectors from the centralized cross-connect without the need to pull additional intrabuilding backbone cables. The intrabuilding backbone fiber count should be sized to deliver present and future applications to the maximum work area density within the area served by the telecommunications room. Generally, two fibers are required for each application delivered to a work area.
Backbone cabling design recommendations :: | 46/55