| Engineering Journal 6.2.1: Numbered ACL configuration example The following example defines ACLs 1 and 2: interface ethernet 0 ip address 1.1.1.1 255.0.0.0 ip access-group 1 in ip access-group 2 out ! access-list 1 permit 5.6.0.0 0.0.255.255 access-list 1 deny 7.9.0.0 0.0.255.255 ! access-list 2 permit 1.2.3.4 access-list 2 deny 1.2.0.0 0.0.255.255 Suppose the interface receives 10 packets from 5.6.7.7, and 14 packets from 1.2.23.21. The first log will look like this: list 1 permit 5.6.7.7 1 packet list 2 deny 1.2.23.21 1 packet