Optical fiber cable transmission performance parameters :: | 50/55
Optical fiber cable type | Wavelength (nm) | Maximum attenuation (dB/km) | Minimum informationtransmission capacityfor overfilled launch (MHz km)
50/125 µm | 850 nm | 3.5 | 500
| 1300 nm | 1.5 | 500
62/125 µm | 850 nm | 3.5 | 160
| 1300 nm | 1.5 | 500
Single Mode | 1310 nm | 1.0 | N/A
Inside plant cable | 1550 nm | 1.0 | N/A
Single Mode | 1310 nm | 0.5 | N/A
Outside Plant Cable | 1550 nm | 0.5 | N/A
Optical fiber cable transmission performance parameters :: | 50/55