Choosing types of horizontal cabling :: | 3/55
| Requirements A minimum of two telecommunications outlet/connectors for each individual work area. NOTE: One telecommunications outlet/connector may be associated with voice and the other with data. Consideration should be given to installing additional outlet/connectors based on present and projected needs. The two telecommunications outlet/connectors shall be configured as: Four-pair 100 Ohm cable, category 3 or higher (category 5e recommended) as specified in ANSI/TIA/EIA-568-B.2. The other/second telecommunications outlet/connector shall be supported by a minimum of one of the following horizontal media. Four-pair 100 Ohm category 5e cable as specified in ANSI/TIA/EIA-568-B.2. Two-fiber multimode optical fiber cable, either 62.5/125 µm or 50/125 µm as specified in ANSI/TIA/EIA-568-B.3.
Choosing types of horizontal cabling :: | 3/55