Backbone link measurement :: | 41/55
| The backbone optical fiber cabling link segment shall be tested in one direction at both operating wavelengths to account for attenuation deltas associated with wavelength. Singlemode backbone links should be tested at 1310 nm and 1550 nm in accordance with ANSI/TIA/EIA-526-7, Method A.1, One Reference Jumper. Multimode backbone links shall be tested at 850 nm and 1300 nm in accordance with ANSI/TIA/EIA-526-14A, Method B, One Reference Jumper. Because backbone length and the potential number of splices vary depending upon site conditions, the link attenuation equation should be used to determine acceptance values at each of the applicable wavelengths.
Backbone link measurement :: | 41/55