|  | 3.3 | VLAN Implementation
| 3.3.3 | Static VLANs
Static VLANs are ports on a switch that you statically assign to a VLAN. These ports maintain their assigned VLAN configurations until you change them. Although static VLANs require the administrator to make changes, they are secure, easy to configure, and straightforward to monitor. Static VLANs work well in networks in which moves are controlled and managed.