|  | 6.5 | The Configuration of Basic Frame Relay
| 6.5.1 | Writing the IOS command sequence to completely configure Frame Relay

A basic Frame Relay configuration assumes that you want to configure Frame Relay on one or more physical interfaces and that LMI and Inverse ARP are supported by the remote router(s). In this type of environment, the LMI notifies the router about the available DLCIs. Inverse ARP is enabled by default, so it does not appear in configuration output. Use the following steps to configure basic Frame Relay.
| Engineering Journal
Configuring Security

| Web Links
| Configuring Frame Relay