Chapter 6: Frame Relay Commands:
enable password | Specifies a password to prevent unauthorized access to the router.
encapsulation frame-relay | Enables Frame Relay encapsulation.
end | Exits configuration mode.
exec-timeout | Sets the interval that the EXEC command interpreter waits until user input is detected.
exit | Exits any configuration mode or closes an active terminal session and terminates the EXEC.
frame-relay local-dlci | Enables the Local Management Interface (LMI) mechanism for serial lines using Frame Relay encapsulation.
hostname | Configures the router with a host name, which is used in prompts and default configuration filenames.
interface serial | Selects the interface and enters interface configuration mode.
ip address | Sets the logical network address of the interface.
ip unnumbered | Enables Internet Protocol (IP) processing on a serial interface without assigning an explicit IP address to the interface.
ipx network | Enables Internetwork Packet Exchange (IPX) routing on a particular interface and optionally selects the type of encapsulation (framing).
keepalive | Enables the LMI mechanism for serial lines using Frame Relay encapsulation.
line console | Configures a console port line.
line vty | Specifies a virtual terminal for remote console access.
login | Enables password checking at terminal session login.
ping | Sends ICMP echo request packets to another node on the network. Checks host reachability and network connectivity. Diagnoses basic network connectivity.
show frame-relay lmi | Displays statistics about the LMI.
show frame-relay map | Displays the current map entries and information about the connections.
show frame-relay pvc | Displays statistics about PVCs for Frame Relay interfaces.
show interfaces serial | Displays information about a serial interface.