This diskette image is for the IBM
4X Stereo PCMCIA CD-Rom Drive (1969009).
This image is for Sound Diskette 2,
which should have been included with the
(1969009) 4X Stereo PCMCIA CD-Rom Drive.
The 4X Stereo PCMCIA CD-Rom Drive should
have included two Sound Diskettes as well
as a Setup Diskette. 

The following should be found after the
4XSND22.ZIP image is unzipped. 


Volume in drive A has no label.
The Volume Serial Number is 2314:5815.

Directory of A:\

TTIMER   EX_    16355   2-27-96   1:00a
TTIMER   HL_     6020   2-27-96   1:00a
AUDCLIPS EX_    13685   2-27-96   1:00a
AUDCLIPS HL_     6536   2-27-96   1:00a
KISS     WA_     3825   2-27-96   1:00a
FROG     WA_    32215   2-27-96   1:00a
CANNON   WA_    60236   2-27-96   1:00a
BIRD     WA_    57166   2-27-96   1:00a
LASER    WA_    36143   2-27-96   1:00a
M16      WA_    42130   2-27-96   1:00a
PHNRING  WA_    24936   2-27-96   1:00a
SKIDS    WA_    59174   2-27-96   1:00a
CAT      WA_    80143   2-27-96   1:00a
CAR      WA_   120256   2-27-96   1:00a
APPLAUS  WA_    51856   2-27-96   1:00a
URGENT   WA_     8353   2-27-96   1:00a
REMINDER WA_     9179   2-27-96   1:00a
THANKHLP WA_    10769   2-27-96   1:00a
FAXED    WA_    10687   2-27-96   1:00a
CALLME   WA_    11474   2-27-96   1:00a
TIMETOGO WA_    11482   2-27-96   1:00a
BOTTOMLN WA_    11766   2-27-96   1:00a
TMELUNCH WA_    11853   2-27-96   1:00a
YCOMMENT WA_    13143   2-27-96   1:00a
CONFIDTL WA_    13946   2-27-96   1:00a
LION     WA_    68618   2-27-96   1:00a
SFXHELIC WA_    85342   2-27-96   1:00a
SFXTHUND WA_    90723   2-27-96   1:00a
SFXTRAIN WA_    86346   2-27-96   1:00a
QUEST1   WA_    47095   2-27-96   1:00a
QUICHITS WA_    87450   2-27-96   1:00a
START    WA_    65106   2-27-96   1:00a
COMMA    WA_   176261   2-27-96   1:00a
       33 file(s)    1430269 bytes used
Total files listed:
       33 file(s)    1430269 bytes used
                       19968 bytes free


The following information is from the
User's Guide to the 4X PCMCIA CD-Rom Drives.
The User's Guide provides a Quick Install
section as well as a detailed installation
section. Follow the User's Guide to install
the Drive. The User's Guide will also
include Software Installation steps.


Installing the Drive Software
Use the installation instructions for the
operating system installed in your computer.

DOS and Windows 3.1x
Use these instructions for both the
base and stereo models:
1. Turn on the computer and turn on the
   CD ROM drive by moving the power
   switch (19) to the on positon.
2. Insert the correct setup diskette
   into diskette drive A: [stereo model
   setup diskette (78H5109) is not the
   same as the base model setup
   diskette (52H3388)].
3. At the DOS command prompt, type
      A:INSTALL   then press enter.
4. Select one of the following options,
   then press enter:
 * Automatic Installation - installs the
   driver and updates the CONFIG.SYS
   and AUTOEXEC.BAT files.
 * Custom Installation - installs the
   driver and updates the CONFIG.SYS
   and AUTOEXEC.BAT files, but first
   lets you change the default IRQ
   and base I/O address.
5. You must confirm the selection by
   selecting Yes. Use the Up Arrow or
   Down Arrow keys to make your selection.
   Press enter. A message appears
   requesting that you restart the computer
   to make the changes take effect.
6. Restart DOS
(page 2-9)


Windows 3.1x Audio Utility (Stereo Model Only)
The stereo model provides an audio utility
for Windows 3.1x that includes sound and
miscellaneous functions. Follow the steps
to install the utility:
1. Start Windows 3.1x (You will hear the
   Windows startup sound if you have
   successfully installed the device
   driver).
2. Insert the Sound Diskette 1 of 2 into
   the A: diskette drive.
3. Start the installation program.
  - Click on FILE from the Program
    Manager Menu Bar.
  - Click on RUN from the menu list.
  - Type A:SETUP and press enter.
4. Review the    Welcome to ...
   and click on Continue.
5. Click on Software Installation.
6. Verify the directory for the installation
   of the audio utility (default is
   C:\PCAUDIO). Click on OK. You will be
   prompted to confirm the directory
   selection. Click on CONFIRM DIRECTORY.
7. Select one of the following options:
  - Complete Installation to install all
    the utility functions.
  - Custom Installation to install selected
    utility functions.
8. Follow the instructions and click on
   EXIT when the process completes.
If you have to resolve a resource conflict,
or want to customize the installation, you
can edit the CD-ROM device driver statement
in the CONFIG.SYS file:

DEVICE=C:\CD400\PCMCDSND.SYS /I:nn /P:nnn
  /D:aaaaaaa /NOBEEP

where:
  /I:nn      To assign an IRQ number (nn) to
             the device driver. The IRQ levels
             you can use with the CDRom drive
             are 7, 9, 11, and 15.
  /P:nnn     To assign a specific I/O address
             (nnn) [hexadecimal] for the
             CD-Rom drive.
  /D:aaaaaaa To specify another device name
             for MSCDEX
  /NOBEEP    To make the device not beep at
             the insertion of the PCMCIA card.
(page 2-10)


Windows 95
Use these instructions for both the base and
stereo models. The Windows 95 installation
process leads you through the installation
process once started. Follow these steps:
1. Turn on the computer and turn on the CD-ROM
   drive by moving the power switch (19) to
   the on position. the CD-ROM drive must
   be connected to the computer.
2. Start Windows 95.
3. Windows 95 recognizes a new drive and
   displays the New Hardware window. Select
   DRIVER PROVIDED BY HARDWARE MANUFACTURER,
   and click on OK.
4. Insert the Setup Diskette into the
   A: diskette drive for the correct
   CD-ROM drive.
5. When you see INSTALL FROM DISK, click
   on OK.
6. When you see the message, DO YOU WANT
   TO RESTART YOUR COMPUTER NOW?, click
   YES. Remove the Setup Diskette from
   the diskette drive.

OS/2 Warp with the Base Model
Use these instructions to install the
base model under OS/2 Warp:
1. Turn on the computer and turn on the
   CD-ROM drive by moving the power
   switch (19) to the on position.
2. Insert the correct Setup Diskette
   into the A: diskette drive for
   the CD-ROM drive model.
3. Double-click on the OS/2 System
   folder and then on System Setup.
4. Double-click on Device Driver Install.
5. Modify the destination directory and
   path or accept the default destination
   path, then click on INSTALL.
6. Click on OK on the Installation Information
   window. Note that Selective Install is not
   required when using these instructions.
7. Click on EXIT on the OS/2 Device
   Driver Installation Window.
8. Click on YES when the message, Exit the
   Program appears.
9. Click on OK when the message, Changes have
   been made to your system configuration. You
   must perform a shutdown and restart OS/2
   for these changes to take effect appears.
(page 2-11)


OS/2 Warp with the Stereo Model
Use these instructions to install the stereo
model under OS/2 Warp:
1. Verify the presence of Multimedia Presentation Manager:
  a. Start OS/2.
  b. If the MMPM/2 is installed on the computer, the
     Multimedia Folder is found on the OS/2 desktop.
     If MMPM/2 is not installed, refer to the OS/2 Warp
     documentation for installation instructions.
2. Install the CD-ROM Device Driver:
  a. Turn on the computer and turn on the CD-ROM drive by
     moving the power switch (19) to the ON position.
  b. Insert the correct Setup Diskette into the A:
     diskette drive for the CD-ROM Drive model.
  c. Double-click on the OS/2 System folder and then
     on System Setup.
  d. Double-chck on Device Driver Install.
  e. Modify the destination directory and path,
     or accept the default destination, then click
     on Install.
  f. Click on OK on the Installation Information
     window. Note that Selective Install is not
     required during this part of the installation.
  g. Click on Exit on the OS/2 Device Driver Installation
     window.
  h. Click on YES when the message, Exit the
     Program appears.
  i. Click on OK when the message, Changes have been made
     to your system configuration. You must perform a
     shutdown and restart OS/2 for these changes to take
     effect appears.
  j. Shut down and restart OS/2.

Install Sound Support
  a. Insert the Setup Diskette into drive A.
  b. Double-click on OS/2 System and then on Drives.
  c. Double-click on Drive A.
  d. Double-click on MINSTALL.EXE to start the program.
  e. Click on External 4X PCMCIA if it is not already
     selected, then click on Install.
  f. Click on Yes on the MMPM/2 Change CONFIG.SYS
     window.
  g. Verify that the number of devices is 1 on the
     Multimedia Installation window, then click on OK.
  h. Click on OK when the message MMPM/2 - CONFIG.SYS
     Changed appears.
  i. Click on OK when the message: MMPM/2 Installation
     Successful appears.
  j. Shut down and restart OS/2.

If you have to resolve a resource conflict, or want to
customize the installation, you can edit the CONFIG.SYS
file:

BASEDEV=CD400CRD.SYS /P:nnn /EXIRQ:n /NOBEEP

where
 /P:nnn    To assign a specific I/O address
           (nnn) (hexadecimal) to the
           CD-Rom drive.
 /EXIRQ:n  To exclude the spcified IRQ number (n).
           The program assigns another IRQ number
           to the CD ROM drive. The IRQ levels you
           can use with the CD ROM drive are 7, 9,
           11, and 15.
 /NOBEEP   To make the device not beep at the
           insertion of the PCMCIA card.
(page 2-12)


Completing the Installation
Ensure that you have shut down and restarted
the operating system so that you can use
the drive. Note the following results from the
installation process:
* The installation process assigns a drive letter
  to the CD Rom drive. If the computer has more
  than one PCMCIA card slot, the process identifies
  the slot with the CD Rom PCMCIA card and enables
  access to the drive.
* The drive letter assigned at installation remains
  unchanged even if the PCMCIA card is inserted
  into another available slot.
* The CD Rom drive operates the same regardless
  of whether the computer starts with or without
  the PCMCIA card inserted into the PCMCIA
  card slot.
* If using stereo model under OS/2 Warp, new icons
  are added to the Multimedia folder when the
  stereo modem sound support has been installed.
  To use the sound support, double-click the
  corresponding icon.
(page 2-13)
