Client Service Pack 3.0
_______________________
	*  Important installation notes
	*  What's new in SP 3.0
	*  Verifying if your new system is up-to-date
	*  Installing the client update on your update server
        *  How to customize the installsp30.xml 
	*  Updating your N2200w


Important installation notes

        *When updating an OS image or downloading a configuration, the update file type you
         use is dependent on your version of the NetVista thin client.
		·	For WBT SP 1.1 or earlier, use .XML files.
		·	For WBT SP 2.0 or later use .BUD files.

	*If you are upgrading to Service Pack 3 from Service Pack 1.1 or earlier, you
         will need to use the .XML files at the initial upgrade. After the initial upgrade
         use .BUD files.

	*Use http or ftp as the transport protocol.  If using FTP, the server MUST support
         the PASV flag (passive FTP).  Microsoft Internet Information Server is known to
         support this flag.

	*If your update server is using http as the transport protocol, ensure that the http          
         server directory permissions for the update directory (e.g. sp30) DO NOT have 
         execute turned on.

---------------------
What's new in SP 3.0

        *What follows is an overview of what is new in Service Pack 3.0.
         For more detailed and the most up-to-date information, visit our website:
                http://www.ibm.com/pc/support

		* Select NetVista, then select NetVista thin client
                * Under Technical Information, click on "Hot News"
                * Select the following document: NetVista N2200w (8363-Wxx)
                * Service packs

Citrix ICA v6 client
User Accounts (individual connection lists)
Japanese Keyboard support
NFUSE external viewer support (start the Citrix connection inside a web browser, but not embedded in the web page).
ISP Dial-In
AT Dial Strings

----------------------------

Verifying if your new system is up-to-date

        It is strongly recommended that before you start to configure your new N2200w
        system, first check to see if it is already loaded with the latest WBT software. To
        do this: 
        1.  Go through the Setup Wizard and wait for the system to restart.
        2.  After the system restarts, it will display the Terminal Connection Manager.
        3.  Press <F2> key to activate the Terminal Properties dialog box
        4.  Click on the "System" tab and check the "Build Version Information"
        5.  If the Build Number is 1087_1, your software is already up-to-date and you can
            skip software update steps and start configuring and using your system.  If the
            Build Number is at 0302, you need to update your system software by using
            .BUD files.

        *  If your Build Version is previous to 0302(SP2), you must use .XML to update to
           the new level of code.

-------------------------

*Instructions on how to update WBT from SP2 to SP3 using .BUD files are described in the N2200W Reference Information at the following URL:
		http://www.ibm.com/nc/pubs

If you are updating from a pre SP2 service pack, you need to install the update using the following XML instructions:

Installing the Client Code on your server using XML:

        To update your client software you must first setup an update server:
        1.  Make sure you have a HTTP server or a FTP server, with anonymous
            login support, as your update server.
        2.  Install the software update package from  the CD  into the appropriate folder on                           
            the update server.

        The SP3.0 is packaged in the client directory on the CD. You must first copy the
        contents into a subdirectory accessible by update protocol on your update server.
        For example, if you are using Microsoft IIS with its default HTTP root directory,
        you can create a folder sp30 as follows:
                 c:\inetpub\wwwroot\sp30 

        You  then copy  all the files in the client subdirectory into this folder. With this                         
        example, the Update URL you  specify on your client systems is:
	         http://update_server/sp30/installsp30.xml

        Where update_server should be substituted with the actual host name or the IP 
        address of the update server. 

        3.  Edit the XML (installsp30.xml) file to reflect your server environment.  You
            need to modify the update XML files with the address of the update server.

-------------------------
How to customize the installsp30.xml 

	You need to customize the installsp30.xml file based on:
		The transport protocol you choose to use (http or ftp)
		The server host name/IP address of your update server
		The directory path used to access the files

	installsp30.xml file:

	<?xml version="1.0" encoding="UTF-8"?>
	<!DOCTYPE Package SYSTEM "SoftwareUpdate.dtd">
	<!-- Upgrade to IBM WBT SP30-->
	<Package ID="1087">
	    <CopyFile>
 	      <Description>Copy getconfig.exe</Description>
     	      <Source>http://update_server/sp30/getconfig.exe</Source>
    	      <Destination>getconfig.exe</Destination>
	    </CopyFile>
 	   <Execute WaitForExit="Yes">
        	<Description>Save Current Configuration</Description>
        	<FileName>getconfig.exe</FileName>
     	        <CommandLine> </CommandLine>
 	   </Execute>
	    <CopyFile OSImage="Yes" OSImageSize="0xB9018F">
	       <Description>Download Software Update for SP3.0</Description>
 	       <Source>http://update_server/sp30/nk_1087.bin</Source>
 	       <Destination>\Program Files\nk.bin</Destination>
 	   </CopyFile>
  	  <Reboot>Yes</Reboot>
	</Package>


Updating your N2200w
	1.  Press F2 to get into the Terminal Properties.  In the Terminal
	    Properties dialog box, click on the "Update" tab.
	2.  Enter the URL for the update server and update xml file. 
	    (e.g. http://update_server/sp30/installsp30.xml)
	3.  Click on the "Update Now . . . " button.
	4.  The system will restart and begin to update the system software.
	5.  After the update has been completed, the system will restart again.
	6.  After the system come back it will restore the save configuration, 
	    then restart again (you will only see a blank screen with a mouse 
            pointer briefly).
	7.  The system should now have the original configuration restored 
            with the new level of code.

*Instructions on how to update WBT from SP2 to SP3 using .BUD files are described in 
The NetVista N2200w Thin Client for Windows-based Terminal Standard 1.5 Reference 
Information available at the following URL:


			http://www.ibm.com/nc/pubs
