IBM USB (Travel) Keyboard with UltraNav - Readme Instructions

I. SYSTEM REQUIREMENTS

Software:
Windows 2000 or Windows XP

Hardware:
IBM or IBM-compatible PC with USB ports.


II. INSTALLATION INSTRUCTIONS

To install the software for your USB (Travel) Keyboard with UltraNav,
please follow below steps:

1. Turn your system on and start Windows.
2. Connect your USB (Travel) Keyboard with UltraNav to the USB port of your PC.
3. If this is the first that you connect the USB (Travel) Keyboard with UltraNav 
   to your system, some "New Device Found" messages may appear on the 
   screen. Follow the onscreen instructions to complete the installation.
4. Run the setup program within this package to install the software for
   your USB (Travel) Keyboard with UltraNav. 


If you would like to do manual installation by updating driver with Device
Manager, please follow below steps:

- Windows 2000 -
1.  Turn your system on, start Windows and logon into the system.
2.  Connect your USB (Travel) Keyboard with UltraNav to the USB port of your PC.
3.  System will automatically configure the USB (Travel) Keyboard with UltraNav 
    and install the standard driver.
4.  Open the Control Panel by clicking Settings from Start Menu.
5.  Double-click System icon and select Hardware tab.
6.  Click Device Manager button to launch the Device Manager.
7.  Expand the devices under Human Interface Device, locate 
    HID-Compliant consumer control device and double-click on it.
8.  In HID-Compliant consumer control device Properties, select the Driver tab and click on 
    the "Update Driver..." button.
9.  Click "Next" button in the showing dialog.
10. Select "Display a list of the known drivers for this device so that I can 
    choose a specific driver" item and click "Next" button in "Install Hardware
    Device Drivers" dialog.
11. Click "Have Disk..." button in the "Select Device Driver" dialog. In the
    "Install From Disk" dialog, input the right path of driver 
    or click "Browse..." button to look for driver manually then Click "OK" .
12. Choose the product you want to install and click "Next" button.
13. Follow the on-screen instructions to complete the driver installation.

- Windows XP -
1.  Turn your system on, start Windows and logon into the system.
2.  Connect your USB (Travel) Keyboard with UltraNav to the USB port of your PC.
3.  System will automatically configure the USB (Travel) Keyboard with UltraNav 
    and install the standard driver.
4.  Open the Control Panel by clicking Settings from Start Menu.
5.  Double-click System icon and select Device Manager tab.
6.  Expand the devices under Human Interface Device, locate 
    HID-Compliant consumer control device and double-click on it.
7.  In HID-Compliant consumer control device Properties, select the Driver tab and click on 
    the "Update Driver..." button.
8.  Select "Install from a list or specific location (Advanced)" item and click "Next"
    button.
9.  Choose "Don't search. I will choose the driver to install" item and click "Next" button.
10. Click "Have Disk..." button. In the "Install From Disk" dialog, input the
    right path of driver or click "Browse..." button to
    look for driver manually then Click "OK" .
11. Choose the product you want to install and click "Next" button.
12. Follow the on-screen instructions to complete the driver installation.



III. UNINSTALLATION INSTRUCTIONS

To remove this software, please follow below steps:

1. Open the Control Panel by clicking Settings from Start Menu.
2. Open the "Add/Remove Program" and select "IBM USB (Travel) Keyboard with UltraNav"
   from the list.
3. Click on the "Add/Remove" button and follow the instructions to
   complete uninstallation.
