ThinkP ad 760

760C , 760CD , 760E, 760ED ,

760L, 760LD , 760EL, & 760 ELD

IBM

T echnical Inf or mation,

Tips , and T echniques

V ersion 3.4

December 1996

Troubleshooting IBM Thinkpad Hardware Setup Problems

If you should experience problems setting up PCMCIA Cards or ISA Adapters (in the docking station), please follow the procedures listed below:

(1) Please ensure that your ThinkPad is using the latest BIOS release for that system. Later BIOS releases correct problems that users have experi-

enced with the earlier releases. Refer to the ThinkPad BIOS section to determine if you need to update your system’s BIOS.

(2) Make sure that your software drivers are at the correct release level and are setup properly. Refer to the ThinkPad PCMCIA Drivers section to

see if you need to update your system’s PCMCIA device drivers. If you are using Point Enablers, please ensure that they are at the latest release

level.

(3) Determine if any upper memory conflicts exist between the areas claimed by ThinkPad BIOS, Card & Socket Services, Point Enablers, the SCSI

Adapter found in IBM Docking Stations, and any ISA Adapters installed in the docking station. Refer to the ThinkPad Memory Map and the

ThinkPad Dock I & Dock II Memory Map sections.

The Device Driver DICRMU01.SYS /MA=C800-CFFF (DOS PCMCIA Resource Map Utility) sets the upper memory addresses used by Card &

Socket Services. The /MA parameter tells Card Services what locations in upper memory can be used by PCMCIA cards or Card Services, and

must match or be a subset of an excluded memory range on the EMM386 line of CONFIG.SYS.

(4) Microsoft Windows can overwrite the upper memory address used by Card & Socket Services. To prevent this, add an EmmExclude=XXXX-

XXXX statement to the [386 Enh] section of SYSTEM.INI (Where XXXX-XXXX is the same as the memory region as used in the /MA parameter

for the DICRMU01.SYS driver). If you are using point enablers, be sure to exclude any upper memory used by the enabler by adding an

EmmExclude statement to SYSTEM.INI.

(5) Make sure that no interrupt conflicts exist between ThinkPad devices, PCMCIA Cards, the SCSI Adapter found in the IBM Docking Stations, and

any ISA Adapters installed in the docking station. Refer to the ThinkPad Interrupt Assignments section to view the default interrupt assignments.

Please note that the ThinkPad System Setup Utility allows you to view and change interrupt assignments for many internal devices.

The Resource Map Utility (DOS - DICRMU01.SYS, OS/2 - ICRMU01.SYS) can automatically detect many IRQs already in use, but may not

detect all. Try excluding the IRQ of the onboard SCSI any ISA Adapters in the Docking Station by adding the /IX=xx parameter to the Resource

Map Utility (where xx is the IRQ number to exclude). Multiple IRQs may be specified by separating with a comma.

(6) Ensure that no DMA conflicts exist between internal ThinkPad devices and any ISA Adapters installed in the docking station. Please refer to the

ThinkPad DMA Assignments section.

(7) Some ISA Adapters in the IBM DOCK I and DOCK II may require the ISA Adapter Timing Fix. Please download YPTF012.EXE from the IBM

BBS.

Troubleshooting IBM Thinkpad MWAVE Modem Problems

If you should experience problems with the MWAVE DSP Modem, please follow the procedures listed below:

(1) Please ensure that your ThinkPad is using IBM ThinkPad MWAVE software Version 2.0 (or later). Earlier versions do not provide 28.8KBPS

support. Please review the Drivers section of this document for thecurrent MWAVE code.

(2) Review the communications settings for your modem software:

To Set: Select highest ranking available setting:

Modem type 1. Mwave modem

2. Generic Hayes-type modem

3. User-defined modem

4. Hayes SmartModem 2400

5. Hayes modem

6. Hayes compatible modem

7. Other (Note: If you select a modem of type "Other," you must include the proper modem initialization string. For most

applications, the initialization string "AT&F" will work. See the Mwave Modem online help for more information.)

Baud Rate 57,600 Kbps, or the maximum setting offered by your communications software.

COM Port COM 2

To determine if communications software configuration is a problem, test the modem using the Windows Terminal program (in the Accessories

Folder). Run Terminal. Select COM2. Select Settings, then Modem Commands and make sure that Hayes is selected, then select OK. Next,

type atdt at the command line and hit Enter. If you receive a dialtone, then you probably have a software configuration problem with your specific

modem software. If you do not receive a dialtone, continue with next step.

(3) Double click on the ThinkPad Setup Icon. The double click on the System Information Icon. Review the IRQ settings to ensure that (a) the DSP

device is active (default is IRQ10); (b) the modem device is active (default is IRQ3); and (c) no other devices conflict with the DSP and Modem

IRQs. Next, review the DMA settings to ensure that the DSP device is active (default DMA7) and that no other devices conflict with the DSP

device.

(4) Within the ThinkPad Setup Icon or Folder, double click on the Serial Icon. Please ensure that Serial Ports A & B are disabled or do not conflict

with the MWAVE Modem.

(5) Open MWAVE ThinkPad Icon or Folder. Double click on the Modem icon. This enables the MWAVE Modem. This program can be minimized.

However, it must remain running while using the MWAVE Modem (please note that this item does not apply to MWAVE 2.0 on Windows 3.1 or

MWAVE 2.1 on Windows 95).

Troubleshooting IBM Thinkpad MWAVE Modem Problems (continued)

(7) Lotus Notes users should download LOTMWAVE.EXE from the IBM BBS. This file provides Lotus Notes with a MWAVE modem definition.

(8) Microsoft Mail users should download MSMMWAVE.EXE from the IBM BBS. This file provides Microsoft Mail with a MWAVE modem definition.

(9) The MWAVE Device is initialized each time Microsoft Windows is started. This means that a communications session started in DOS would be

terminated when Windows is started. Users who need to start the MWAVE Modem in DOS and keep it running while starting Microsoft Windows

should use MWAVE Version 1.1 and download MWDOSMOD.EXE. A fix for MWAVE Version 2 should be available shortly.

Installing Windows 95 on the ThinkPad 760

(1) For complete Windows 95 directions, please download 760W95.TXT from the IBM BBS.

(2) The ThinkPad 760 uses a Trident Cyber9320 or 9385 Graphics Accelerator. Ensure that Windows 95 is installed using the ThinkPad 760 Win-

dows 95 Video Driver Diskette.

(3) It is STRONGLY RECOMMENDED that you update your system BIOS to the latest BIOS release before installing Windows 95 on your system.

Early BIOS releases do not support Plug & Play or MWAVE under Windows 95. Refer to the BIOS section for the latest BIOS level for you

ThinkPad.

(4) Install Windows 95. On ThinkPad’s with internal CD-ROM Drives, Windows 95 comes with a generic ATAPI CD-ROM driver and it will work with

the ThinkPad integrated CD-ROM. To make sure that you are using Windows 95 generic ATAPI CD-ROM driver, remove the following driver

from CONFIG.SYS: IBMTPCD.SYS.

Start the Windows 95 SETUP program. Follow the instructions that came with the Windows 95 program (normally File, Run, D:\SETUP). If you

are installing from a CD-ROM with the ThinkPad 760 internal CD-ROM drive, the CD-ROM and Diskette drives can only be swapped while the

system is powered off or in FULL Suspend mode (Suspend LED lit and one audible beep).

IMPORTANT: Follow these special instructions during the Windows 95 installation

"Setup Options" screen - Choose "Custom" setup

"Analyzing Your Computer" screen - Choose "No, I want to modify the hardware list". After clicking "Next", highlight "Display". In the right hand

box (Manufacturer and model) REMOVE the check mark from these two lines:

S3 801/805/928/864/964 Display Adapter

S3 Display Adapter

Then choose next and complete the Windows 95 installation.

(5) The ThinkPad Features Program for Windows works on Windows 95. If you install Windows 95 on a blank hard disk or you haven’t installed

ThinkPad Features Program, follow the instructions of "ThinkPad Features Program - Installing for Windows" in the ThinkPad User’s Guide.

Please ensure that you are at the latest levels (refer to Driver Levels section of this document).

(6) Enable the Windows 95 Integrated PCMCIA Support Software. Install the ThinkPad 760 Socket Services Driver and PC Card Director for Win-

dows 95 (using the Windows 95 & OS/2 PCMCIA Drivers diskette).

(7) To install MWAVE Modem and Audio support, obtain the latest MWAVE DOS and MWAVE Windows 95 Drivers from the IBM BBS.

(8) You can use ThinkPad Infrared device driver on Windows 95. If you don’t have ThinkPad Infrared device driver version 2.01 or later, you may

encounter some problems. Refer to the Driver Levels section of this document.

Installing Windows 95 on the ThinkPad 760 (continued)

(9) The ThinkPad 760CD provides MPEG Video. Install the MPEG for Windows 95 support.

(10) If you are using an IBM PCMCIA Token-Ring Adapter, download TRCC1.EXE for an updated driver for Windows 95.

(11) Windows 95 treats the IBM Ethernet Credit Card Adapter as a Plug & Play Adapter. However, some older versions of this adapter do not support

Plug & Play. If you insert this adapter into a system running Windows 95, the system may lock until you remove the adapter. To correctly config-

ure this adapter for Windows 95, boot in Safe Mode, go into Device Manager, and manually configure the adpater for I/O 300, IRQ 9, Mem

Address D400.

(12) If you are using an Ethernet PCMCIA Adapter in the ThinkPad 760C, 760CD, 760L, or 760LD, please make sure your system’s BIOS is at version

1.22 or later. This BIOS release corrects some hang conditions when using Ethernet PCMCIA Adapters and Windows 95.

Installing Windows NT 4.0 on the ThinkPad 760

(1) Update your system BIOS to the latest BIOS release before installing Windows NT on your system.

(2) Download the latest ThinkPad Windows NT 4.0 Installation Instructions (TPWINT40.TXT) from the IBM BBS or Web site. Also download the

latest drivers required for your system (see Drivers for Windows NT section for the files to download)

(3) Install Windows NT on the ThinkPad.

(4) After NT has been installed, update the ThinkPad 760 Windows NT Video Device Driver. Use the ThinkPad Video Driver you downloaded from

the BBS. Insert the diskette in Drive A. Select Control Panel, then Display, then Settings, then Display Type, then Change, then Have Disk.

Choose IBM ThinkPad (Cyber 9320/9382/9385). Restart Windows NT after installation. After restart, select the proper resolution.

(5) Install the Windows NT version ThinkPad Utilities program. Using this program, you can change your hardware configuration, display the fuel

gauge, and set the device stand-by timers (same as in the Windows 3.1 or Windows 95 environments). Logoff and log back on to enable the

ThinkPad Utilities. Once you install the ThinkPad Utilities, Suspend/Resume and Power Management are supported under Windows NT.

(6) For the ThinkPad 760E, 760EL, 760ED, and 760ELD, install the ThinkPad PIIX Busmaster IDE Driver using the file from the IBM BBS. Close any

running applications. Insert the diskette in Drive A. Select Control Panel, then SCSI Adapters, then Drivers, the Add, the Have Disk. Select OK.

The Select IBM ThinkPad PIIX IDE Driver, then OK. Click No when asked if you want to restart NT.

Copy TPFDD.EXE and TPSWAP.EXE from the ThinkPad Utilities disk to your hard drive. TPFDD.EXE is used to change the active floppy drive

port for the ThinkPad 760. TPFDD.EXE I -- enables the internal floppy port. TPFDD.EXE E -- enables the external floppy port.

TPSWAP.EXE is used to enable/disable warm swapping of the floppy drive and the internal CD-ROM drive. TPSWAP.EXE E -- enables warm

swapping. TPSWAP.EXE D -- disables it. You need to restart Windows NT whenever you change this setting.

(7) For the ThinkPad 760L, 760LD, 760EL, & 760ELD models, Windows NT Audio Support is provided via a file from the IBM BBS. Install Audio

support using the appropriate diskette.

(8) For the ThinkPad 760C, 760CD, 760E, & 760ED models, Windows NT Audio & Modem Support is provided via MWAVE files from the IBM BBS.

Before installing MWAVE support, verify that the MWAVE Modem is enabled in the ThinkPad features program. Then, install MWAVE support for

Windows NT (for MWAVE systems).

(9) Install ThinkPad infrared support using the file from the IBM BBS.

Currently, the following functions are not supported on Windows NT:

(1) IBM MPEG-II (ThinkPad 760CD/ED) and enhanced video function such as video overlay features not supported.

(2) Hibernation functions are not supported on NTFS partitions.

(3) Windows NT supports the IBM Dock-I, Dock-II, SelectaDock Base Model I, and SelectaDock Model I/II. However, hot/warm docking is not sup-

ported. To use the device in the Docking station, you must power off the system prior to docking/undocking.

Installing OS/2 WARP on the ThinkPad 760

(1) Update your system BIOS to the latest BIOS release before installing OS/2 Warp on your system.

(2) Obtain the necessary driver diskettes from the IBM BBS or web site.

(3) The Thinkpad 760CD/LD/ED/ELD has a port on the back of the unit which will allow attachment of the floppy drive externally using IBM part

66G3618. Both the floppy drive and the CD-ROM drive must be attached to the machine in order to install from CD -ROM. The floppy and CD-

ROM drives can not be hot-swapped during installation. Non-CD Thinkpad 760 models can be installed via CD-ROM mounted in a docking

station.

(4) Boot the Thinkpad from the OS/2 WARP Installation diskettes and proceed through the first part of the installation.

(5) OS/2 WARP Version 4 users proceed to step 6. At the end of t his stage of installation, at the screen which says "...Remove the Diskette and

Press Enter to Restart the System..."; press the F3 key to exit to a command prompt.

At this point, insert the Video Graphics Fix for OS/2 Warp and from the A:\ prompt, type REPVGA x where x is the drive in which OS/2 has been

installed (i.e. REPVGA C for installation on drive C:). Remove the diskette from the drive and type EXIT to re turn back to the installation screen.

Press ENTER to proceed with the rest of the installation.

(6) After the Thinkpad re-boots to the System Configuration Screen, select VGA for the video display (the installation will auto-detect a Trident 8900,

this will not work).

(7) For the 760C and 760L series, choose Thinkpad 755CE/CsE for PCMCIA support. For the 760E series, chose No Support for PCMCIA support

(this is the default). For the 760L/LD and 760EL/ELD machines, select Multimedia Device Support and change to Port Address for the ESS 688

device to 240. For the Thinkpad 760CD/LD/ED/ELD models, select the Thinkpad 755CD, TEAC CD-40E for CD-ROM support. Select OK from

the System Configuration Screen and proceed with the installation of desired software components.

Note: The ESS 688 driver may give an error on re-boot if the device was not previously set to Port Address 240. Ignore the error and proceed

with the installation. Use the Thinkpad Features to set the device to 240 at the end of the installation.

(8) OS/2 WARP Version 4 users proceed to step 10. When this stage of the installation completes, at the screen which says "...System Configu-

ration is Complete...Remove Diskette and Press Enter...", reboot the machine and at the IBM Thinkpad logo, insert the OS/2 Warp Installation

disk and let the machine boot from the floppy. Insert diskette 1 and continue to the main installation screen. Press F3 to exit to the command

prompt.

(9) Insert the Video Graphics Fix for OS/2 Warp and from the A:\ prompt, type REPVGA x where x is the drive in which OS/2 has been installed (i.e.

REPVGA C for installation on drive C:). Remove the diskette and re-boot the machine.

(10 ) Install the Thinkpad Features for OS/2 using the INSTALL2 program from the Thinkpad Utilities diskette 1. The INSTALL2 program can be run

from an OS/2 window.

Installing OS/2 WARP on the ThinkPad 760 (continued)

(11) For the Thinkpad 760C and 760L series, installation of the PC Card Director v4.02 is not necessary unless the features of this version are desired.

It is required for the Thinkpad 760E series machines in order to utilize the PCMCIA controller on these machines. Install the PC Card director by

running the PCMINST2 command from the PC Card Director for OS/2 and Win95 -TP 760 v4.02 diskette.

(12) Install the Video Disk for OS/2 Warp by inserting the respective diskette for the Thinkpad being used and type INSTALL x, where x is the drive in

which OS/2 is installed; and follow the instructions.

Note: Due to the implementation of the Trident CYBER9320 and CYBER9385 chipsets in the Thinkpad 760 series, a machine CAN NOT be set back to

VGA using Alt-F1 on boot and choosing option V. This will install the default OS/2 Warp VGA drivers and the mac hine will boot to a black screen.

The Alt-F1 - M option for the Maintenance Desktop will work, and the machine will boot back into the proper VGA mode afterwards. A machine

can also be set back to VGA by using Selective Install for VGA, rebooting fro m diskette, and re-applying the Video Graphics Fix for OS/2 Warp

diskette.

(13) Install any other desired utilities for your system (MWAVE, Infrared, MPEG).Latest Version of ThinkPad BIOS

Latest Version of ThinkPad BIOS

Latest BIOS

ThinkPad Model Part Number Date BIOS Update on IBM BBS

760C, 760CD, 760L, & 760LD 91G2007 11/08/96 SYTPF124.EXE

760E Model 9546-U9B 11J9031 12/11/96 SYTPH101.EXE

760E (All Other Models) 11J9029 12/11/96 SYTPG105.EXE

760EL Models 9547-x4G & 9547-x4T Only 11J9030 12/11/96 SYTPG105.EXE

760EL (All Other Models) 11J9029 12/11/96 SYTPG105.EXE

760ELD 11J9029 12/11/96 SYTPG105.EXE

760ED Model 9546-U9A 11J9031 12/11/96 SYTPH101.EXE

760ED (All Other Models) 11J9030 12/11/96 SYTPG105.EXE

To view the BIOS Part Number, turn off the computer, press and hold F1, then turn on the computer. Hold F1 until the Easy-Setup menu appears.

Select Config followed by SystemBoard.

Upgrading The ThinkPad Flash BIOS

- You need an AC adapter and a charged battery pack to update the system program.

- If your computer is attached to a ThinkPad Docking Station or a port replicator, turn off the computer and detach it before proceeding.

(1) Firmly connect the AC adapter to the computer.

(2) Insert the System Program Service Diskette into the diskette drive and turn on the computer.

(3) Select "Update system program" and follow the instructions on the screen.

Warning: Do not turn off or suspend the computer until the update has been completed. IF YOU TURN OFF OR SUSPEND THE

COMPUTER WHILE THE UPDATE IS STILL IN PROGRESS, THE SYSTEM BOARD MAY HAVE TO BE REPLACED.

- After the update has been completed, you MAY need to initialize the system. Please note that initalizing the systems resets all customization

settings (IRQ, DMA, I/O, and Device Settings made with the ThinkPad Utilities) to the factory default.

(1) Remove the System Program Service Diskette from the diskette drive and turn off the computer.

(2) Press and hold F1, then turn on the computer. Hold F1 until the Easy-Setup menu appears.

(3) If a password prompt appears, type the correct password.

(4) Select Config, then select Initialize.

(5) Select OK to initialize system.

- You may want to run the diagnostics to make sure that the computer runs with no errors:

(1) Turn off the computer, press and hold F1, then turn on the computer. Hold F1 until the Easy-Setup menu appears.

(2) Select Test, then select Start to run all the basic tests.

(3) Verify that OK appears for all of the devices tested.

(4) Press Esc to exit Test and turn off the computer.

Latest Version of DOS Card & Socket Services Drivers for ThinkPad 760

File Name Driver Description Version File Date File Size

IBMDSS01.SYS DOS PCMCIA Socket Services Driver 2.02 04-03-96 16502

IBMDSS04.SYS DOS PCMCIA Socket Services Driver 2.02 04-19-96 14036

IBMDSS14.SYS DOS PCMCIA Socket Services Driver 2.02 04-19-96 15506

IBMDOSCS.SYS DOS PCMCIA Card Services Driver 3.11 05-13-96 41264

DICRMU01.SYS DOS PCMCIA Resource Map Utility 1.28 05-13-96 12733

$ICPMDOS.EXE DOS PC Card Power Management Driver 3.03 05-13-96 20092

AUTODRV.SYS DOS PCMCIA PC Card Auto Configurator 2.01 06-13-95 8361

Latest Version of OS/2 Card & Socket Services Drivers for ThinkPad 760

File Name Driver Description Version File Date File Size

IBM2SS01.SYS OS/2 PCMCIA Socket Services Driver 2.02 04-03-96 19014

IBM2SS04.SYS OS/2 PCMCIA Socket Services Driver 2.02 04-19-96 14926

IBM2SS14.SYS OS/2 PCMCIA Socket Services Driver 2.02 04-19-96 19400

PCMCIA.SYS OS/2 PCMCIA Card Services Driver 1.44 04-22-96 48646

VPCMCIA.SYS OS/2 Virtual Card Services Driver 1.40 04-22-96 13824

ICRMU01.SYS OS/2 PCMCIA Resource Map Utility 1.24 04-22-96 10381

$ICPMOS2.SYS OS/2 PC Card Power Management Driver 2.06 07-08-96 5992

AUTODRV2.SYS OS/2 PCMCIA PC Card Auto Configurator 2.01 03-22-96 9178

Latest Drivers for ThinkPad 760

IBM BBS File Name Driver Description Version File Date

Drivers for DOS/Windows 3.1x:

PCTPGW31.EXE DOS/Windows 3.1X PCMCIA Drivers 4.03 10-03-96

UTTPGDOS.EXE ThinkPad Utility Programs - DOS 3.51 10-31-96

UTTPGWIN.EXE ThinkPad Utility Programs - Windows 3.1X/Windows 95 3.51 10-31-96

VFTPGW31.EXE Windows 3.1X Video Drivers (All TP 760 Except 760ED) 1.10 08-20-96

VFTPKW31.EXE Windows 3.1X Video Drivers (TP 760ED Only) 1.10 08-26-96

MWD202-1.EXE MWAVE DOS Drivers (Disk #1) 2.02 06-21-96

MWD202-2.EXE MWAVE DOS Drivers (Disk #2) 2.02 06-21-96

MWW202-1.EXE MWAVE Windows Drivers (Disk #1) 2.02 06-21-96

MWW202-2.EXE MWAVE Windows Drivers (Disk #2) 2.02 06-21-96

AFTPGW31.EXE 760L/LD/EL/ELD Windows 3.1 Audio Driver 1.00 10-15-96

IRTPGALL.EXE Infrared Drivers 3.01 10-15-96

CDTPGW31.EXE CD-ROM Drivers 2.02 08-05-96

ATADO200.EXE PC Card Hard Disk Drive Device Drivers 2.00 03-22-94

MPTPFW31.EXE MPEG Windows Drivers (760CD Only) 1.11 01-30-96

MPTPGW31.EXE MPEG Windows Drivers (760ED Only) 1.12 01-02-97

VCTPGW31.EXE MPEG Capture Overlay - Windows (760ED Only) 1.11 09-25-96

MPTPGCD1.EXE MPEG Video CD Player (760CD/760ED ) 1.20 10-15-96

WIN32S11.EXE WIN32S Disk 1 of 2 (760CD/760ED ) 1.20 10-15-96

WIN32S21.EXE WIN32S Disk 2 of 2 (760CD/760ED ) 1.20 07-23-96

VETPFW31.EXE Enhanced Video (760CD Only) 08-30-96

Latest Drivers for ThinkPad 760

IBM BBS File Name Driver Description Version File Date

Drivers for Windows 95:

PCTPGO95.EXE Windows 95 & OS/2 PCMCIA Drivers 10-31-96

UTTPGDOS.EXE ThinkPad Utility Programs - DOS 3.51 10-31-96

UTTPGWIN.EXE ThinkPad Utility Programs - Windows 3.1X/Windows 95 3.51 10-31-96

VFTPGW95.EXE Windows 95 Video Drivers 1.10 10-15-96

MW9222A.EXE MWAVE Windows 95 Drivers (Disk #1) 2.22 10-17-96

MW9222B.EXE MWAVE Windows 95 Drivers (Disk #2) 2.22 10-17-96

MW9222C.EXE MWAVE Windows 95 Drivers (Disk #3) 2.22 10-17-96

AFTPGW95.EXE 760L/LD/EL/ELD Windows 95 Audio Driver 1.00 10-15-96

IRTPGALL.EXE Infrared Drivers 3.01 10-15-96

MPTPFW95.EXE MPEG Windows Drivers (760CD Only) 1.11 08-28-96

MPTPGW95.EXE MPEG Windows Drivers (760ED Only) 1.12 01-02-97

VCTPGW95.EXE MPEG Capture Overlay - Windows 95 (760ED Only) 1.11 09-25-96

MPTPGCD1.EXE MPEG Video CD Player (760CD/760ED ) 1.20 10-15-96

VETPFW95.EXE Enhanced Video (760CD Only) 1.10 09-17-96

Latest Drivers for ThinkPad 760

IBM BBS File Name Driver Description Version File Date

Drivers for OS/2:

PCTPGO95.EXE Windows 95 & OS/2 PCMCIA Drivers 10-31-96

UTTPGDOS.EXE ThinkPad Utility Programs - DOS 3.51 10-31-96

UTTPGOS2.EXE ThinkPad Utility Programs - OS/2 3.51 10-31-96

VFTPGOS2.EXE OS/2 Warp Video Drivers (All TP 760 Except 760ED) 1.10 08-26-96

VFTPKOS2.EXE OS/2 Warp Video Drivers (TP 760ED Only) 1.10 08-26-96

MWO202-1.EXE MWAVE OS/2 WARP Drivers (Disk #1) 2.02 06-21-96

MWO202-2.EXE MWAVE OS/2 WARP Drivers (Disk #2) 2.02 06-21-96

MWAUDOS2.EXE MWAVE Audio Driver for OS/2 WARP 2.02 06-04-96

AFTPGOS2.EXE 760L/LD/EL/ELD OS/2 Audio Driver 1.01 10-15-96

IRTPGALL.EXE Infrared Drivers 3.01 10-15-96

MPTPFOS2.EXE MPEG OS/2 WARP Drivers (760CD Only) 1.00 07-22-96

MPTPGOS2.EXE MPEG OS/2 WARP Drivers (760ED Only) 1.20 09-25-96

VCTPGOS2.EXE MPEG Capture Overlay - OS/2 (760ED Only) 1.10 09-25-96

VETPFOS2.EXE Enhanced Video (760CD Only) 1.00 08-28-96

Drivers for Windows NT:

UTTPGWNT.EXE ThinkPad Utility Programs - Windows NT 1.00 10-31-96

VFTP3WNT.EXE Windows NT 3.51 Video Drivers 1.10 10-31-96

VFTP4WNT.EXE Windows NT 4 Video Drivers 1.00 10-31-96

TPIDEWNT.EXE ThinkPad PIIX Busmaster IDE Driver 1.00 08-28-96

AFTP3WNT.EXE Windows NT 3.51 Audio Driver - 365X, 560, 760L & EL 1.10 10-31-96

AFTP4WNT.EXE Windows NT 4 Audio Driver - 365X, 560, 760L & EL 1.00 10-31-96

MWAVENT1.EXE MWAVE Windows NT (Disk #1) 2.2 11-05-96

MWAVENT2.EXE MWAVE Windows NT (Disk #2) 2.2 11-05-96

IRTPGWNT.ZIP Infrared Drivers - Windows NT 1.00 01-06-97

ThinkPad 760 Memory Map

Location Use

0000 - 9FFF System RAM

A000 - AFFF Video Graphics

B000 - B7FF Mono Video

B800 - BFFF Video Text

C000 - C7FF Video BIOS 1

C800 - DFFF Available 2

E000 - E7FF Available

E800 - EFFF Available

F000 - FFFF System BIOS

1 With some early BIOS versions, the ThinkPad 760ED’s Video BIOS was located at C000-CBFFF

2 Available means open for either PCMCIA card usage, ISA Adapter card usage (in Dock I or Dock II), or for mapping as upper memory blocks.

ThinkPad Dock I & Dock II Memory Map

Location of SCSI Adapter ROM in DOCK I Location of SCSI-II Adapter ROM in DOCK II

CA00-CBFF Default DC00-DFFF Default

C800-C9FF Selectable by Switch Setting C800-CBFF Selectable by Switch Setting

CE00-CFFF Selectable by Switch Setting CC00-CFFF Selectable by Switch Setting

DE00-DFFF Selectable by Switch Setting D000-D3FF Selectable by Switch Setting

D400-D7FF Selectable by Switch Setting

D800-DBFF Selectable by Switch Setting

Attaching Devices to the ThinkPad Dock I

Some CD-ROM Drives, SCSI Attached Scanners, and other devices require either an ASPI (Advanced SCSI Programming Interface) or CAM

(Common Access Method) driver. This support is provided by the PowerSCSI utility. This utility does not ship with your IBM ThinkPad DOCK I.

Please download POWRSCSI.DSK from the IBM BBS.

ThinkPad 760C Interrupt Assignments

2 3 4 5 7 9 10 11 15

Cascade Interrupt Req From IRQ 8-15 Default

DSP Modem Default Optional

Serial Port Optional Optional

Infrared Optional Default Optional Optional Optional Optional

DSP Sound Blaster Emulation Default Optional

Parallel Port Optional Default

DSP Audio Optional Optional Default Optional Optional

DOCK I Internal SCSI Optional Optional Optional Default

DOCK II Internal SCSI Optional Optional Default

UltraBay Hard Disk Drive Optional

PCMCIA Cards Optional Optional Optional Optional Optional Optional Optional Optional

ISA Adapters (In Docking Station) Optional Optional Optional Optional Optional Optional Optional Optional

Note 1

The following interrupts are used by the system: IRQ 0 (Timer), IRQ 1 (Keyboard), IRQ 6 (Floppy Diskette Drive), IRQ 8 (Real-time Clock), IRQ 12

(Mouse/Trackpoint), IRQ 13 (Math Coprocessor), and IRQ 14 (Hard Disk Drive).

Note 2

If you enable the second hard disk drive in the UltraBay, it must use IRQ 15. This could cause a conflict with an existing device.

ThinkPad 760C DMA Channel Assignments

DMA Default Assignment Other Possible Uses

DRQ0 Infrared MWAVE DSP, Sound Blaster Audio, Parallel Port ECP Mode

DRQ1 Sound Blaster Audio MWAVE DSP, Parallel Port ECP Mode

DRQ2 Diskette Drive

DRQ3 Infrared Parallel Port ECP Mode

DRQ4 Cascade

DRQ5 Unused

DRQ6 Unused MWAVE DSP, Sound Blaster Audio

DRQ7 MWAVE DSP Sound Blaster Audio

ThinkPad 760CD Interrupt Assignments

2 3 4 5 7 9 10 11 15

Cascade Interrupt Req From IRQ 8-15 Default

DSP Modem Default Optional

Serial Port Optional Optional

Infrared Optional Default Optional Optional Optional Optional

DSP Sound Blaster Emulation Default Optional

Parallel Port Optional Default

DSP Audio Optional Optional Default Optional Optional

DOCK I Internal SCSI Optional Optional Optional Default

DOCK II Internal SCSI Optional Optional Default

CD-ROM/UltraBay Hard Disk Drive Optional

MPEG Enhanced Video Optional Optional Default Optional Optional Optional

PCMCIA Cards Optional Optional Optional Optional Optional Optional Optional Optional

ISA Adapters (In Docking Station) Optional Optional Optional Optional Optional Optional Optional Optional

Note 1

The following interrupts are used by the system: IRQ 0 (Timer), IRQ 1 (Keyboard), IRQ 6 (Floppy Diskette Drive), IRQ 8 (Real-time Clock), IRQ 12

(Mouse/Trackpoint), IRQ 13 (Math Coprocessor), and IRQ 14 (Hard Disk Drive).

ThinkPad 760CD DMA Channel Assignments

DMA Default Assignment Other Possible Uses

DRQ0 Infrared MWAVE DSP, Sound Blaster Audio, Parallel Port ECP Mode

DRQ1 Sound Blaster Audio MWAVE DSP, Parallel Port ECP Mode

DRQ2 Diskette Drive

DRQ3 Infrared Parallel Port ECP Mode

DRQ4 Cascade

DRQ5 Unused MPEG Enhanced Video

DRQ6 MPEG Enhanced Video MWAVE DSP, Sound Blaster Audio

DRQ7 MWAVE DSP Sound Blaster Audio , MPEG Enhanced Video

ThinkPad 760E Interrupt Assignments

2 3 4 5 7 9 10 11 15

Cascade Interrupt Req From IRQ 8-15 Default

DSP Modem Default Optional

Serial Port Optional Optional

Infrared Optional Default Optional Optional Optional Optional

DSP Sound Blaster Emulation Default Optional

Parallel Port Optional Default

DSP Audio Optional Optional Default Optional Optional

Secondary IDE Optional

PCMCIA Cards Optional Optional Optional Optional Optional Optional Optional Optional

PCI IRQ (For PCI Devices) Optional Optional Optional Optional Optional Optional Default Optional

ISA Adapters (In Docking Station) Optional Optional Optional Optional Optional Optional Optional Optional

DOCK I Internal SCSI Optional Optional Optional Default

DOCK II Internal SCSI Optional Optional Default

SelectaDock Internal SCSI Optional Optional Optional Optional Optional Optional Default Optional

Note 1

The following interrupts are used by the system: IRQ 0 (Timer), IRQ 1 (Keyboard), IRQ 6 (Floppy Diskette Drive), IRQ 8 (Real-time Clock), IRQ 12

(Mouse/Trackpoint), IRQ 13 (Math Coprocessor), and IRQ 14 (Hard Disk Drive).

Note 2

The PCI Adapter in SelectaDock, and SelectaDock Internal SCSI share IRQ 11.

ThinkPad 760E DMA Channel Assignments

DMA Default Assignment Other Possible Uses

DRQ0 Infrared MWAVE DSP, Sound Blaster Audio, Parallel Port ECP Mode

DRQ1 Sound Blaster Audio MWAVE DSP, Parallel Port ECP Mode

DRQ2 Diskette Drive

DRQ3 Infrared Parallel Port ECP Mode

DRQ4 Cascade

DRQ5 Unused

DRQ6 Unused MWAVE DSP, Sound Blaster Audio

DRQ7 MWAVE DSP Sound Blaster Audio

ThinkPad 760ED Interrupt Assignments

2 3 4 5 7 9 10 11 15

Cascade Interrupt Req From IRQ 8-15 Default

DSP Modem Default Optional

Serial Port Optional Optional

Infrared Optional Default Optional Optional Optional Optional

DSP Sound Blaster Emulation/Midi Port Default Optional Optional Optional

Parallel Port Optional Default

DSP Audio Optional Optional Default Optional Optional

Secondary IDE Optional

MPEG Enhanced Video Optional Optional Optional Optional Optional Optional Default Optional

PCI IRQ (For PCI Devices) Optional Optional Optional Optional Optional Optional Default Optional

ISA Adapters (In Docking Station) Optional Optional Optional Optional Optional Optional Optional Optional

DOCK I Internal SCSI Optional Optional Optional Default

DOCK II Internal SCSI Optional Optional Default

SelectaDock Internal SCSI Optional Optional Optional Optional Optional Optional Default Optional

Note 1

The following interrupts are used by the system: IRQ 0 (Timer), IRQ 1 (Keyboard), IRQ 6 (Floppy Diskette Drive), IRQ 8 (Real-time Clock), IRQ 12

(Mouse/Trackpoint), IRQ 13 (Math Coprocessor), and IRQ 14 (Hard Disk Drive).

Note 2

The MPEG Enhanced Video, PCI Adapter in SelectaDock, and SelectaDock Internal SCSI all share IRQ 11.

ThinkPad 760ED DMA Channel Assignments

DMA Default Assignment Other Possible Uses

DRQ0 Infrared MWAVE DSP, Sound Blaster Audio, Parallel Port ECP Mode

DRQ1 Sound Blaster Audio MWAVE DSP, Parallel Port ECP Mode

DRQ2 Diskette Drive

DRQ3 Infrared Parallel Port ECP Mode

DRQ4 Cascade

DRQ5 Unused MPEG Enhanced Video

DRQ6 MPEG Enhanced Video MWAVE DSP, Sound Blaster Audio

DRQ7 MWAVE DSP Sound Blaster Audio , MPEG Enhanced Video

ThinkPad 760EL Interrupt Assignments

2 3 4 5 7 9 10 11 15

Cascade Interrupt Req From IRQ 8-15 Default

Serial Port Optional Optional

Infrared Optional Default Optional Optional Optional Optional

Parallel Port Optional Default

Audio Default Optional Optional

Secondary IDE Optional

PCI IRQ (For PCI Devices) Optional Optional Optional Optional Optional Optional Default Optional

ISA Adapters (In Docking Station) Optional Optional Optional Optional Optional Optional Optional Optional

DOCK I Internal SCSI Optional Optional Optional Default

DOCK II Internal SCSI Optional Optional Default

SelectaDock Internal SCSI Optional Optional Optional Optional Optional Optional Default Optional

Note 1

The following interrupts are used by the system: IRQ 0 (Timer), IRQ 1 (Keyboard), IRQ 6 (Floppy Diskette Drive), IRQ 8 (Real-time Clock), IRQ 12

(Mouse/Trackpoint), IRQ 13 (Math Coprocessor), and IRQ 14 (Hard Disk Drive).

Note 2

The PCI Adapter in SelectaDock, and SelectaDock Internal SCSI share IRQ 11.

ThinkPad 760EL DMA Channel Assignments

DMA Default Assignment Other Possible Uses

DRQ0 Infrared Audio, Parallel Port ECP Mode

DRQ1 Audio Parallel Port ECP Mode

DRQ2 Diskette Drive

DRQ3 Infrared Parallel Port ECP Mode

DRQ4 Cascade

DRQ5 Unused

DRQ6 Unused

DRQ7 Unused

ThinkPad 760ELD Interrupt Assignments

2 3 4 5 7 9 10 11 15

Cascade Interrupt Req From IRQ 8-15 Default

Serial Port Optional Optional

Infrared Optional Default Optional Optional Optional Optional

Parallel Port Optional Default

Audio Default Optional Optional

Secondary IDE Optional

PCI IRQ (For PCI Devices) Optional Optional Optional Optional Optional Optional Default Optional

ISA Adapters (In Docking Station) Optional Optional Optional Optional Optional Optional Optional Optional

DOCK I Internal SCSI Optional Optional Optional Default

DOCK II Internal SCSI Optional Optional Default

SelectaDock Internal SCSI Optional Optional Optional Optional Optional Optional Default Optional

Note 1

The following interrupts are used by the system: IRQ 0 (Timer), IRQ 1 (Keyboard), IRQ 6 (Floppy Diskette Drive), IRQ 8 (Real-time Clock), IRQ 12

(Mouse/Trackpoint), IRQ 13 (Math Coprocessor), and IRQ 14 (Hard Disk Drive).

Note 2

The PCI Adapter in SelectaDock, and SelectaDock Internal SCSI share IRQ 11.

ThinkPad 760ELD DMA Channel Assignments

DMA Default Assignment Other Possible Uses

DRQ0 Infrared Audio, Parallel Port ECP Mode

DRQ1 Audio Parallel Port ECP Mode

DRQ2 Diskette Drive

DRQ3 Infrared Parallel Port ECP Mode

DRQ4 Cascade

DRQ5 Unused

DRQ6 Unused

DRQ7 Unused

ThinkPad 760L Interrupt Assignments

2 3 4 5 7 9 10 11 15

Cascade Interrupt Req From IRQ 8-15 Default

Serial Port Optional Optional

Infrared Optional Default Optional Optional Optional Optional

Parallel Port Optional Default

Audio Default Optional Optional

DOCK I Internal SCSI Optional Optional Optional Default

DOCK II Internal SCSI Optional Optional Default

UltraBay Hard Disk Drive Optional

PCMCIA Cards Optional Optional Optional Optional Optional Optional Optional Optional

ISA Adapters (In Docking Station) Optional Optional Optional Optional Optional Optional Optional Optional

Note 1

The following interrupts are used by the system: IRQ 0 (Timer), IRQ 1 (Keyboard), IRQ 6 (Floppy Diskette Drive), IRQ 8 (Real-time Clock), IRQ 12

(Mouse/Trackpoint), IRQ 13 (Math Coprocessor), and IRQ 14 (Hard Disk Drive).

Note 2

If you enable the second hard disk drive in the UltraBay, it must use IRQ 15. This could cause a conflict with an existing device.

ThinkPad 760L DMA Channel Assignments

DMA Default Assignment Other Possible Uses

DRQ0 Infrared Audio, Parallel Port ECP Mode

DRQ1 Audio Parallel Port ECP Mode

DRQ2 Diskette Drive

DRQ3 Infrared Parallel Port ECP Mode

DRQ4 Cascade

DRQ5 Unused

DRQ6 Unused

DRQ7 Unused

ThinkPad 760LD Interrupt Assignments

2 3 4 5 7 9 10 11 15

Cascade Interrupt Req From IRQ 8-15 Default

Serial Port Optional Optional

Infrared Optional Default Optional Optional Optional Optional

Parallel Port Optional Default

Audio Default Optional Optional

DOCK I Internal SCSI Optional Optional Optional Default

DOCK II Internal SCSI Optional Optional Default

CD-ROM/UltraBay Hard Disk Drive Optional

PCMCIA Cards Optional Optional Optional Optional Optional Optional Optional Optional

ISA Adapters (In Docking Station) Optional Optional Optional Optional Optional Optional Optional Optional

Note 1

The following interrupts are used by the system: IRQ 0 (Timer), IRQ 1 (Keyboard), IRQ 6 (Floppy Diskette Drive), IRQ 8 (Real-time Clock), IRQ 12

(Mouse/Trackpoint), IRQ 13 (Math Coprocessor), and IRQ 14 (Hard Disk Drive).

Note 2

If you enable the second hard disk drive in the UltraBay, it must use IRQ 15. This could cause a conflict with an existing device.

ThinkPad 760LD DMA Channel Assignments

DMA Default Assignment Other Possible Uses

DRQ0 Infrared Audio, Parallel Port ECP Mode

DRQ1 Audio Parallel Port ECP Mode

DRQ2 Diskette Drive

DRQ3 Infrared Parallel Port ECP Mode

DRQ4 Cascade

DRQ5 Unused

DRQ6 Unused

DRQ7 Unused

THINKPAD DOS/WINDOWS MEMORY MANAGEMENT TIPS

IBM Card & Socket Services Drivers for ThinkPad 760

DEVICEHIGH=C:\THINKPAD\IBMDSS01.SYS /D (DOS PCMCIA Socket Services Driver for PCMCIA Socket Services 2.1)

The /D parameter allows warm docking when used with a Dock II docking station. If you are not using a Dock II then removing the /D parameter

will reduce the amount of upper memory this driver uses by approximately 1KB. Socket Services uses between 6KB and 7KB of memory .

DEVICEHIGH=C:\THINKPAD\IBMDOSCS.SYS (DOS PCMCIA Card Services Driver for PCMCIA Socket Services 2.1)

Card Services uses 26KB of memory.

DEVICEHIGH=C:\THINKPAD\DICRMU01.SYS /MA=C800-CFFF (DOS PCMCIA Resource Map Utility)

The /MA parameter tells Card Services what locations in upper memory can be used by PCMCIA cards or Card Services, and must match or be a

subset of an excluded memory range on the EMM386 line. The PCMCIA Resource Memory Map Utility Driver does not remain in memory.

DEVICEHIGH=C:\THINKPAD\$ICPMDOS.SYS (DOS PC Card Power Management Driver)

This driver uses 3KB of memory.

DEVICEHIGH=C:\THINKPAD\AUTODRV.SYS

This statement loads the PCMCIA Super Client Driver (AUTODRV.SYS) into upper memory. AUTODRV.SYS recognizes many popular modems,

3270 cards, and SCSI cards. It does not recognize 5250 PCMCIA cards, SDLC cards, or LAN PCMCIA cards. AUTODRV.SYS uses 7KB of

memory.

Please note that Card & Socket Services also requires a 4KB block of upper memory.

IBM MWAVE DSP DOS Drivers for ThinkPad 760C & 760CD only

DEVICEHIGH=C:\MWD\MANAGER\MWDP0400.EXE (MWAVE DSP Driver)

The MWAVE DSP DOS Driver uses 2KB of memory .

THINKPAD DOS/WINDOWS MEMORY MANAGEMENT TIPS

IBM MWAVE DSP Windows Drivers for ThinkPad 760C & 760CD only

(1) Version 1.00 Mwave drivers required a large amount of memory below 1MB in the Windows environment, often limiting the number or Windows

applications that could be loaded at one time. Please update to the latest MWAVE Drivers

Disabling SCSI BIOS in ThinkPad DOCK II

(1) If you are not using a SCSI device in the DOCK II or are only using the internal SCSI CD-ROM, you can disable SCSI BIOS and reclaim 16KB of

upper memory. SCSI BIOS can be disabled by rebooting the system while in the DOCK II, pressing Ctrl A at the prompt, selecting Configure/

View Host Adapter Settings, and changing Host Adapter BIOS to Disabled. SCSI BIOS can also be disabled by removing the DOCK II’s cover

and changing the switch settings on the DIP switch block: Switch 1, 2, and 3 to ON. Do not change switch 4.

Memory Management Without PCMCIA Cards

(1) If you do not intend to use PCMCIA Cards, there is no reason to load Card & Socket Services Drivers. Remove all IBM Card and Socket Services

Device Drivers from CONFIG.SYS (See previous page).

(2) Card & Socket Services Drivers are not required to use the MWAVE DSP Modem or DSP Audio functions.

(3) Review the ThinkPad Memory Map for your system. Include any upper memory areas not used by adapter cards in the Docking Station. Be sure

to exclude the address of the SCSI adapter in the Docking Station if SCSI support is needed.

(4) If you are not using the monochrome video mode (most applications do not), the Monochrome Video Area (B000 - B7FF) may be mapped (by

adding I=B000-B7FF to the EMM386.EXE line in CONFIG.SYS). If using Microsoft Windows, add a Device=C:\DOS\MONOUMB.386 statement

to the [386Ehn] section of SYSTEM.INI.

THINKPAD DOS/WINDOWS MEMORY MANAGEMENT TIPS

Memory Management With PCMCIA Cards

(1) Many PCMCIA card manufacturers provide Point Enablers with their products. Point Enablers are small programs that provide an interface

directly to the PCMCIA controller; therefore they must be written to support a particular type of controller.

Point Enablers are relatively simple to configure, do not require Card & Socket Services Drivers, consume no memory (they remove themselves

from memory after configuring the card), and provide the maximum DOS memory for your ThinkPad. However, with Point Enablers, you must

specify the slot number of the card (therefore , the card must always be in a specific slot). You must also manually assign any upper memory

blocks and IRQs used by that card. In addition, hot-plugging of the card is prohibited (in fact, it may damage the card). If Point Enablers are

provided with the PCMCIA card(s) you are using, decide whether to use the Point Enablers or Card & Socket Services.

(2) If you use Card & Socket Services, decide whether to use the Super Client Driver (AUTODRV.SYS) or the drivers that are provided with your

PCMCIA card(s). The Super Client Driver automatically recognizes many popular PCMCIA cards (including modems, 3270 cards, and SCSI

adapters -- it does not recognize 5250 PCMCIA cards, SDLC cards, or LAN PCMCIA cards.). However, the Super Client Driver can consume

more memory than do the drivers provided with the PCMCIA card.

(3) Determine the amount and location of upper memory required by your PCMCIA card(s), Docking Station, and ISA Adapter cards. If possible,

locate upper memory required by all PCMCIA cards and ISA Adapters in one contiguous block. If using Card & Socket Services, these drivers

require a 4KB upper memory block that can be located anywhere in upper memory.

(4) Review the ThinkPad Memory Map for your system. Exclude from EMM386.EXE’s usage the upper memory areas used by (a) the PCMCIA

card(s), (b) Card & Socket Services (4KB), (c) the upper memory area used by the SCSI Adapter in the ThinkPad Docking Station (if applicable),

and (d) the upper memory areas used by any ISA adapters in the ThinkPad Docking Station. Include any available upper memory areas not

excluded above.

(5) If using Card & Socket Services, modify the DEVICE=C:\THINKPAD\DICRMU01.SYS /MA=XXXX-XXXX line in CONFIG.SYS. Make the XXXX-

XXXX range match the upper memory area used by any PCMCIA cards (plus the 4KB used by Card & Socket Services).

(6) Exclude any memory area allocated to PCMCIA Cards from usage by Microsoft Windows by adding an EmmExclude=XXXX-XXXX line to the

[386Enh] section of the SYSTEM.INI File. Where XXXX-XXXX is the upper memory range allocated to the PCMCIA cards. If you are using Card

& Socket Services, the EmmExclude range must match the /MA= range of the DICRMU01.SYS Driver.

(7) If you are not using the monochrome video mode (most applications do not), the Monochrome Video Area (B000-B7FF) may be mapped (by

adding I=B000-B7FF to the EMM386.EXE line in CONFIG.SYS). If using Microsoft Windows, add a Device=C:\DOS\MONOUMB.386 statement

to the [386Ehn] section of SYSTEM.INI.

(8) If you are using an IBM PCMCIA Token-Ring Adapter, an IBM Token-Ring Adapter in a Docking Station, or an IBM EtherJet Adapter in a Docking

Station, download the IBM LAN Client Code from the IBM BBS. This code loads 802.2 Support, Netbios, the Netware Requester, and a TCP/IP

stack into extended memory (not upper memory). It can reduce the DOS memory consumption of these protocols to 5KB.

Sample Config: IBM PCMCIA Token-Ring Adapter Installed in 760 Systems

Recommended Memory Locations

IBM Token-Ring PCMCIA Adapter ROM CC00-CDFF

IBM Token-Ring PCMCIA Adapter RAM C800-CBFF Note: Use D000-D4FF for 760ED

IBM Card Services (If Used) CE00-CEFF

Card Services CONFIG.SYS (Please ensure that you are using the latest Card & Socket Services Drivers)

DEVICE=C:\DOS\EMM386.EXE NOEMS X=C000-CEFF I=CF00-EFFF

DEVICE=C:\THINKPAD\IBMDSS01.SYS

DEVICE=C:\THINKPAD\IBMDOSCS.SYS

DEVICE=C:\THINKPAD\DICRMU01.SYS /MA=C800-CEFF

Note: Latest IBM Token-Ring Credit Card Adapter Drivers are Version 3.06 (TRCC1.EXE & TRCC2.EXE on the IBM BBS).

Point Enabler CONFIG.SYS

DEVICE=C:\DOS\EMM386.EXE NOEMS X=C000-CDFF I=CE00-EFFF

DEVICE=C:\POINTTR.EXE SB RS=16 MMIO=CC00 IRQ=9 SRAM=C800,16 Where: SB is Slot B (Bottom Slot) and RS is Ring Speed

If you are using the IBM PCMCIA Token-Ring Adapter in the PCMCIA slot in the Port replicator, you must add the PCIC parameter to your point enabler

device statement: For example: DEVICE=C:\POINTTR.EXE PCIC=03E2 SB RS=16 MMIO=CC00 IRQ=9 SRAM=C800,16. The Port Replicator uses

3E2 as its I/O port base address.

Microsoft Windows SYSTEM.INI

[386Enh]

EmmExclude=C800-CDFF (or EmmExclude=C800-CEFF if using Card Services)

Setting the Token-Ring ROM & RAM Address

(1) Novell Netware ODI Drivers (NET.CFG File): Link Driver TOKEN (Or TOKENCS Or LANSUP)

MEM #1 CC000

MEM #2 C8000

(2) For IBM LAN Support Native Drivers: DEVICE=C:\LSP\DXMC0MOD.SYS N ,C800,0,0,0

(3) The IBM LAN Support NDIS Drivers (PROTOCOL.INI File): RAM = 0xC800

MMIO = 0xCC00

RAMSIZE = 16

Sample Config: IBM PCMCIA Ethernet Adapter Installed in 760 Systems

Recommended Memory Locations

IBM Ethernet PCMCIA Adapter RAM C800-CBFF Note: Use D000-D4FF for 760ED

IBM Card Services (If Used) CC00-CCFF

Card Services CONFIG.SYS (Please ensure that you are using the latest Card & Socket Services Drivers)

DEVICE=C:\DOS\EMM386.EXE NOEMS X=C000-CCFF I=CD00-EFFF

DEVICE=C:\THINKPAD\IBMDSS01.SYS

DEVICE=C:\THINKPAD\IBMDOSCS.SYS

DEVICE=C:\THINKPAD\DICRMU01.SYS /MA=C800-CCFF

Note: Latest IBM Ethernet Credit Card Adapter Drivers are Version 2.06 (ETCC.EXE on the IBM BBS).

Point Enabler CONFIG.SYS

DEVICE=C:\DOS\EMM386.EXE NOEMS X=C000-CBFF I=CC00-EFFF

DEVICE=C:\NET\POINTETH.SYS SB IRQ=9 SRAM=C800 IO=300 Where: SB is Slot B (Bottom Slot)

If you are using the IBM PCMCIA Ethernet Adapter in the PCMCIA slot in the Port replicator, you must add the PCIC parameter to your point enabler

device statement: For example: DEVICE=C:\POINTETH.SYS PCIC=03E2 SB IRQ=9 SRAM=C800 IO=300. The Port Replicator uses 3E2 as its I/O port

base address.

Microsoft Windows SYSTEM.INI

[386Enh]

EmmExclude=C800-CBFF (or EmmExclude=C800-CCFF if using Card Services)

Setting the Ethernet RAM Address

(1) Novell Netware ODI Drivers (NET.CFG File): Link Driver PCMDMCS

PORT 300

INT 9

MEM C8000

(2) The IBM LAN Support NDIS Drivers (PROTOCOL.INI File): RAMADDRESS = 0xC800

INTERRUPT = 9

IOBASE = 0x300

IBM PCMCIA MODEM CONFIGURATION

Using the IBM Super Client Driver (AUTODRV.SYS)

(1) The IBM Super Client Driver will automatically recognize IBM PCMCIA Modems. Sample CONFIG.SYS file:

DEVICE=C:\DOS\HIMEM.SYS

DEVICE=C:\DOS\EMM386.EXE NOEMS X=C800-CFFF

DEVICE=C:\THINKPAD\IBMDSS01.SYS

DEVICE=C:\THINKPAD\IBMDOSCS.SYS

DEVICE=C:\THINKPAD\DICRMU01.SYS /MA=C800-CFFF

DEVICE=C:\THINKPAD\$ICPMDOS.SYS

DEVICE=C:\THINKPAD\AUTODRV.SYS C:\THINKPAD\AUTODRV.INI

Using the IBM PCMCIA Modem Point Enabler (Note: Not All IBM PCMCIA Modems Support this Point Enabler)

(1) The IBM PCMCIA Modem Point Enabler (called PCCOMDOS.SYS) does not require Card & Socket Services. It does reside in memory and

requires 16KB. Using the Point Enabler can save up to 36KB (if you do not load Card & Socket Services or AUTODRV.SYS). However, with the

IBM Point Enabler hot-plugging of the card is prohibited (in fact, it will damage the card).

(2) Be sure to exclude a 4KB block for the modem in upper memory. If you are also using card services, do not include the 4KB block in the /

MA=XXXX-XXXX parameter of the DICRMU01.SYS driver.

(3) Sample CONFIG.SYS file:

DEVICE=C:\PCCOMDOS\PCCOMDOS.SYS COM2 /BEEP /WINBIOS /AMEM CE

Where: COM2 is the COM 1, 2, 3, or 4 COM 2 is recommended

/AMEM is the memory location CE00 is recommended

for the modem’s 4KB block

Using the IBM PCMCIA Modem Driver

(1) The IBM PCMCIA Modem Driver (called ESTDFM.EXE) does require Card & Socket Services. It does reside in memory and requires 25KB.

Therefore, I recommend that you use the AUTODRV.SYS driver since it takes less memory. ESTDFM.EXE is loaded via the AUTOEXEC.BAT:

ESTDFM.EXE S1C2 Where: S1 is the Slot Number

C2 is the Communications Port (C1, C2, C3, or C4)

MEGAHERTZ MODEM CONFIGURATION

Using the IBM Super Client Driver (AUTODRV.SYS)

(1) The IBM Super Client Driver will automatically recognize most Megahertz PCMCIA Modems. Sample CONFIG.SYS file:

DEVICE=C:\DOS\HIMEM.SYS

DEVICE=C:\DOS\EMM386.EXE NOEMS X=C800-CFFF

DEVICE=C:\THINKPAD\IBMDSS01.SYS

DEVICE=C:\THINKPAD\IBMDOSCS.SYS

DEVICE=C:\THINKPAD\DICRMU01.SYS /MA=C800-CFFF

DEVICE=C:\THINKPAD\$ICPMDOS.SYS

DEVICE=C:\THINKPAD\AUTODRV.SYS C:\THINKPAD\AUTODRV.INI

Using the MegaHertz PCMCIA Modem Point Enabler

(1) The MegaHertz PCMCIA Modem Point Enabler (called SETMHZ.EXE) does not require Card & Socket Services. In addition, it removes itself

from memory once it has configured the modem. This can save up to 49KB (if you eliminate Card & Socket Services). However, with the

MegaHertz Point Enabler, you must specify the slot number of the card (therefore, the card must always be in a specific slot). In addition, hot-

plugging of the card is prohibited (in fact, it will physically damage the card).

(2) Obtain the latest Megahertz Point Enabler. Versions before 3.1 do not support the ThinkPad 760. Latest version is 4.3. Be sure to exclude a

4KB block for the modem in upper memory. If you are also using card services, do not include the 4KB block in the /MA=XXXX-XXXX parameter

of the DICRMU01.SYS driver.

(3) The SETMHZ program is loaded via the AUTOEXEC.BAT file. Format of the SETMHZ.EXE Program:

SETMHZ.EXE /cn /in /sn /pnnnn /dnnnn

Where: /cn is COM 1, 2, 3, 4 COM 2 is recommended

/in is IRQ 1 .. 15 IRQ 3 is recommended

/sn is Slot A, B, C, or D

/pnnnn is the memory location CE00 is recommended

/dnnnn is the delay in milliseconds 1500 is recommended

Obtaining Updated Drivers

IBM PC Company Bulletin Board System

BBS Phone Number 919-517-0001

Baud Rate 300-14400 bps

Parity/Data Bits/Stop Bits N/8/1

IBM PC Company Internet FTP Site

ftp.pcco.ibm.com cd /pub and get the allfiles.txt file for a listing of available files

IBM PC Company World Wide Web Site

www.pc.ibm.com

Obtaining Updated Version of this Document

Download any of the following files:

365_tips.ps ThinkPad 365 Tips in PostScript format.

365_tips.txt ThinkPad 365 Tips in ASCII format.

701_tips.ps ThinkPad 701 Tips in PostScript format.

701_tips.txt ThinkPad 701 Tips in ASCII format.

750_tips.ps ThinkPad 360, 750, 755 Base Models Tips in PostScript format.

750_tips.txt ThinkPad 360, 750, 755 Base Models Tips in ASCII format.

755_tips.ps ThinkPad 755 Enhanced Models Tips in PostScript format.

755_tips.txt ThinkPad 755 Enhanced Models Tips in ASCII format.

760_tips.ps ThinkPad 760 Tips in PostScript format.

760_tips.txt ThinkPad 760 Tips in ASCII format.

cdtips.ps Commercial Desktop Tips in PostScript format.

cdtips.txt Commercial Desktop Tips in ASCII format.