# RAID levels that can use a hot-spare or standby hot-spare drive

Hot-spare and standby hot-spare drives supply additional protection to a RAID configuration. When you select the RAID level for your configuration, consider the following:

RAID level | Can use a hot spare? | Can use a standby hot spare?
0 | No | No
1 | Yes | Yes
1E | Yes | Yes
5 | Yes | Yes
5E* | Yes | Yes
00 | No | No
10 | Yes | Yes
1E0 | Yes | Yes
50 | Yes | Yes

* RAID level-5E integrates a distributed hot-spare drive, but also can use traditional hot-spare and standby hot-spare drives. If a physical drive fails in a RAID level-5E logical drive and the configuration includes a hot-spare or standby hot-spare drive, the data is rebuilt on the hot-spare or standby hot-spare drive. A RAID level-5E compression does not occur. If a second physical drive fails in the RAID level-5E logical drive, a data compression will take place on the distributed hot-spare drive.

## More information

- Understanding RAID level-5E

Glossary | Contents

x-1068-SRM-00-03-EN