# The ServeRAID Manager started in local-only mode.

## Explanation:

- If you specified -l (that is, minus and a lowercase letter L) as a command-line parameter, the ServeRAID Manager starts in local-only mode.
  The ServeRAID Manager is not network-enabled. In this mode, you can configure and monitor the local system only. You cannot configure or monitor remote systems. If you added remote systems to your tree view, they are not visible in this mode. They will be visible in the tree when you start the ServeRAID Manager in non-local-only mode.
- If the network is unreachable, the ServeRAID Manager starts in local-only mode. An additional event is displayed in the event viewer indicating that the network is unreachable.
- If the port number is in use on the local system, the ServeRAID Manager starts in local-only mode. An additional event is displayed in the event viewer indicating that the network is unreachable.

## Action:

- If the network is unreachable, check the event viewer for details on any networking errors.
- If the port number is in use, exit from the application using the port number, or specify a different port number. Complete the following steps to specify a different port number:
  1. Open the RaidAgnt.pps file for the ServeRAID Manager running on the local machine.
  2. Type a new value for the port number in the following line in RaidAgnt.pps:
     agent.startupPortNum= 34571
     The default port number for local access is 34571.
     Note: When changing the port number, consider the following:
     - This change does not take effect until you restart the ServeRAID Manager.
     - Any system that is accessing this system remotely must have the port number changed to match the value you type. On the remote system, you can change this value in the "Add remote system" window.
     - Any system that contains this system in its Notification list must change the port number to the new port number. On the remote system, you can change the port number in the Notification Manager by clicking Modify system.

Glossary | Contents

x-0048-SRM-00-05-EN