This README file contains the latest information about installing 
IBM TotalStorage™ FAStT Storage Manager version 8.4 for Windows Server
2003.  

Refer to the IBM TotalStorage™ Support Web Site or CD for the
installation and support guide.

For other related publications (refer to Related Publications in the 
installation and support guide) and the latest information and 
updated readme file.

Last Update:  09/11/2003

Products Supported: 

      ---------------------------------------------------
     |		 | Machine Type	|     Model		 | 
     |-----------|--------------|------------------------|
     | FAStT 900 |     1742	| 90X ,	90U		 |
     |-----------|--------------|------------------------|
     | FAStT 700 |     1742	| 1RX ,	1RU		 |
     |-----------|--------------|------------------------|
     | FAStT 600 |     1742	| 60X ,	60U		 |
      ---------------------------------------------------

=======================================================================

CONTENTS
--------
1.0   Overview
2.0   Change History
3.0   Installation and Setup Instructions
4.0   Configuration Information
5.0   Unattended Mode
6.0   Web Sites and Support Phone Number
7.0   Trademarks and Notices
8.0   Disclaimer

=======================================================================

1.0   Overview
--------------

1.1  Overview
--------------

   This IBM Storage Manager release includes the IBM FAStT Storage 
   Manager version 8.4 for all versions of Windows Server 2003. The 
   \WS03_32bit or the \WS03_64bit and the Docs CD-ROM directories 
   contain the documentation and files necessary for installing 
   the IBM FAStT Storage Manager Software for Windows Server 2003
   in 32-bit or 64-bit servers.

   The IBM FAStT Storage Manager version 8.4 Installation and Support
   Guide for Intel-based Operating System Environments is also available
   on IBM's Support Web Site as a downloadable Portable Document
   Format (PDF) file. 
   
   This is a purchase upgrade for IBM machine types 1722 and 1742 only. 
   Please contact your IBM service representative or IBM resellers for
   purchasing info. This storage manager client software version 8.4
   upgrade will not be available for IBM machine types 3542 and 3552 
   with controller firmware 05.3x.xx.xx or lower. It will be able to
   manage these IBM machine types 3542 and 3552; but, any new features
   and updates that are introduced in this FAStT Storage Manager 
   version 8.4 will not be available for them.

=======================================================================

1.2  Limitations
----------------

1. If you are upgrading controller firmware in IBM FAStT500 storage
   controller with 512MB Cache, you will have to stop I/O and reboot 
   both controllers before upgrading firmware followed by NVSRAM. You 
   can reboot the controllers either by power cycling the storage 
   subsystem or by pressing the Reset button on both controllers. The
   Reset button is located on the right of the indicator lights in
   the opening on the front of each controller unit. 

   To determine Storage Controller cache level, perform the following:

   a. On a storage management station start the client software and 
      select a storage subsystem.
   b. Select Tools -> Manage Device to open the Subsystem Management 
      Window.
   c. Highlight the Storage Subsystem that you are upgrading and then 
      select Storage Subsystem -> Profile. It may take a little time 
      for it to create the Storage Subsystem profile.   
   d. Under the Controllers heading is an entry that displays 
      information similar to the following example:

      Cache/processor size (MB):  256/32

   If this setting is listed as 512/32 you will need to arrange to 
   perform this upgrade procedure at a time that you can stop I/O 
   to the Storage Subsystem in order to ensure a successful firmware
   download and installation.

2. Storage Manager prompts you for a password if all hard disk 
   drives are removed from the storage subsystem.

   After removing all drives from a storage subsystem (or not powering
   on drives and only the controller), the IBM FAStT Storage Manager 
   software will prompt you for a password when trying to start the 
   software or trying to perform protected operations. Any password 
   entered will fail.

   Password information is stored on a reserved area of each hard disk 
   drive on the storage subsystem.  Each drive stores a mirrored copy
   of the password data.  When there are no drives in the storage
   subsystem, the storage management software does not find the 
   password data when you attempt password protected operations. Add
   one drive to the storage subsystem and retry the operation.

   Since the RAID controller unit should not be powered on until the 
   expansion units are attached and powered on, this should be done by 
   powering off the RAID controller unit, properly attaching all 
   expansion units (with drives installed), to the RAID controller unit 
   and powering them on, and then powering the RAID controller unit back 
   on.  At this point the storage subsystems can be rediscovered and 
   managed using the IBM FAStT Storage Manager software.

3. The Disable/Enable and Uninstall menu functions will be displayed
   when you right-click the RDAC Multi-Path Pseudo-Bus entry in SCSI
   and RAID controllers list of the Device Manager folder. The folder
   is in the Computer Management window. You should not use these 
   menu functions but rather using the Add/Remove program function
   in the Control Panel window to uninstall or to disable the IBM 
   FAStT Storage Manager RDAC device. To reenable the IBM FAStT 
   Storage Manager RDAC device, follow the instructions in the IBM 
   FAStT Storage Manger vrsion 8.4 Installation and support guide 
   for Intel-based Operating System Environments.  

4. You must always uninstall IBM FAStT Storage Manager RDAC before 
   you uninstall the Host Bus Adapter driver. Failure to do so may 
   result in system hung or blue-screen. 

5. When the FAStT storage subsystem controller firmware is upgraded 
   from any version 05.00.xx.xx or earlier to version 05.2x.xx.xx or 
   later, all of the Windows 2000 servers that had LUNs mapped in this
   storage subsystem must be rebooted after the new FAStT storage 
   subsystem controller firmware and NVSRAM are successfully applied. 
   The reason is that when the new FAStT storage subsystem controller 
   firmware is installed, the controller returns the first four bytes
   of the firmware revision in the Product Revision field of the SCSI
   LUN inquiry data. Windows 2000 uses the Product Revision data as 
   part of the LUN identification. So, as the Product Revision data 
   changes due to the new firmware revision level, Windows 2000 
   thinks that the LUNs with the old Product Revision data were 
   removed from the server. When the 'scan for hardware changes' task
   is executed by running the FAStT storage manager hot_add utility
   or by selecting the Scan For Hardware Changes menu option of the 
   Devices folder in the Computer Management window, Windows 2000
   displays Unsafe Removal of Devices dialogs for these LUNs. The
   devices in these dialogs are RDAC Virtual Disks and xxxx SCSI 
   devices where xxxx are either 1742, 3552 or 3542 depending on the
   model type of  FAStT storage server(s) that the Windows 2000 
   server had LUNs mapped from. The Windows 2000 server will lose 
   connectivity to the LUNs in the FAStT storage that has firmware
   updated. The server must be rescaned for hardware changes. If
   the logical drives are not added back to the server, one must 
   reboot the server to reconnect to the logical drives. 

   This problem will not occurred when upgrading the FAStT storage 
   subsystem controller firmware from version 05.20.xx.xx to version
   05.3x.xx.xx or later because the product revision data field was 
   fixed at 0520.

6. When the server HBA ports are directly connected to the FAStT 
   storage server controllers, do not download firmware and NVSRAM 
   files to the controllers with IOs being generated to the LUNs in 
   the FAStT storage server. There is no IOs restriction in SAN
   Fabric environment ie. the HBA port are connected to the FAStT
   storage server controller ports via Fibre Channel switches.
   
7. The supplied SMrepassist utility did not utilize Microsoft Volume
   Shadow Services APIs to quiesce the LUNs. Appropriate steps are 
   still need to shut down/quiesce the applications like MS Exchange
   and SQL Server before the FlashCopy logical drive can be made.

8. Rebooting host server may cause its mapped LUNs move to non-preferred
   path. Use Storage Manager client program to redistribute the LUNs to
   their preferred path.

9. Uninstalling RDAC may cause Windows Dynamic disks to fail. After the
   new RDAC is installed and the server is rebooted, these disks must be 
   reactivated and Chkdsk must be run. The work-around is to stop the
   applications and remove the drive letters or the mount points to 
   these disks before uninstalling and reinstalling RDAC.
   
10. The current RDAC driver will coexist with Storport model driver as
    long as it is not the driver for the adapter that talks to the LUNs
    in the FAStT storage subsystems. Note: the current release drivers
    for all of the Fibre Channel host bus adapters that FAStT storage
    subsystem supported are based on the Scsiport model.
       
12. In Xseries x330 server, when two of the Dymanic disks are mirrored
    together by the Windows OS, it may cause the server to hang after
    the LUN that these disks are defined on fail-over/fail-back. There
    is no work-around.
    
13. Multiple Windows cluster configurations to a single FAStT Controller 
    Subsystem with firmware 05.40.xx.xx are not supported at this time. 
    Single two node cluster is supported with firmware 05.40.03.03 or later. 
    FAStT Controller Subsystems need to be factory preloaded or upgraded 
    with a previous version of firmware 05.40.03.xx before firmware 
    05.40.03.04 will download to the FAStT Controller. FAStT Subsystem 
    Controller firmware 05.40.03.04 is available for download from IBM's 
    Web Sites.       


=======================================================================
                
1.3  Enhancements
-----------------
     N/A

=======================================================================
            
1.4  Prerequisites
------------------

   If the host type of either the Default Group or the defined host 
   ports in a storage mapping partition is set to "Windows NT ...", 
   it could take up to 2 hours to boot a Windows Server 2003 host
   after installing Windows Server 2003 RDAC driver. One must make  
   management connection to the storage subsystem via Ethernet ports 
   (out-of-band management) and set the host type to the "Windows 
   2000/ ..." setting.


=======================================================================
            
1.5  Dependencies
-----------------

   IBM FAStT Storage Manager version 8.4 provides full management support
   IBM machine types 3552 and 3542 storage subsystems that have at least
   firmware version 04.00.02.xx, IBM machine type 1742 (models 1RX, 1RU)
   storage subsystem that have at least firmware version 05.00.04.xx or
   IBM machine type 1742 (models 90X, 90U) and 1722 storage subsystems
   that have at least firmware version 05.3x.xx.xx.
    
   The only IBM FAStT Storage Manager 8.4 supported management function 
   on controllers with firmware version 04.xx.xx.xx to 04.xx.01.xx is 
   controller firmware and NVSRAM download. 

=======================================================================

2.0   Change History
-----------------------------

This is the latest release of IBM FAStT Storage Manager for Windows 
Server 2003 only. The FAStT client software package in the \WS03_32bit
and the \WS03_64bit directories will not function correctly in Windows 
Windows 2000 and NT 4.0 servers. Please refer to the FAStT client software 
package in the \Win32 directory for Windows 2000 and NT 4.0 servers.

=======================================================================

2.1 Key Features added to IBM FAStT Storage Manager 8.4 with controller 
    firmware level 05.4x.xx.xx.
    
---------------------------------------------------------------------
    
   See the IBM FAStT Storage Manager version 8.4 Installation and Support
   Guide for Intel-based Operating System Environments.
    
=======================================================================
        
2.2 Client Code levels at time of release are as follows
---------------------------------------------------------

     1. IBM FAStT Storage Manager RDAC version:  08.40.35.01
                        
     2. IBM FAStT Storage Manager Utilities version: 08.40.35.00
     
   Refer to the http://ssddom02.storage.ibm.com/techsup/webnav.nsf/support/disk
   IBM TotalStorage™ Disk Storage Systems Technical Support web site for the 
   latest released code levels.
          
   IBM FAStT Storage Manager Client and IBM FAStT Storage Manager Agent
   software packages are not available at this time for the 64 bit Windows
   Server 2003 hosts. Please either check IBM Support web site for the 
   availability of these software packages or set up a 32-bit computer as 
   the FAStT storage subsystem management station. Please refer to the
   IBM FAStT Storage Manager version 8.4 Installation and Support Guide
   for Intel-based Operating System Environments for instructions 
   on setting up out-of-band management.

=======================================================================
              
3.0   Installation and Setup Instructions
-----------------------------------------

3.1  Step-by-step instructions for this code update are as follows
------------------------------------------------------------------
                     
1. Install and update the driver for the IBM FAStT Host Bus Adapter.
                
   a. Install the hardware by using the instructions that come with the 
      adapter. 
   b. Install the IBM FAStT Host Adapter driver by using the 
      instructions provided in the readme.txt file located in the 
      Host_Adapter directory on this installation CD.

2. Install the new Storage Manager version 8.4 software. If there are
   previous version of the IBM FAStT Storage Manager version installed 
   in the system, uninstall it before installing the new version of the 
   storage manager software. Refer to the IBM FAStT Storage Manager version
   8.4 Installation and Support Guide for Intel-based Operating System 
   Environments for detailed installed and uninstalled instructions.
   
=======================================================================
   
3.2 Refer to the Host_Adapter directory on the installation CD for 
    the applicable drivers.  
     
   Refer to the http://ssddom02.storage.ibm.com/techsup/webnav.nsf/support/disk
   IBM TotalStorage™ Disk Storage Systems Technical Support web site for the 
   latest supported host adapters, device drivers, and updated readme. 
      
=======================================================================
                                
3.3  Helpful Hints
------------------

1. If you are unable to see the maximum number of drives during 
   Automatic Configuration, you should be able to use Manual 
   Configuration to select individual drives and select the maximum 
   number of drives allowed.

2. Depending on the storage subsystem that you have purchased, you
   may have to purchase the FAST storage partitioning premium feature
   option or an option to upgrade the number of supported partitions
   in a storage subsystem. Please see IBM Marketing representatives
   or IBM resellers for more information.
   
   - IBM FAStT600 storage subsystem (machine type 1722): The standard
     configuration does not have the FAST storage partitioning feature
     enabled. Four partition, eight partition, an upgrade from four
     to eight partition and an upgrade from eight to sixteen partition
     storage partitioning premium feature options can be purchased.
     
     A Turbo option is available for the FAStT600 which includes an
     eight partition storage partitioning premium feature option. The
     FAStT600 with Turbo option can have up to 64 storage partitions
     via 8 to 16 partition and 16 to 64 partition storage partition 
     premium feature upgrade options.  

   - IBM FAStT700 storage subsystems (machine type 1742 - models 1RU
     and 1RX): The standard configuration has 64 partitions storage 
     partitioning premium option installed. No additional storage 
     partitioning premium feature options can be purchased for these 
     storage subsystems.

   - IBM FAStT900 storage subsystem (machine type 1742 - models 90X and
     90U): The standard configuration has 16 partition storage partitioning
     premium option installed. An upgrade from 16 to 64 partition storage
     partitioning premium feature option can be purchased.

3. Do not delete the Access LUN or Access Volume. The Access LUN is required
   by the SMclient to communicate with the storage controllers when using the 
   in-band management method.
   
4. The RDAC driver must be digitally signed by Microsoft in order for it to
   work correctly. Always use the IBM provided signed RDAC driver package.

=======================================================================

4.0 Configuration Information
-----------------------------

        
4.1 Configuration Settings
--------------------------


1. By default, the IBM FAStT Storage Manager 8.4 firmware does not 
   automatically map logical drives when the IBM FAStT storage 
   partitioning premium feature is enabled. This means that the logical 
   drives after being created are not automatically presented to the host
   systems.
   
   For a new installation, after creating new arrays and logical drives; 
   a. If the host OS type is not Windows NT, create a partition with the
      appropriate OS host type and map the logical drives to this partition. 
   b. If your host OS type is Windows NT non-clustered (SP5 or higher),
      you can map your logical drives to the "Default Host Group" or 
      create a partition with Windows non-clustered (SP5 or higher) host
      type.
      
   Note: The host type setting for the Windows Server hosts is the same as
   Windows 2000. Select either Windows 2000 Clustered or Window 2000 
   Non-Clustered host type if the correct host types of Windows 2000/Server
   2003 Clustered or Windows 2000/Server 2003 Non-Clustered are not 
   displayed in the host type pull down list.
                                 
   When upgrading from previous versions of IBM FAStT Storage Manager
   to version 8.4x. 
   a. If you are upgrading with no defined storage partitions in 
      operating system other than Windows NT, you will need to create
      a storage partition with the appropriate operating system host
      type and map the logical drives from the "Default Host Group" 
      to this partition.
   b. If you are upgrading with defined storage partitions and an 
      operating system other than Windows NT is accessing the default
      host group, you will need to change the default host type to
      this operating system host type after upgrading. The FAStT 
      Storage Manager upgrading will reset the default host type to
      Windows NT host type. 
              
   Refer to the IBM FAStT Storage Manager online help to learn
   more about creating storage partitions and changing host types.

2. When you are configuring IBM machine type 1722, 1742, 3542 or 3552
   storage controllers as boot devices, contact IBM support for 
   supported configurations and instructions for configuring LUNs in
   IBM FAStT storage subsystems as boot devices. 

3. Running script files for specific configurations. Apply the 
   appropriate scripts  to your subsystem based on the instructions
   you have read in the publications or any instructions in the 
   operating system readme file. A description of each script is 
   shown below.

   - SameWWN.scr: Setup RAID controllers to have the same World Wide 
     Names. The World Wide Names (node) will be the same for each 
     controller pair. The NVSRAM default sets the RAID controllers
     to have the same World Wide Names.

   - DifferentWWN.scr:  Setup RAID controllers to have different World 
     Wide Names. The World Wide Names (node) will be different for each 
     controller pair. The NVSRAM default sets the RAID controllers 
     to have the same World Wide Names.

   - EnableDriveMigration.scr:  The Enable drive migration script
     scans the drives for configurations when they are added to a 
     storage system and will also attempt to use configurations found
     on the newly added drives. The NVSRAM default will enable drive
     migration.

   - DisableDriveMigration.scr:  The disable drive migration script 
     allows the addition of disk drives while the system is running.
     In addition, it identifies the drives as unused capacity 
     regardless of past drive configuration. The NVSRAM default will
     enable drive migration.
     
4. When you are configuring IBM machine type 1742 storage controllers
   in host cluster Remote Mirror configurations, contact IBM support
   for supported host cluster configurations and instructions for 
   configuring IBM storage controllers in clustered Remote Mirror 
   configurations. 

=======================================================================

4.2 Hardware status and information
-----------------------------------

   New installations for IBM Machine types 1722 and 1742 should be
   installed with the IBM FAStT FC2-133 Host Bus Adapter and Microsoft 
   Windows device driver version 8.2.3.61. For more information, refer
   to the IBM Support Web site.
 
=======================================================================

4.3 Unsupported configurations
------------------------------

   The following lists configurations that are currently not being 
   supported with IBM FAStT Storage Manager 8.4x.

   1. Fibre Channel loop environments with the IBM Fibre Channel hub, 
      machine type 3523 and 3534, in conjunction with the IBM Fibre 
      Channel switch, machine types 2109-S16, 2109-F16, 2109-S8 or 
      3534-F08. In this configuration, the hub is connected between 
      the fibre channel switch and the IBM FAStT storage subsystem
      controller ports.

   2. The IBM Fibre Channel hub, machine type 3523, connected to IBM 
      machine type 1722 and 1742.
      
=======================================================================

5.0   Unattended Mode
---------------------
        N/A

=======================================================================

6.0   WEB Sites and Support Phone Number
----------------------------------------

   6.1  IBM TotalStorage™ Disk Storage Systems Technical Support web site:
        http://ssddom02.storage.ibm.com/techsup/webnav.nsf/support/disk

   6.2  IBM TotalStorage™ Marketing Web Site:
        http://www.storage.ibm.com/hardsoft/disk/fastt/index.html

   6.3  If you have any questions about this update, or problem
        applying the update go to the following Help Center World
        Telephone Numbers URL:
        http://www.ibm.com/planetwide

=======================================================================

7.0   Trademarks and Notices
----------------------------

7.1 The following terms are trademarks of the IBM Corporation in the
    United States or other countries or both:

     IBM
     
     FAStT

     TotalStorage™ 
     
     the e-business logo

     xSeries

     HelpCenter
     
     Linux is a registered trademark of Linus Torvalds.

     Microsoft, Windows 2000, Windows Server 2003 and Windows NT 
     are trademarks of Microsoft Corporation in the United States, 
     other countries, or both.

     Java and all Java-based trademarks and logos are trademarks or
     registered trademarks of Sun Microsystems, Inc. in the United
     states, other countries, or both.

     UNIX is a registered trademark of The Open Group in the United
     States and other countries.

     Other company, product, and service names may be
     trademarks or service marks of others.

=======================================================================

8.0   Disclaimer
----------------

        8.1  THIS DOCUMENT IS PROVIDED "AS IS" WITHOUT WARRANTY OF
             ANY KIND. IBM DISCLAIMS ALL WARRANTIES, WHETHER EXPRESS
             OR IMPLIED, INCLUDING WITHOUT LIMITATION, THE IMPLIED
             WARRANTIES OF FITNESS FOR A PARTICULAR PURPOSE AND
             MERCHANTABILITY WITH RESPECT TO THE INFORMATION IN THIS
             DOCUMENT. BY FURNISHING THIS DOCUMENT, IBM GRANTS NO
             LICENSES TO ANY PATENTS OR COPYRIGHTS.


        8.2  Note to U.S. Government Users -- Documentation related to
             restricted rights -- Use, duplication or disclosure is
             subject to restrictions set forth in GSA ADP Schedule
             Contract with IBM Corporation.
