### Could not flash the drive light(s).

Explanation: The drive lights could not flash because of one of the following:

- The drives are not managed by an enclosure.
- A hardware error occurred.

Action:

1. Verify that the device is managed by an enclosure (that is, SAF-TE) device on the SCSI drive channel.
2. Verify that the controller, cables, and hard disk drives are installed properly.
3. Verify that there is power to the drives.
4. Retry the command.
5. If the command still fails, restart the server and retry the command.