This README file contains the latest information about the IBM 
TotalStorage™ FAStT Storage Server controller firmware version 05.41.xx.xx.

Refer to the IBM TotalStorage™ Support Web Site or CD for the IBM 
TotalStorage™ FAStT Storage Manager version 8.4x Installation and Support 
Guide for Intel-based Operating System Environments or the IBM TotalStorage
FAStT Storage Manager version 8.4x Installation and Support Guide for AIX,
HP-UX and Solaris. This guide along with the FAStT Storage Manager program
Online Help provide the installation and support information.

For other related publications (refer to Related Publications in the 
installation and support guide) and the latest information and 
updated readme file.

Last Update:  04/09/2004

Products Supported: 

      ---------------------------------------------------
     |           | Machine Type |     Model              | 
     |-----------|--------------|------------------------|
     | FAStT 900 |     1742     | 90X , 90U              |
     |-----------|--------------|------------------------|
     | FAStT 600 |     1722     | 60U , 60X              |
     |-----------|--------------|------------------------|
     | EXP   100 |     1710     | 10U , 10X              |
      ---------------------------------------------------

Note: 
  The IBM TotalStorage™ FAStT Storage Manager version 8.41 software 
  package is required for managing FAStT storage servers that are connecting
  to the FAStT EXP100 drive expansion enclosures. The controller firmware
  and NVSRAM files that are part of this release are required to be loaded
  in the FAStT storage server enabling it to recognize the FAStT EXP100 
  drive expansion enclosures. 
   
  Furthermore, the FAStT storage server controller firmware and NVSRAM files 
  that are part of the IBM TotalStorage™ FAStT Storage Manager version 
  8.41 release should not be loaded into the FAStT storage server connecting
  to FAStT EXP700 and EXP500 drive expansion enclosures. Please use the 
  FAStT storage server controller firmware and NVSRAM files that were part 
  of the IBM TotalStorage™ FAStT Storage Manager version 8.4 or the IBM 
  TotalStorage™ FAStT Storage Manager version 8.3x software releases instead.
  
  IMPORTANT: 

  Register at the IBM Support and Download WEB Site to obtain notification 
  of important product updates at www.ibm.com/servers/storage/support/fastt.
  Refer to the "Personalized Support" section of the web page and click on 
  "My Support". When the Please Sign In web page displayed, if you have not 
  previously registered to use this site, please do so now by clicking on 
  highlighted register word in window section titled "We use IBM 
  Registration" on the top left corner of the web page. Follow the 
  instructions in the displayed web page to register yourself to ibm.com. 

  Once you have registered, log into the site by entering your user id and
  password. In the Welcome Page, select Computer Storage in the "Select a  
  Product Family" pull down in the hardware section and click on "go".
  In the Computer Storage page, scroll down to "Disk Storage Systems" 
  category and select "1710" by clicking on the check box. Scroll to the 
  bottom of the web page and select "Save and Return" . You will be 
  returned to the main page.

  From the main page select your mail preferences. It is recommended to 
  select "Flashes" and "Downloadable files" to  be provided with important
  information on product updates. Select Submit. You should see a 
  confirmation indicating that "Your profile was successfully updated".



=======================================================================
CONTENTS
--------
1.0  Overview
2.0  Change History
3.0  Installation and Setup Instructions
4.0  Configuration Information
5.0  Unattended Mode
6.0  Web Sites and Support Phone Number
7.0  Trademarks and Notices
8.0  Disclaimer


=======================================================================
1.0   Overview
--------------

   This IBM Storage Manager release includes the IBM FAStT Storage 
   Server controller firmware and NVSRAM files version 05.41.xx.xx for 
   upgrading the following IBM machine types - 1722 (models 60X and 60U),
   1742 (models 90X and 90U). It does not contains the controller and
   NVSRAM files for the following machine types and models - 3542 (all 
   models), 3552 (all models) and 1742 (models 1RX and 1RU).
   
   The IBM TotalStorage™ FAStT Storage Manager version 8.4x Installation 
   and Support Guide for Intel-based Operating System Environments or the
   IBM TotalStorage™ FAStT Storage Manager version 8.4x Installation and 
   Support Guide for AIX, HP-UX and Solaris is available on IBM's Support 
   Web Site as a downloadable Portable Document Format (PDF) file. This 
   guide along with the FAStT Storage Manager program Online Help provide
   the installation and support information.

   In addition, IBM FAStT Copy Services premium features - FlashCopy,
   VolumeCopy and Remote Mirror - are not supported in this release of
   IBM FAStT Storage Manager version 8.41. Please contact your IBM 
   representatives or resellers for availability date of support.
    
   The FAStT storage partitioning premium feature is standard on all 
   IBM FAStT storage subsystems with the exception of the IBM FAStT600
   (machine type 1722 with Standard option) storage subsystem. Please 
   contact IBM Marketing representatives or IBM resellers if you want
   to purchase the IBM FAStT storage partitioning premium feature option
   for it. The Turbo option of the IBM FAStT600 is shipped with the IBM
   FAStT storage partitioning premium feature enabled (8 partitions).

   The IBM FAStT Storage Manager version 8.41 is shipped with IBM FAStT 
   EXP100 external drive expansion enclosures. The host software component 
   of IBM FAStT Storage Manager 8.41 will manage all FAStT storage server 
   with the controller firmware 04.00.02.xx or newer. But, any new features
   and updates that are introduced in this FAStT Storage Manager version 
   8.41 will not be available for any FAStT storage server controllers 
   without the controller firmware version 05.41.xx.xx installed.

   Refer to the IBM Support Web Site for the latest Firmware and 
   NVSRAM files for the IBM FAStT Storage Subsystems.
   http://www.ibm.com/storage/support/fastt

=======================================================================
1.1  Limitations
---------------------

1. Storage Manager prompts you for a password if all hard disk 
   drives are removed from the storage subsystem.

   After removing all drives from a storage subsystem (or not powering 
   on drives and only the  controller), the IBM FAStT Storage Manager 
   software will prompt you for a password when trying to start the 
   software or trying to perform protected operations. Any password 
   entered will fail.

   Password information is stored on a reserved area of each hard disk 
   drive on the storage subsystem.  Each drive stores a mirrored copy of 
   the password data.  When there are no drives in the storage 
   subsystem, the storage management software does not find the password 
   data when you attempt password protected operations. Add one drive to 
   the storage subsystem and retry the operation.
   
   Since the RAID controller unit should not be powered on until the 
   expansion units are attached and powered on, this should be done by 
   powering off the RAID controller unit, properly attaching all 
   expansion units (with drives installed), to the RAID controller unit 
   and powering them on, and then powering the RAID controller unit back 
   on.  At this point the storage subsystems can be re-discovered and 
   managed using the IBM FAStT Storage Manager 8.2 software.

2. Auto LUN/Array Transfer is not enable for Microsoft Windows, IBM AIX 
   and SUN Solaris OS's. If a controller fails over arrays to the alternate
   controller and the failed controller is replaced and brought back online,
   the arrays do not automatically transfer to the preferred controller. 
   This must be done manually by selecting the redistributing arrays menu
   option in the storage subsystem window of the IBM FAStT storage manager 
   client program.

3. The FAStT Storage Management dialog windows may be displayed 
   cropped without the vertical and horizontal scroll bars. Just move 
   the mouse pointer over the edge of the window until the mouse pointer 
   change to window resize pointer, left click and hold to grip the 
   window edge to resize it. 

4. If you get "Error 21 - The Operation cannot complete because a 
   ...  is in progress" error when you issue a Subsystem Management 
   command from the IBM FAStT Storage Manager Client, the command may be 
   cached. If the command is cached, the IBM FAStT Storage Manager 
   Client will run the command as soon as the controller resources are 
   available. Wait for at least ten minutes and check to see whether the 
   command has been run. If not, re-attempt the command. 

5. The IBM FAStT Storage Server hardware and software is designed to 
   have redundant paths from the host system to ensure the availability 
   of storage. However, it is possible to connect a single host adapter 
   from the host system to one of the controller minihubs and then 
   connect this minihub to the minihub of the other controller. This 
   configuration will create a FC-AL loop between the host adapter and 
   the two IBM FAStT Storage Server controllers and no redundant path to 
   the host system. When you connect the two minihubs together, always 
   connect the "IN" port of one minihub to the "OUT" port of the other 
   minihub or vice versa. Do not connect the "IN" port of one to the 
   "IN" port of the other minihub or the "OUT" port of one minihub to 
   the "OUT" port of the other minihub.
                        
6. The FAStT Storage Manager version 8.41 does not support Veritas DMP
   in Windows operating system environment. Please contact IBM 
   representatives or resellers for the availability of support.

7. The FAStT storage server when configured with the FAStT EXP100 
   SATA Drive Expansion Unit is currently reporting a higher frequency 
   of informational events such as Destination Driver Events (DDEs) 
   and Fibre Channel link up/down events ... in the FAStT Controller event
   log compared to the FAStT storage server configured with Fibre Channel 
   drives. Slower response times of SATA disk drives compared to Fibre 
   Channel disk drives cause higher I/O retries from the FAStT storage 
   server controllers, resulting in a greater number of informational 
   events logged. In addition, the number of information events reported in
   the FAStT storage server event log will also grow in proportion to the 
   increase in I/Os to the Logical Drives. In all cases, the FAStT Storage
   Server controller will always successfully service the timeout I/O on 
   the subsequent retries. 
   
=======================================================================
                
1.2  Enhancements
-----------------
     N/A

=======================================================================
            
1.3  Prerequisites
------------------
     N/A

=======================================================================
            
1.4  Dependencies
-----------------


   IBM FAStT Storage Manager version 8.41 provides full management support
   IBM machine types 3552 and 3542 storage subsystems that have at least
   firmware version 04.00.02.xx, IBM machine type 1742 (models 1RX, 1RU)
   storage subsystem that have at least firmware version 05.00.04.xx or
   IBM machine types 1742 (models 90X, 90U) and 1722 storage subsystems
   that have at least firmware version 05.3x.xx.xx.
    
   The only IBM FAStT Storage Manager 8.41 supported management function 
   on controllers with firmware version 04.xx.xx.xx to 04.xx.01.xx is 
   controller firmware and NVSRAM download. 
   
=======================================================================

2.0   Change History
-----------------------------

======================================================================

2.1 Version history.
       
   
    - 05.41.11.0x - 4/08/2004
      - 73777 (LHA) Drive firmware downloads fail 
      - 75567 (CL #75479) Memory leak beginning in controller fw 
              version 05.40.xx.xx code thread.     
    
    - 05.41.01.0x - 12/22/2004  -  initial release 
      - Support for IBM TotalStorage EXP100 drive expansion enclosures.
    
=======================================================================
        
2.2 Code levels at time of release are as follows
-------------------------------------------------

                                           
     1. Storage Controller Firmware versions (Web Download):
     
        The controller firmware files that are posted in the IBM support 
        web site can only be download to the FAStT controllers that already 
        have the controller firmware version 05.41.xx.xx installed. These 
        controller firmware files are basically the same with the firmware
        files included in the FAStT Storage Manager V8.41 Support for 
        FAStT EXP100 SATA Storage Expansion Unit CD that is in the EXP100
        shipping container. However, it is packaged so that it can not
        be accidently loaded in non-supported FAStT storage server 
        configurations.
        
          FAStT 900:  FW_05411101_05400200.dlp
          FAStT 600:  SNAP_05411101.dlp

     2. Storage Controller NVSRAM versions:
        These controller NVSRAM files are available in both the FAStT Storage 
        Manager V8.41 Support for FAStT EXP100 SATA Storage Expansion Unit 
        CD and the IBM support web site.    

          FAStT 900:  N1742F900R841V05.dlp
          FAStT 600:  N1722F600R841V03.dlp
       
                                    
   Refer to the IBM TotalStorage™ Disk Storage Systems Technical Support 
   web site for the latest released code levels.
   http://www.ibm.com/storage/support/fastt
   
=======================================================================
              
3.0   Installation and Setup Instructions
-----------------------------------------

3.1  Important: You must install the firmware update prior to downloading  
                the NVSRAM update.

   To download firmware, do the following: 
   
   a.  Open the Subsystem Management window. 
   b.  Click Storage Subsystem => Download => Firmware. 
       Follow the online instructions.

   To download NVSRAM, do the following: 
   
   a.  Open the Subsystem Management window. 
   b.  Click Storage Subsystem => Download => NVSRAM. 
       Follow the online instructions.
       
3.2  After the controller firmware and NVSRAM is updated, consider
     checking the IBM TotalStorage™ Disk Storage Systems Technical Support 
     web site for the latest released drive expansion enclosure ESM 
     firmware and the Fibre Channel hard drive firmware. 
     
   To download drive expansion ESM firmware, do the following: 
   
   a.  Open the Subsystem Management window. 
   b.  Click Advanced => Download => Environmental(ESM) Card Firmware. 
       Follow the online instructions.

   To download hard disk drive firmware, do the following: 
   
   a.  Open the Subsystem Management window. 
   b.  Click Advanced => Download => Drive Firmware. 
       Follow the online instructions.
      

=======================================================================
                                
3.2  Helpful Hints
------------------

1. The ideal configuration for SATA drives is one drive in each EXP per 
   array, one logical drive per array and one OS disk partition per logical
   drive. This configuration minimizes the random head movements that increase
   stress on the SATA drives. As the number of drive locations to which the
   heads have to move increases, application performance and drive reliability
   may be impacted. If more logical drives are configured, but not all of 
   them used simultaneously, some of the randomness can be avoided. SATA 
   drives are best used for long sequential reads and writes.
 
2. IBM recommends 2 hot spares per EXP100 drive expansion enclosure - 
   one in an even slot and the other in an odd slot. To fully protect 
   against single EXP100 ESM loss, 8 hot-spares will be required which results 
   in a FAStT storage server configuration with at least four EXP100 
   enclosures. If there are not enough enclosures for hot-spares or not 
   enough hot-spares, some of the arrays will be in degraded state when a
   single ESM in an EXP100 enclosure fails. However, the logical drive 
   accessibility and data availability are still intact. The failing ESM 
   must be replaced as soon as possible.

   In the FAStT 900 configuration with two redundant drive loops, it is 
   recommended to put half of the hot-spares in one redundant drive loop 
   and the rest on the other redundant drive loop.
  
   Note: a total of 15 hot-spares can be defined per FAStT storage server 
   configuration

3. If you are unable to see the maximum number of drives during 
   Automatic Configuration, you should be able to use Manual 
   Configuration to select individual drives and select the maximum 
   number of drives allowed.

4. Depending on the storage subsystem that you have purchased, you
   may have to purchase the FAST storage partitioning premium feature
   option or an option to upgrade the number of supported partitions
   in a storage subsystem. Please see IBM Marketing representatives
   or IBM resellers for more information.
   
   - IBM FAStT600 storage subsystem (machine type 1722): The standard
     configuration does not have the FAST storage partitioning premium
     enabled. Four partition, eight partition and an upgrade from four
     to eight partition storage partitioning premium feature options 
     can be purchased.

   - IBM FAStT900 storage subsystem (machine type 1742 - models 90X and
     90U): The standard configuration has 16 partition storage partitioning
     premium option installed. An upgrade from 16 to 64 partition storage
     partitioning premium feature option can be purchased.

5. It is recommenced to either use the switch zoning function or rearrange 
   the SAN device connections so that only the maximum number of host 
   connections can be seen and log into the controller. The FAStT Storage 
   Subsystem (IBM machine type 1742 - all models) have two ports per 
   controller -  one port per minihub slot. The FAStT Storage FAStT600 
   (IBM machine type 1722 - all models) has two ports per controller. 

=======================================================================

4.0 Configuration Information
-----------------------------

        
4.1 Configuration Settings
--------------------------

1. By default the IBM FAStT Storage Manager 8.41 firmware does not 
   automatically map logical drives if storage partitioning feature is
   enabled. This means that the logical drives are not automatically 
   presented to host systems.

   For a new installation, after creating new arrays and logical drives; 
   a. If your host type is not Windows NT, create a partition with your 
      host type and map the logical drives to this partition. 
   b. If your host type is Windows NT, you can map your logical drives to the 
      "Default Host Group" or create a partition with a NT host type.   
                                 
   When upgrading from previous versions of IBM FAStT Storage 
   Manager to version 8.41. 
   a. If upgrading with no partitions created and you have an operating
      system other than Windows NT,  you will need to create a partition
      with your host type and map the logical drives from the "Default
      Host Group" to this partition.
   b. If upgrading with Storage Partitions and an operating system other 
      than Windows NT is accessing the default host group, you will need 
      to change the default host type.  After upgrading,  the default host 
      type is reset to Windows NT. 
              
   Refer to the IBM FAStT Storage Manager online help to learn
   more about creating storage partitions and changing host types.

2. When you are configuring IBM machine type 1722 and 1742 storage
   subsystems as boot devices, contact IBM support for supported 
   configurations and instructions for configuring LUNs in the IBM 
   storage subsystems as boot devices. 

3. Running script files for specific configurations. Apply the 
   appropriate scripts  to your subsystem based on the instructions you 
   have read in the publications or any instructions in the operating 
   system readme file. A description of each script is shown below.

   - SameWWN.scr: Setup RAID controllers to have the same World Wide 
     Names. The World Wide Names (node) will be the same for each 
     controller pair. The NVSRAM default sets the RAID controllers to have 
     the same World Wide Names.

   - DifferentWWN.scr:  Setup RAID controllers to have different World 
     Wide Names. The World Wide Names (node) will be different for each 
     controller pair. The NVSRAM default sets the RAID controllers to have 
     the same World Wide Names.

   - EnableDriveMigration.scr:  The Enable drive migration script scans 
     the drives for configurations when they are added to a storage system 
     and will also attempt to use configurations found on the newly added 
     drives. The NVSRAM default will enable drive migration.

   - DisableDriveMigration.scr:  The disable drive migration script 
     allows the addition of disk drives while the system is running. in 
     addition, it identifies the drives as unused capacity regardless of 
     past drive configuration. The NVSRAM default will enable drive 
     migration.
     
6. If the controller in the IBM FAStT Storage Server with firmware 
   05.3x.xx.xx is connected to a SAN with more than 64 host connections
   per controller port that can log into the controllers, one must 
   either use the switch zoning function or rearrange the SAN 
   connections so that only the maximum number of host connections can
   be seen and log into the controller. The FAStT Storage Subsystem 
   FAStT900, FAStT700 (IBM machine type 1742) have two ports per controller -
   one per minihub slot. The FAStT Storage FAStT600 (IBM machine type 1722) 
   has two ports per controller. 

=======================================================================

4.2 Unsupported configurations
------------------------------

   The following lists configurations that are currently not being 
   supported with IBM FAStT Storage Manager 8.41.

   1. Fibre Channel loop environments with the IBM Fibre Channel Hub, 
      machine type 3523 and 3534, in conjunction with the IBM Fibre Channel 
      Switch, machine types 2109-S16, 2109-F16 or 2109-S8. In this 
      configuration, the hub is connected between the switch and the IBM 
      Fibre Channel RAID Controllers.

   2. The IBM Fibre Channel Hub, machine type 3523, connected to IBM 
      machine type 1722, 1742, 3542 and 3552.

=======================================================================

5.0   Unattended Mode
---------------------
        N/A

=======================================================================

6.0   WEB Sites and Support Phone Number
----------------------------------------

   6.1  IBM TotalStorage™ Disk Storage Systems Technical Support web site:
        http://www.ibm.com/storage/support/fastt

   6.2  IBM TotalStorage™ Marketing Web Site:
        http://www.storage.ibm.com/hardsoft/disk/fastt/index.html

   6.3  If you have any questions about this update, or problem
        applying the update go to the following HelpCenter World
        Telephone Numbers URL:
        http://www.ibm.com/planetwide

=======================================================================

7.0   Trademarks and Notices
----------------------------

        7.1  The following terms are trademarks of the IBM Corporation
             in the United States or other countries or both:

               IBM
               
               FAStT
               
               ToTalStorage™ 

               the e-business logo

               xSeries
               
               pSeries

               HelpCenter

               Microsoft, Windows, and Windows NT are trademarks of Microsoft
               Corporation in the United States, other countries, or both.
              
               Java and all Java-based trademarks and logos are 
               trademarks or registered trademarks of Sun Microsystems, 
               Inc. in the United states, other countries, or both.

               UNIX is a registered trademark of The Open Group in the 
               United States and other countries.

               Linux is a registered trademark of Linus Torvalds.

               Other company, product, and service names may be 
               trademarks or service marks of others.


=======================================================================

8.0   Disclaimer
----------------

        8.1  THIS DOCUMENT IS PROVIDED "AS IS" WITHOUT WARRANTY OF
             ANY KIND. IBM DISCLAIMS ALL WARRANTIES, WHETHER EXPRESS
             OR IMPLIED, INCLUDING WITHOUT LIMITATION, THE IMPLIED
             WARRANTIES OF FITNESS FOR A PARTICULAR PURPOSE AND
             MERCHANTABILITY WITH RESPECT TO THE INFORMATION IN THIS
             DOCUMENT. BY FURNISHING THIS DOCUMENT, IBM GRANTS NO
             LICENSES TO ANY PATENTS OR COPYRIGHTS.


        8.2  Note to U.S. Government Users -- Documentation related to
             restricted rights -- Use, duplication or disclosure is
             subject to restrictions set forth in GSA ADP Schedule
             Contract with IBM Corporation.
