# Enabling and disabling copy back mode

Note: Copy back is supported on the ServeRAID-6M and ServeRAID-6i controllers only. It is not supported in cluster or failover pair configurations.

Use this action to change the copy back-mode setting. This setting determines if the ServeRAID Manager restores a logical drive's original configuration after you replace a failed drive in an array.

Copy back is enabled by default except when you upgrade the ServeRAID software from a previous release; then, copy back mode is disabled by default.

1. In the tree, click (controller).
2. Right-click Enable or Disable copy back mode.

## More information

- Understanding copy back mode

Glossary | Contents

x-0370-SRM-00-05-EN