This README file contains the latest information about the  
IBM TotalStorage™ DS4000 Mid-range disk system controller firmware
version 05.3x.xx.xx.

Refer to the IBM TotalStorage™ Support Web Site or CD for the IBM 
DS4000 Storage Manager Version 9 Installation and Support Guide for 
Windows 2000/Server 2003, Netware, ESX Server, and Linux or the IBM 
DS4000 Storage Manager version 9 Installation and Support Guide for 
AIX, HP-UX, Solaris, and Linux on POWER publication for firmware 
and NVSRAM download instructions.

For other related publications (refer to Related Publications in the 
installation and support guide) and the latest information and 
updated README file.

Last Update:  03/18/2005

Products Supported: 
    --------------------------------------------------------------
   | DS4000 Model        | Machine Type  | Model Number           |
   |---------------------|---------------|------------------------|
   | DS4500 (FAStT900)   |     1742      | 90X, 90U               |
   |---------------------|---------------|------------------------|
   | DS4400 (FAStT700)   |     1742      | 1RX, 1RU               |
   |---------------------|---------------|------------------------|
   | DS4300 (FAStT600)   |     1722      | 6LX, 6LU, 60X, 60U     |
   |---------------------|---------------|------------------------|
   | FAStT500            |     3552      | 1RX, 1RU               |
   |---------------------|---------------|------------------------|
   | FAStT200            |     3542      | 1RX, 1RU, 2RX and 2RU  |
    --------------------------------------------------------------
  
 NOTE 1
   For the following DS4000 models it is strongly encouraged by IBM 
   to migrate the controller firmware to version 06.12.xx.00 level.
     DS4300 (FAStT600) Dual controller models (60X, 60U)
     DS4400 (FAStT700) 1RX, 1RU
     DS4500 (FAStT900) 90X, 90U

   All future maintenance releases for these DS4000 models will be 
   with version 06.12.xx.00 controller firmware levels.
   
   See IBM TotalStorage Support web site for further details on 
   migrating the DS4000 models from controller firmware 05.30.xx 
   or 05.34.xx to 06.12.xx.00 level.
   http://www-307.ibm.com/pc/support/site.wss/document.do?lndocid=MIGR-59007
   
   Pre-requisite requirement prior to upgrading the controller 
   firmware to 06.12.xx.00 is to have all DS4000 EXP700 expansion 
   units at ESM firmware level 9326 or higher.
   
 NOTE 2
   The following DS4000/FAStT models will continue to be supported by
   the 05.30.xx and 05.34.xx controller levels. These models cannot be
   migrated to 06.12.xx firmware level.
     
     05.30.xx
     FAStT200, FAStT500

     05.34.xx
     DS4300 Single Controller (6LX, 6LU)
     
    

CONTENTS
--------
1.0 Overview
2.0 Change History
3.0 Installation and Setup Instructions
4.0 Configuration Information
5.0 Unattended Mode
6.0 Web Sites and Support Phone Number
7.0 Trademarks and Notices
8.0 Disclaimer

=======================================================================
1.0 Overview
------------

   This IBM DS4000 mid-range disk system controller firmware 
   release includes the IBM DS4000 05.3x.xx.xx disk system c
   controller firmware and NVSRAM files for upgrading the following 
   IBM machine types - 1722(all models), 1742 (all models), 3542 
   (all models ) and 3552 (all models).
   
   The IBM DS4000 Storage Manager Version 9 Installation and Support 
   Guides for Windows 2000/Server 2003, Netware, ESX Server, and 
   Linux or the IBM DS4000 Storage Manager Version 9 Installation and 
   Support Guides for AIX, HP-UX, Solaris and Linux on POWER 
   publication is available on IBM's Support Web Site as a 
   downloadable Portable Document Format (PDF) file. 

   In addition, IBM DS4000 FlashCopy and IBM DS4000 Remote Mirror 
   premium feature options are purchased separately. The IBM 
   FlashCopy option requires firmware version 05.00.04.xx or higher. 
   The IBM Remote Mirror option requires firmware version 
   05.20.0x.xx or higher. 
   
   The DS4000 storage partitioning premium feature is standard on all 
   IBM DS4000 disk systems with the exception of the IBM DS4300 
   (machine type 1722) mid-range disk system. Please contact IBM 
   Marketing representatives or IBM resellers if you want to purchase 
   the IBM DS4000 storage partitioning premium feature option for it. 

   Refer to the IBM Support Web Site for the latest Firmware and 
   NVSRAM files for the IBM DS4000 Mid-range disk systems.

=======================================================================
1.1 Limitations
---------------

IMPORTANT:
The listed limitations are cumulative. However, they are listed by the 
DS4000 mid-range disk controller firmware and Storage Manager host 
software releases to indicate which controller firmware and Storage 
Manager client software release that they were first seen and 
documented. 

New limitations with version 05.30.23.00, 05.34.08.00 controller 
firmware maintenance releases.

1. Do not cut and paste the information in the DS4000 Storage 
   Manager Version 9 online help into the DS4000 Storage Manager 
   script command window or into the text file that will be used as 
   input for the SMcli script engine. Extra space may be inserted in 
   the required parameter names which will cause error(s) during the 
   script command execution. (IBM problem record 267873)
 
2. Currently, IBM does not support Gold key Premium Feature as a 
   chargeable upgrade. The Gold key Premium Feature is enable or 
   disable depending on the DS4000 mid-range disk system models.

3. The Asynchronous Remote Mirroring utility, asyncRVMUtil, is not
   supported. This utility is used to automatically synchronize the 
   logical drives in the Remote Mirroring pairs. Please contact IBM 
   representatives or resellers for the support of this utility in 
   the future.

Limitations with current and previous maintenance releases.

1. Upgrading FAStT500 with 512MB Cache. When upgrading controller 
   firmware on a FAStT500 (machine type 3552) with 512MB of cache, 
   all reading and writing to the disk system must be stopped. The  
   controller needs to be rebooted before upgrading controller firmware 
   followed by NVSRAM.

   To determine disk system controller cache level, perform the 
   following:

   a. On a storage management station start the client software and 
      select a storage subsystem.
   b. Select Tools -> Manage Device to open the Subsystem Management 
      Window.
   c. Highlight the Storage Subsystem that you are upgrading and then 
      select Storage Subsystem -> Profile. It may take a little time 
      for it to create the Storage Subsystem profile.   
   d. Under the Controllers heading is an entry that displays 
      information similar to the following example:

      Cache/processor size (MB):  256/32

   If this setting is listed as 512/32 you will need to arrange to 
   perform this upgrade procedure at a time that you can stop I/O to 
   the Storage Subsystem in order to ensure a successful firmware 
   download and installation.

2. DS4000 Storage Manager prompts you for a password if all hard 
   disk drives are removed from the storage subsystem.

   After removing all drives from a storage subsystem or if drives   
   do not have power but the controller power is on. The IBM DS4000 
   Storage Manager will prompt you for a password when trying to 
   start the software or when attempting to perform protected 
   operations. Any password entered will fail.

   Password information is stored on a reserved area of each hard 
   disk drive on the storage subsystem. Each drive stores a 
   mirrored copy of the password data. When there are no drives 
   in the disk system, the storage management software does 
   not find the password data when you attempt password protected 
   operations. Add one drive to the disk system and retry the 
   operation.
   
   If the DS4000 controller unit has power, then turn power off 
   the controller unit. The DS4000 controller unit shall not be 
   powered on until the EXP expansion units are attached and 
   powered on. Properly attach all expansion units (with drives 
   installed), to the DS4000 controller unit and apply power to 
   the EXP. The controller can now be powered on.  At this point 
   the mid-range disk system can be re-discovered and managed using 
   the IBM DS4000 Storage Manager.

3. Auto LUN/Array Transfer is not enable for IBM AIX and SUN Solaris 
   operating systems. If arrays failover to an alternate controller 
   and the failed controller is replaced and then brought back online, 
   the arrays do not automatically transfer to the preferred 
   controller. The operation must be done manually by selecting 
   the redistributing arrays menu option in the storage subsystem 
   window of the IBM DS4000 Storage Manager.
      
4. Display issues when using 256 color settings. A brownish hash 
   pattern is displayed on the windows and in online help when running 
   in 256 color mode.  Run the DS4000 Storage Manager 8 or higher 
   in a higher display mode.

5. The DS4000 Storage Management dialog windows may be displayed 
   cropped without the vertical and horizontal scroll bars. Just move 
   the mouse pointer over the edge of the window until the mouse 
   pointer change to window resize pointer, left click and hold to 
   grip the window edge to resize it. 

6. If you get "Error 21 - The operation cannot complete because a 
   ...  is in progress" error when you issue a subsystem management 
   command from the IBM DS4000 Storage Manager, the command may 
   be cached. If the command is cached, the IBM DS4000 Storage Manager 
   client will run the command as soon as the controller resources are 
   available. Wait for at least ten minutes and check to see whether 
   the command has been run. If not, re-attempt the command. 

7. When a DS4000 disk system with controller firmware 05.3x.xx.xx is 
   connected to a SAN with more than 64 host port logins. Fibre 
   channel switch zoning must be used or the number of SAN 
   connections must be configured to be no more then the maximum 
   allowed number of host login connections allowed by the controller. 
   
   The DS4500, DS4400 and FAStT500 IBM machine type 1742 and 3552)
   have two ports per controller - one per minihub slot. 
   The DS4300 (IBM machine type 1722) has two ports per controller. 
   The FAStT200 IBM machine type 3542) has only one port per 
   controller.
 
8. The IBM DS4000 mid-range disk system hardware and software is 
   designed to have redundant paths from the host system to ensure 
   the availability of disk storage. However, it is possible to 
   connect a single host adapter from the host system to one of 
   the controller minihubs and then connect this minihub to the 
   minihub of the other controller. This configuration will create 
   a FC-AL loop between the host adapter and the two IBM DS4000 
   disk system controllers and no redundant path to the host system. 
   When connecting the two minihubs together, always connect the 
   "IN" port of one minihub to the "OUT" port of the other minihub 
   or vice versa. Do not connect the "IN" port of one to the "IN" 
   port of the other minihub or the "OUT" port of one minihub to 
   the "OUT" port of the other minihub.
                     
9. When creating a Remote Mirror from a base volume the following 
   restriction applies. First, a flashcopy has been created using 
   a base volume and the base volume is experiencing write and 
   read operations. Second, a mirror relationship has been created, 
   using the base volume as the primary volume in the mirrored pair. 
   As the mirror relationship is created, the flashcopy volume fails. 
   
   The work around to this type problem is to stop write and read 
   operations to the base volume while creating the mirror 
   relationship. Alternatively, if the mirror relationship is 
   created before creating the flashcopy volume, the problem will
   not occur.

10. In Microsoft cluster, MSCS configurations, the MSCS service 
    must be stopped and set to manual start after server is 
    rebooted. The Clusdisk driver must be set to offline and the 
    Windows server must be rebooted before uninstalling the RDAC 
    driver in the server. 
    
    If the Clusdisk driver is not set to offline and the MSCS 
    service is not set to manual start, the MS cluster service 
    will not start after the new RDAC driver is installed. 
    The cluster cannot bring the Quorum disk resources online because 
    the disk signature changes caused the problem. 
    The workaround is stated in the first sentence of this 
    paragraph.
    
    To recover from this problem, you must:
     
    1. Look up the old disk signatures of the disk that are defined 
       as cluster disk resources. They could be found either in 
       the registry under the 
HKLM/System/CurrentControlSet/Services/Clusdisk/Parameters/Signatures
       registry key or in the cluster.log file.
    2. Look up the new disk signatures of the disks that are 
       defined as cluster disk resources using the dumpcfg 
       utility that is packaged in the Microsoft Windows resource 
       kit. 
    3. Compare the new and old disk signatures. If new disk 
       signature did not match the old signature, you have to 
       change the new disk signature to the old disk signature 
       values by using the dumpcfg command. The syntax of the 
       command is:
       
       dumpcfg.exe -s <old-signature> <Disk#>     
       For example, dumpcfg.exe -s 12345678 0 

12. In a SAN boot configuration, before updating the Windows RDAC 
    driver in a Windows server, one of the two Fibre Channel (FC) 
    cables that are connected to the server must be disconnected. 
    The Windows server will blue screen during the reboot after the 
    un-installation of the RDAC driver if one of the FC cables 
    is not removed. (IBM problem record 258127)

12. Controller diagnostics will not run in a DS4000 storage subsystem 
    with single controller.
    
=======================================================================
                
1.2 Enhancements
----------------
     N/A

=======================================================================
            
1.3 Prerequisites
-----------------
     N/A

=======================================================================
            
1.4 Dependencies
----------------

   The IBM TotalStorage DS4000 Storage Manager Version 9 provides full 
   management support for:

   IBM machine types 3552 and 3542 (FAStT200, FAStT500) disk systems 
   that have a minimum firmware version of 04.00.02.xx. 
   
   IBM machine type 1742 (DS4300 models 1RX, 1RU) disk system that 
   have a minimum firmware version of 05.00.04.xx.
   
   IBM machine types 1742 (DS4500 models 90X, 90U) and 1722 (DS4300) 
   mid-range disk systems that have a minimum firmware version of 
   05.3x.xx.xx.
    
   The only IBM TotalStorage DS4000 Storage Manager Version 9 
   supported management function on controllers with firmware 
   version 04.xx.xx.xx to 04.xx.01.xx is the ability to download 
   controller firmware and NVSRAM. 
      
=======================================================================

2.0 Change History
------------------

======================================================================

2.1 Version History
-------------------

This is the latest maintenance release of IBM DS4000 TotalStorage™
controller firmware / NVSRAM for the following DS4000 mid-range 
disk system models: 
FAStT200, FAStT500, DS4400 (FAStT700), DS4500 (FAStT900).
   
Version 05.30.23.00 03/31/2005 (First Quarter 2005 maintenance release)
    
    IBM Problem
    Record        Abstract 
    ---------     -------------------------------------------------
    260503        Storage Partition feature key changed after firmware 
                  upgrade and reboot
    263452        Controller sends LPE with out specifying ID in 
                  primitive
    265068        Media Scan not running on all LUNs
    hlpct_53699   Hot spare capacity reported as unconfigured in 
                  controller firmware 05.30.19.00
    269144 80751 (78907) Data corruption while running I/O to 
                 snapshot on fastt600 where the LBA in the head
                 and tail did match as expected
    269145 81685 (79691) Prefetch requests not generated with RAID 1 
                 16K segments 
    hlpct_51223 82372 (78999) Mirror relationship becomes out of sync 
                 when path is broken between switch ISL
    269146 83556 (77888) Invalid CDB for read capacity caused 
                         I/O error
    269147 83831 (82874) Controller panic in SOD routines
    269148 84622 (82306) DBM Blockset mismatch causes occasional 
                         controller reboot
    269152 84739 (83625) Bad record entry in DBM 
    269153 85319 (66322) PANIC error occurred on fastt600 controller
    275524 85343 (66322) PANIC error occurred on fastt600 controller
    269154 85476 (84906) memory fault from mhmI2cRequestHandle
    269155 85728 (84886) Read Capacity command returns the new capacity 
                         before the expansion of a volume is completed
    269156 85757 (85456) Data corruption after large VolGrp with 2 luns


This is the latest maintenance release of IBM DS4000 TotalStorage™
controller firmware / NVSRAM for the following DS4000 mid-range disk 
system model: DS4300 (FAStT600).
 
Version 05.34.04.00 03/31/2005 (First Quarter 2005 maintenance release)

    IBM Problem
    Record        Abstract 
    ---------     -------------------------------------------------
    260503        Storage Partition feature key changed after firmware 
                  upgrade and reboot
    263452        Controller sends LPE with out specifying ID in 
                  primitive
    265068        Media Scan not running on all LUNs
    269157 80752 (78907)  Data corruption while running I/O to 
                          snapshot on fastt600 where the LBA in the 
                          head and tail did match as expected
    269158 83558 (77888) Invalid CDB for read capacity caused 
                         I/O error
    269159 83833 (82874) Controller panic in SOD routines
    hlpct_53699 84041 (79556) Hot spare capacity reported as 
                              unconfigured in controller firmware 
                              05.30.19.00
    269161 84623 (82306)DBM Blockset mismatch causes occasional 
                         controller reboot
    269162 84740 (83625) Bad record entry in DBM 
    269163 85321 (66322) PANIC error occurred on fastt600 controller
    269165 85729 (84886) Read Capacity command returns the new 
                         capacity before the expansion of a volume 
                         is completed


2.2 Previous Version History for 05.30.xx.xx controller firmware
----------------------------------------------------------------

    This is previous maintenance releases of the DS4000 mid-range 
    disk system controller firmware and NVSRAM. 
    The fix lists for the 05.30.xx.xx controller code releases.
    Supported DS4000 subsystem controller models:
     FAStT200, FAStT500, DS4400 (FAStT700), DS4500 (FAStT900).

Version 05.30.21.00 code release
  
   IBM Problem Record       Abstract
   ------------------       ---------------------------------------       
   71338  253097            Need a way to clear both SSTOR header and 
                            DBM database from a given drive 
   78095  253100 (76791)    Data corruption detected by hammer 
                            after transfer
   78384  253101 (75360)    Data corruption while running triple 
                            fault test
   78437  253104 (74842)    Data corruption when pulling and 
                            replacing a drive
   79063  253106 (78862)    Reconstruction active to a GHS for the 
                            second 
   79479  253107 (79298)    Data corruption occurred after spindown of 
                            GHS
   79556  253109            (BST) The capacity of the hotspare shows 
                            in the logical/physical view
   79698  253111 (79212)    Data corruption during triple fault test      
   79819  253112 (70279)    Divide by zero error while executing 
                            _cfgSetLunS
   79590  hlpct52107(79573) Multiple controllers go into PCI lockdown
   81062  hlpct_53699       upgraded fw to 05.30.19, unconf capacity 
                            is appear  
   78999  hlpct_51223       mirroring relationship be established 
                            once isl out  
   81444  255496            DS4000 RAID 10 not any longer redundant 
                            after DVE
   77628  253323            Volume state not consistent between the 
                            controllers
   77580  253322            Controller did not clear AEN after the 
                            failed drive
   77502  253310            Controllers did not agree on the state 
                            of a drive
   77878  253330            Memory fault during SOD when IAC received   
   77950  253336            Memory fault while running sysReboot 
   78049  253340            Mapping exceeds 32-lun limit for default 
                            host
   78348  253384            Fatal vproc after replacing drive
   80018  253394            Watchdog timeout while running I/Os 
                            and sysReboot
         
Version 05.30.19.00 07/2004 Maintenance Release  
    
   IBM Problem Record  Abstract
   ------------------ ----------------------------------------
    76117             Rebooting controller during FlashCopy
    71777             Can't create volume if drive sizes are similar 
                      (181 and 146GB)
    72991 hlpct_42401 Error importing a 7.3 Gig FlashCopy LUN
    73058  C221434    Recovery guru indicates Subsystem errors when 
                      no error exists
    72230 (71757)     AWM and Recovery Guru give conflicting status 
    78208 (78004)     242386 - RAID1 remained degraded after a drive 
                      pull/replace
    78344 (77338)     Fatal vproc after replacing drive
    78606 (78357)     disk array became unmanageable in benchmark
    73225 (72542)     Log Select with PCR bit set to 1 fails to reset 
                      drive stat
    73409 (70407)     C221434 Recovery guru indicates Subsystem error
    73427 (71088)     Drives came back unassigned after powering off 
    73686 (72414)     Inconsistent vdUnit structure between two 
                      controllers     
    75055             DCE operation on RAID 1 volume invalidates tray 
                      loss protection       
    75283  C236739    I/O error during controller offline testing  
                      with SUN and WS03 
    76013 (75805)     Incomplete transfer of host information during 
    76148             Controller assertion when validateCmdInfo 
                      routine calls cfgSaveCmdInfo
    76184 (75746)     Ancient I/O (mode select I/O) during 2 second 
    76881             IAF process hangs if multiple IAFs in progess 
                      on same volume group    
    77497 (77464)     Controllers did not agree on the state of a 
                      spindown drive
    77530 (65736)     How a Controller locks down on too many ECC 
                      errors should 
    77534 (75629)     MEMORY FAULT in "symPrepareAltControllerInfo"  
    77552 (75895)     Request for ctlr resets to be blocked by ctlr 

Version 05.30.16.00  04/2004 Maintenance Release

    IBM Problem Record  Abstract      
    ------------------  -----------------------------------------
    71777 (67670)        Can't create volume if drive sizes are 
                         similar (181 and 146GB) 
    72991 (72339)        hlpct_42401 Error importing a 7.3 Gig 
                         FlashCopy 
                         LUN 
    73058 (70407)        C221434 Recovery guru indicates Subsystem errors 
                         when no error exists 
    72244 (71546)(59229) CAL00622 Have FW check alt path to FC drive 
                         before failing
    68894                Analysis of a MEL log shows Dacstore Scrub is 
                         repeating on a volume group
    69761 (68870)(68351) TD_PT871 I/O Error after Sonoran 3 
                         controller swapped into
    69941 (69630)        There is a memory leak when sending DOMI 
                         messages.
    70383 (70309)        C222814 Data corruption on AIX hosts.
    70419 (68603)        Ancient I/Os reported during sysReboot stress
    70551 (68445) C219318 C217537 Data miscompare while doing online 
                         controller 
    71550 (62602) CAL01413 Critical Event for Loss of Drive Path 
                           Redundancy
  
- Modify the NVSRAM file to disable Cache Sync in the Windows 2000 
  host region.

Version 05.30.12.00  12/2003 Maintenance Release

Version 05.30.09.01  09/2003 Initial Web Release initially a fee base 
                     firmware.

Version 05.30.09.00  09/2003 Initial Release and Upgrade from 
                     controller firmware 04.xx.xx.xx.

2.3 Previous Version History for 05.34.xx.xx controller firmware
----------------------------------------------------------------
   
    This is previous maintenance releases of the DS4000 mid-range  
    disk system controller firmware and NVSRAM. 
    The fix lists for the 05.34.xx.xx controller code releases.
    Supported DS4000 disk system controller model: 
    DS4300 (FAStT600)

Version 05.34.07.00 code release

   IBM Problem Record      Abstract      
   ------------------      ---------------------------------------
   71338  253097           Need a way to clear both SSTOR header and 
                           DBM database from a given drive
   78095  253100  (76791)  Data corruption detected by hammer after 
                           transfer
   78384  253101  (75360)  Data corruption while running triple fault 
   78437  253104  (74842)  Data corruption when pulling and replacing 
                           a drive
   79063  253106  (78862)  Reconstruction active to a GHS for the 
                           second 
   79479  253107  (79298)  Data corruption occurred after spindown of 
                           GHS 
   79556  253109           (BST) The capacity of the hotspare shows 
                           in the logical/physical view
   79698  253111  (79212)  Data corruption during triple fault test      
   79819  253112  (70279)  Divide by zero error while executing 
                           _cfgSetLunS
   81761  255595f_1        memory leak problem with 5.34.02.00
   81444  255496           DS4000 RAID 10 not any longer redundant 
                           after DVE
   77628  253323           Volume state not consistent between the 
                           controllers
   77580  253310           Controllers did not agree on the state 
                           of a drive
   77878  253330           Memory fault during SOD when IAC received
   77950  253336           Memory fault while running sysReboot 
   78049  253340           Mapping exceeds 32-lun limit for default 
                           host
   78348  253394           Watchdog timeout while running I/Os and 
                           sysReboot

Version 05.34.04.00 Second Maintenance Release 

IBM Problem Record   Abstract      
-------------------  ---------------------------------------
    72232 (71757)    AWM and Recovery Guru give conflicting status
    78200 (78004)    242386 - RAID1 remained degraded after a drive 
                     pull/replace
    78345 (77338)    Fatal vproc after replacing drive
    78606 (78357)    disk array became unmanageable in benchmark
    74127 (70794)    One volume never finishes reconstruction when
    75769  237800    Multiple Hot Spare failures.                                  
    76014 (75805)    Incomplete transfer of host information during 
    76185 (75746)    Ancient I/O (mode select I/O) during 2 second
    76248 (76148)    Controller assertion when validateCmdInfo 
                     routine calls
    76265 (75283)    C236739 I/O error during controller offline 
                     testing
    76723 (75055)    DCE operation on RAID 1 volume invalidates 
                     tray loss protection
    77498 (77464)    Controllers did not agree on the state of a 
                     spindown drive
    77531 (65736)    How a Controller locks down on too many ECC 
                     errors 
    77535 (75629)    MEMORY FAULT in "symPrepareAltControllerInfo"  
    77553 (75895)    Request for ctlr resets to be blocked by ctlr 
    77577 (69894)    Controller did not clear AEN after the failed 
                     drive was replaced
    73409 (70407)    C221434 Recovery guru indicates Subsystem 
                     error
    73275 (73265)    Pick up Mojave 2 Flash driver changes into 
                     Sonoran 3 thread
    76148            Controller assertion when validateCmdInfo 
                     routine calls cfgSaveCmdInfo
    75283  C236739   I/O error during controller offline testing 
                     with SUN and WS03 

Version 05.34.02.00 04/2004 First Maintenance Release 

    The controller firmware version 05.34.xx.xx replaces the 
    controller firmware version 05.33.xx.xx. 
    
IBM Problem Record   Abstract      
-------------------  ---------------------------------------
    70561 (68445)    C219318 CMVC 217537: Data miscompare while 
                     doing online controller firmware downloads 
    70772 (68894)    Analysis of a MEL log shows Dacstore Scrub is 
                     repeating on a volume group 
    72993 (72339)    hlpct_42401 Error importing a 7.3 Gig 
                     FlashCopy LUN 
    73059 (70407)    C221434 Recovery guru indicates Subsystem errors 
                     when no error exists 
    70385 (70309)    C222814 Data corruption on AIX hosts. 
    70443 (68872)    Stable storage method write Header sends address 
                     of a pointer to main write Header method. 
    70444 (67313)    Memory fault when error reading drive headers at 
                     start-of-day. 
    67718 C214226    Logical drive shows rebuilding in Client but has 
                     finished in Controller.
    67990 (67720)    Improve handling of drive reported parity/CRC 
                     error
    68263 (67670)    Can't create volume if drive sizes are similar 
                     (181 and 146GB)
    68387 (68281)    Drive failed by controller still being logged 
                     after removing
    68506 (68410)    "Link Error" component location = "none" in 
                     MEL
    68580 (68565)    NVSRAM setting to ignore Sync Cache requests 
    68736 (68330)    DDE with devnum of 0 is logged when removed 
                     drive is present
    69202 (68807)    Profile not reporting correct unconfigured 
                     capacity on volume group
        
Version 05.33.07.00 09/2003 Initial Release

Version 05.33.05.00 09/2003 Initial Release for Netware only

           
=======================================================================
        
2.4 Code levels at time of release are as follows
-------------------------------------------------

       a. Controller firmware version 
       
          DS4500                  :  FW_05302300_05300300
          DS4400                  :  FW_05302300_05300300
          DS4300  (non-Turbo)     :  SNAP_05340800
          FAStT500                :  FW_05302300_05300300
          FAStT200                :  SNAP_05302300
                                            
       b. NVSRAM versions:
       
          DS4500                  :  N1742F900R830V06
          DS4400                  :  N1742R700R830V05
          DS4300  (non-Turbo)     :  N1722F600R834V01
          DS4300  (6LU/6LX)       :  N1722F60LR834V04
          FAStT500                :  N3552F500R830V05
          FAStT200                :  1RU - N3542-1RUR830V09
                                     2RU - N3542-2RUR830V12
                                    
 
 Refer to the IBM TotalStorage™ support web site for the latest 
 released code levels.
 http://www.ibm.com/servers/storage/support/disk/ 
          
=======================================================================
              
3.0 Installation and Setup Instructions
---------------------------------------

ATTENTION: If you have not already done so, please check the 
Dependencies section for ANY MINIMUM FIRMWARE REQUIREMENTS for the 
DS4000 mid-range disk system controllers, the drive expansion 
enclosure ESMs and the hard drives in the DS4000 configurations 
before upgrading the controller firmware. 
Make any firmware updates as required BEFORE proceeding to upgrade the 
DS4000 controller with the firmware and NVSRAM files packaged with this 
README file. FAILURE to observer the minimum firmware requirement might 
cause your DS4000 mid-range disk system to be OUT-OF-SERVICE.  

3.1  Updated the firmware of the ESMs in the attached drive expansion
     enclosures to latest levels before the upgrading the controller 
     firmware. 
     Specifically, if the to-be-updated controller is attached to any 
     EXP700 drive expansion enclosures, the EXP700 ESM firmware must 
     be updated to version 9326 or higher.
     
     To download drive expansion ESM firmware, do the following: 
   
     a.  Open the Subsystem Management window. 
     b.  Click Advanced => Download => Environmental(ESM) Card Firmware. 
         Follow the online instructions.
         
         Note: If the existing controller firmware in the DS4000 storage 
         server is of version 05.30.xx.xx or higher, the drive expansion 
         enclosure ESM firmware can be updated online with no downtime if 
         both ESMs in each of the drive expansion enclosures are 
         functional and one (and ONLY one) drive expansion enclosure is 
         selected in the ESM firmware download window for ESM firmware 
         updating at a time.
     
     Note: The latest ESM firmware versions for EXP700 and EXP710
     drive expansion enclosures are 9327 and 9629, respectively.

3.2 Important: You must install the firmware update prior to 
                downloading the NVSRAM update.

   To download firmware, do the following: 
   
   a. Open the Subsystem Management window. 
   b. Click Storage Subsystem => Download => Firmware. 
      Follow the online instructions.

   To download NVSRAM, do the following: 
   
   a. Open the Subsystem Management window. 
   b. Click Storage Subsystem => Download => NVSRAM. 
      Follow the online instructions.
       
3.3 After the controller firmware and NVSRAM is updated, consider
    checking the IBM TotalStorage™ Support web site for the latest 
    released drive expansion enclosure ESM firmware and the Fibre 
    Channel hard drive firmware. 
    http://www-1.ibm.com/servers/storage/support/index.html
     
   To download drive expansion ESM firmware, do the following: 
   
   a. Open the Subsystem Management window. 
   b. Click Advanced => Download => Environmental(ESM) Card Firmware. 
      Follow the online instructions.

   To download hard disk drive firmware, do the following: 
   
   a. Open the Subsystem Management window. 
   b. Click Advanced => Download => Drive Firmware. 
      Follow the online instructions.

=======================================================================
                                
3.4 Helpful Hints
-----------------

1. If you are unable to see the maximum number of drives during 
   Automatic Configuration, you should be able to use Manual 
   Configuration to select individual drives and select the maximum 
   number of drives allowed.

2. Depending on the DS4000 mid-range disk system that has been 
   purchased, there may be a need to purchase the DS4000 storage 
   partitioning premium feature option or an option to upgrade 
   the number of supported partitions in a disk system. 
   Please see IBM Marketing representatives or IBM resellers for 
   more information.
   
   - IBM DS4300 mid-range disk system (machine type 1722). The 
     standard configuration does not have the DS4300 storage 
     partitioning premium enabled. Four partition, eight partition, 
     sixteen and an upgrade from four to eight partition storage 
     partitioning premium feature options can be purchased. The 
     IBM DS4300 Turbo option comes with 8 partition storage 
     partitioning premium option installed. An upgrade to 64 
     partitions can be purchased for the IBM DS4300 with Turbo 
     option. 

   - IBM FAStT200, FAStT500, and DS4400 mid-range disk systems 
     (machine type 3542, 3552 and 1742 - models 1RU and 1RX, 
     respectively): The standard configuration has 64 partitions 
     storage partitioning premium option installed. No additional 
     storage partitioning premium feature options can be purchased 
     for these disk systems.

   - IBM DS4500 mid-range disk system (machine type 1742 - models 
     90X and 90U): The standard configuration has a 16 storage 
     partition premium option installed. An upgrade from 16 to 
     64 partition storage partitioning premium feature option can 
     be purchased.

=======================================================================

4.0 Configuration Information
-----------------------------

        
4.1 Configuration Settings
--------------------------

1. By default the IBM DS4000 Storage Manager Version 9 client, the 
   controller firmware does not automatically map logical drives if 
   storage partitioning feature is enabled. This means that the 
   logical drives are not automatically presented to host systems.

   For a new installation, after creating new arrays and logical 
   drives; 
   a. If your host type is not Windows NT, create a partition with your 
      host type and map the logical drives to this partition. 
   b. If your host type is Windows NT, you can map your logical drives 
      to the "Default Host Group" or create a partition with a NT host 
      type.   
                                 
   When upgrading from previous versions of IBM DS4000 Storage 
   Manager to Version 9. 
   a. If upgrading with no partitions created and you have an 
      operating system other than Windows NT,  you will need to 
      create a partition with your host type and map the logical 
      drives from the "Default Host Group" to this partition.
   b. If upgrading with Storage Partitions and an operating system 
      other than Windows NT is accessing the default host group, you 
      will need to change the default host type.  After upgrading,  
      the default host type is reset to Windows NT. 
              
   Refer to the IBM DS4000 Storage Manager online help to learn
   more about creating storage partitions and changing host types.

2. When you are configuring IBM machine type 1722, 1742, 3542 or 3552 
   disk systems as boot devices, contact IBM support for 
   supported configurations and instructions for configuring LUNs 
   as operating system boot devices. 

3. Running script files for specific configurations. Apply the 
   appropriate scripts  to your subsystem based on the instructions 
   you have read in the publications or any instructions in the 
   operating system readme file. A description of each script is 
   shown below.

   - SameWWN.scr: Setup DS4000 controllers to have the same World 
     Wide Names. The World Wide Names (node) will be the same for 
     each controller pair. The NVSRAM default sets the DS4000 
     controllers to have the same World Wide Names.

   - DifferentWWN.scr:  Setup DS4000 controllers to have different 
     World Wide Names. The World Wide Names (node) will be different 
     for each controller pair. The NVSRAM default sets the DS4000 
     controllers to have the same World Wide Names.

   - EnableDriveMigration.scr:  The Enable drive migration script 
     scans the drives for configurations when they are added to a 
     storage system and will also attempt to use configurations found 
     on the newly added drives. The NVSRAM default will enable 
     drive migration.

   - DisableDriveMigration.scr:  The disable drive migration script 
     allows the addition of disk drives while the system is running. 
     In addition, it identifies the drives as unused capacity 
     regardless of past drive configuration. The NVSRAM default will 
     enable drive migration.
     
4. When you are configuring IBM machine type 1742 or 3552 disk system 
   controllers in host cluster Remote Mirror configurations, contact 
   IBM support for supported host cluster configurations and 
   instructions for configuring IBM storage controllers in clustered 
   Remote Mirror configurations. 

=======================================================================

4.2 Unsupported configurations
------------------------------

   The following lists configurations that are currently not being 
   supported with IBM DS4000 Storage Manager Version 9.

   1. Fibre Channel loop environments with the IBM Fibre Channel Hub, 
      machine type 3523 and 3534, in conjunction with the IBM Fibre 
      Channel Switch, machine types 2109-S16, 2109-F16 or 2109-S08. 
      In this SAN configurations, the hub is connected between the 
      switch and the IBM DS4000 controllers.

   2. The IBM Fibre Channel Hub, machine type 3523, connected 
      to IBM machine type 1722, 1742, 3542 and 3552.

=======================================================================

5.0 Unattended Mode
-------------------
        N/A

=======================================================================

6.0 WEB Sites and Support Phone Number
--------------------------------------

   6.1 IBM TotalStorage™ Support: Disk Storage Systems web site:
       http://www.ibm.com/servers/storage/support/disk/

   6.2 IBM TotalStorage™ Disk Storage Systems: Overview Web Site:
       http://www.ibm.com/servers/storage/disk

   6.3 If you have any questions about this update, or problem
       applying the update go to the following HelpCenter World
       Telephone Numbers URL:
       http://www.ibm.com/planetwide
       IBM Directory of worldwide contacts

  IMPORTANT: 
  You should download the latest version of the DS4000 Storage 
  Manager software, the DS4000 mid-range disk controller firmware, 
  the DS4000 drive expansion enclosure ESM firmware and the drive 
  firmware at the time of the initial installation and when product 
  updates become available. To be notified of important product 
  updates, you must first register at the IBM Support and download 
  web site:  
  http://www-1.ibm.com/servers/storage/support/index.html
    
  Perform the following steps to register at the IBM Support and Download 
  Web site: 
  
  1. Click on My Support in the Additional support box in the right side 
     of the IBM TotalStorage support web page.
  2. The Sign In window displays. Either enter your IBM ID and Password 
     in the sign in area to sign in and proceed to step 6 or, if you are 
     not currently registered with the site, click Register Now. 
  3. The My IBM Registration window Step 1 of 2 opens. Enter the 
     appropriate information and click Continue to get to the second My 
     IBM Registration window. 
  4. In the My IBM Registration window Step 2 of 2, enter the appropriate 
     information and click Submit to register. 
  5. The My IBM Registration windows opens with the following message, 
     “Thank you for registering with ibm.com. Continue to explore ibm.com 
     as a registered user.” Click Edit Profile in the My IBM box on the 
     right side of the window. 
  6. The My Support window opens. Click Add Products to add products to 
     your profile. 
  7. Use the pull-down menus to choose the appropriate DS4000 disk  
     system and expansion enclosures that you want to add to your 
     profile.
     To add the product to your profile, select the appropriate box or 
     boxes next to the product names and click Add Product. 
  8. Once the product or products are added to your profile, click 
     Subscribe to Email folder tab 
  9. Select Storage in the pull down menu. Select Please send these 
     documents by weekly email and select Downloads and drivers and 
     Flashes to receive important information about product updates. 
     Click Updates. 
 10. Click Sign Out to log out of My Support.
 

=======================================================================

7.0 Trademarks and Notices
--------------------------

        7.1 The following terms are trademarks of the IBM Corporation
            in the United States or other countries or both:
                 
                 DS4000
                 
                 IBM
                 
                 FAStT
                 
                 ToTalStorage™ 

                 the e-business logo

                 xSeries
                 
                 pSeries

                 HelpCenter

                 Microsoft, Windows, and Windows NT are trademarks of Microsoft
                 Corporation in the United States, other countries, or both.
                
                 Java and all Java-based trademarks and logos are trademarks or
                 registered trademarks of Sun Microsystems, Inc. in the United
                 states, other countries, or both.

                 UNIX is a registered trademark of The Open Group in the United 
                 States and other countries.

                 Linux is a registered trademark of Linus Torvalds.

                 Other company, product, and service names may be 
                 trademarks or service marks of others.

=======================================================================

8.0 Disclaimer
--------------

        8.1 THIS DOCUMENT IS PROVIDED "AS IS" WITHOUT WARRANTY OF
            ANY KIND. IBM DISCLAIMS ALL WARRANTIES, WHETHER EXPRESS
            OR IMPLIED, INCLUDING WITHOUT LIMITATION, THE IMPLIED
            WARRANTIES OF FITNESS FOR A PARTICULAR PURPOSE AND
            MERCHANTABILITY WITH RESPECT TO THE INFORMATION IN THIS
            DOCUMENT. BY FURNISHING THIS DOCUMENT, IBM GRANTS NO
            LICENSES TO ANY PATENTS OR COPYRIGHTS.


        8.2 Note to U.S. Government Users -- Documentation related to
            restricted rights -- Use, duplication or disclosure is
            subject to restrictions set forth in GSA ADP Schedule
            Contract with IBM Corporation.

