				Release Notes

Driver Name  : QLogic PCI Fibre Channel Adapter StorMiniport Driver
Version      : 9.1.1.16
Date         : 11/02/2005
OS platform  : Windows Server 2003
FW version   : 3.03.18 (23xx), 4.00.12 (24xx)

 
Table of Contents
I.   Overview
II.  Enhancements
III. Bug Fixes
IV.  Known Issues
V.   Additional Information
VI.  History
 
I.   Overview

The following document provides details of QLogic's PCI Fibre Channel StorMiniport driver 
changes between version 9.1.1.15 and 9.1.1.16.

II.  Enhancements

None.

III. Bug Fixes

9.1.1.16 QL 3.03.18 4.00.12 - 11/02/05
    *   Close PTR 90818: (For 24XX) Qlogic 4 GB driver returns selection Timeout immediateley after cable pull in an OEM special dual loop configuration.
    *   Close PTR 90652: (For 24XX) Qlogic Driver returns a selection timeout when rebooting a controller in an OEM special dual loop configuration.

IV.  Known Issues

None.

V.   Additional Information

None.


VI.  History

9.1.1.15 QL 3.03.18 4.00.12 - 10/12/05
    *   Close PTR 90818: Qlogic 4 GB driver returns selection Timeout immediateley after cable pull in an OEM special dual loop configuration.
    *   Close PTR 90652: Qlogic Driver returns a selection timeout when rebooting a controller in an OEM special dual loop configuration.

9.1.0.18 QL 3.03.18 4.00.12 - 10/11/05
    *   Added support for the following devices:
            PCI\VEN_1077&DEV_2422&SUBSYS_12D7103C
            PCI\VEN_1077&DEV_2312&SUBSYS_01491077

9.1.0.17 QL 3.03.18 4.00.12 - 09/21/05
    *   RISC code 3.03.18

9.1.0.16 QL 3.03.16 4.00.12 - 08/29/05
    *   Embed 24XX FW in the driver
    *   Close ER43175: New driver could not detect any device to install as BOOT from SAN on 
        one specific setup.  Investigation showed that driver detects the target device successfully but 
        failed the logins because the target had previously been logged in through by the HBA firmware.  
        Driver is changed to handle this particular case correctly.

9.1.0.15 QL 3.03.16 - 08/10/05
    *   Add 24XX support
    *   Close ER42601 - Need to change bit used to control LED mode. 

