ic2400a

              ICOM 2400A MINI REPEATER FUNCTION

1. CUT D9 (MAY NOT BE REQUIRED NOT IN ALL RADIOS)
2. TURN OFF POWER
3. PUSH AND HOLD MONI, MHZ, SET BUTTONS & MIC DOWN BUTTON
4. TURN ON POWER
5. RELEASE ALL BUTTONS

            ICOM 2400A REPEATER FUNCTION CANCELL
1. PUSH AND HOLD SET BUTTON
2. THEN DEPRESS MHZ


                           NOTES:
IF YOUR RIG HAS D9, THE DIODE ABOVE IT WILL EXPAND THE 440
BAND RECIVE IF IT IS CUT ALSO.

TO FIND D9, LOOK AT THE BACK OF THE FACE PLATE INSIDE RADIO
ON LEFT HAND SIDE, YOU SHOULD SEE A VERTICAL LINE OF 7
DIODES, D9 FOR REPEATER IS 2ND FROM THE BOTTOM AND 440
EXPANDED RECIEVE IS THE 3RD ONE FROM THE BOTTOM.  THIS IS
KINDA HARD TO EXPLAIN, AS OF THIS WRITING THERE ARE NO
SERVICE MANUALS AVAILABLE, BUT ICOM WILL SEND YOU THE MOD
WITH A PHOTOCOPY OF THE MOD IF REQUESTED.
CALL GARY FIBER KF7XV, ICOM TECH. CUSTOMER SERVICE REP. AT
PHONE # 206-454-7619, OR FAX AT 206-454-1509.
*END*



