MODIFICATION FOR THE KENWOOD TS-530

----- WARC BANDS

AS SUPPLIED, THE TS-530 WILL RECEIVE BUT NOT TRANSMIT ON THE 
THREE NEW WARC BANDS.  IF TRANSMIT CAPABILITY IS DESIRED,
A MINOR WIRING CHANGE IS REQUIRED.. THERE ARE JUST TWO MINOR CHANGES THAT 
COULD BE MADE AND THEY ARE AS FELLOWS .......

1 --- FOR ALL 3 BANDS . BREAK THE LINE 
BETWEEN THE RF UNIT
X44-1360-01 CONNECTOR #6, PIN #1 (TOP 
TERMINAL) AND 
AF UNIT X49-1150-00, CONNECTOR #7, PIN
#4 (TOP TERMINAL).

2 --- OR, FOR INDIVIDUAL BANDS. ON THE 
RF UNIT X44-1360-01:

BAND          REMOVE/CUT
----------------------------------------
10 MHZ          D4
18 MHZ          D5
24.5 MHZ        D6

I DID THE FIRST MODIFICATION AND
FOUND IT TO BE THE BEST WAY
TO GO, GOOD LUCK AND HAPPY HAMMING !

                    DE KC2AR BOB IN STARRUCCA,PA. 
----------------------------------------------------------------------------
Note: I haven't tried or verified this, proceed at your own risk.  And don't
transmit outside of legal bands!  WA2ISE
