
Scott, here is the new release of TM733A.DOC.  You can also delete the
TM733.MOD file from /pub/hamradio/mods/kenwood because all the info in the
.MOD file is in the .DOC file, but in a more updated and specific format.

Thanks for the great ham radio ftp site.

--
Brad A. Killebrew N5LJV, EMT-B        | Student of Computer Engr Technology
President, University of Houston ARC  |    University of Houston, Texas
Internet: n5ljv@uh.edu                |  U of H Amateur Radio Club  WB5FND
AMPRnet : n5ljv@sugarland.ampr.org    |      uharc@post-office.uh.edu
Packet  : n5ljv@f6cnb.#setx.tx.usa.na | Box 85-T2, 4800 Calhoun, 77204-4083
AT&Tnet : 713-743-6676  Fax 743-4032  | For info, finger tech14c@jetson.uh.edu



-------------------------------- TM733.DOC ----------------------------------


Modifications, Undocumented Features, and Bugs for the Kenwood TM-733A.
Release 2.0   Updated October 1, 1994

Updates for Release 2.0 are identified by parenthetical statements.
There is also some new information sprinkled throughout the previous material
either to update it, to correct misinformation, or to be more specific.

This document is a compilation of Internet messages from 
Steve Haehnichen KE6JGK and Brad Killebrew N5LJV, edited by Brad Killebrew.

------------------------------
Extended RF Modifications
------------------------------

Refer to diagram below. (Inserted into Release 2.0)

Remove power source from the radio.

Remove the display panel.

Remove the top cover the radio. 

Face the front of the radio away from you.

Remove the speaker.

Looking from the back of the radio, the control board is vertically
mounted just behind the front panel wall (which can be removed easily
if better access is needed.)

Just to the right of a chip labeled XRU4066BCF and just to the left of
two green wires (B2 & B3 which are draped over the board to the rear) are 
two zero-ohm SMT resistors, B0 and B1, marked "000".  

Remove B0. (the one on the left - furthest from the green wires)

Taking it out might be a bit tricky.  It's glued down for surface-mount 
assembly.  Be careful not to pull the trace from the board.

Perform a CPU reset by holding [MR] while turning on the radio.  
It will then ask if it is "OK?" to reset, press [MR] again.

The ranges after modification are as follows:

Tx: 136-174 410-470
Rx: 118-174 300-470

The cellular band is indeed missing.  

ONLY Removing Jumper 1 (B2) is the MARS/CAP modification.

** Diagram of specified area on Control Board **

EDGE OF BOARD, viewed from the rear, looking toward front panel

                              Green jumper wires (B2, B3)
     _______        ___     ___     ___     ___     ___
   -|       |-     | _ |   | _ |   |_ _|   |_ _|   |___|
   -| XRU   |-    B0| |   B1| |   B2 |    B3 |
   -| 4066BF|-      |_|     |_|     _|_     _|_     ___
   -|       |-     |___|   |___|   |___|   |___|   |___|
   -|       |-             _______
   -|       |-           -|       |-
   -|_______|-           -|       |-
                         -|       |-
                         -|       |-
                         -|       |-
                         -|       |-
                         -|_______|-

The jumpers are actually soldered on the other side of the board,
but the loops come up over the top and hang over the B0/B1 side.

B0=R414
B1=R412

Here's something interesting!  According the Kenwood rep I spoke to,
performing this mod *does not* void your factory warranty.  The same
goes for any Kenwood published service bulletin or modification info.
We are encouraged to perform the repairs ourselves to save them the
trouble and expence.

------------------------------
DTMF Remote via Microphone
------------------------------

The TM-733 is fully DTMF remotable via the microphone (documented).  
The radio can also be externally DTMF controllable with an HT, but that
will be described later.  

The DTMF control keys are exactly as shown on page 81 of the
manual.  Note that the microphone is active all the time, so any
ambient DTMF tones near your mic will also change rig settings.  This
includes tones coming in on the other band and out the speaker.  

------------------------------
Cross Band Repeating
------------------------------

Cross band repeat isn't documented but comes ready from the factory.  
To enable cross band repeat from the front panel, first select a band 
by pressing BAND SELECT.  Then, change the control to the other band by 
hitting [CONT SEL].  Next, press [F] for one second, then the "X" button 
(far right side).  Decimals will appear between the Kilohertz digits, and 
the "ON" indicator will light momentarily.  The microphone sequence to 
enable cross band repeat while in remote control mode is "DC".  

The transmitter hang time can be toggled between 500ms to 0ms by
turning on the radio with [LOW] pressed.  They also recommend enabling
the Time-out Timer, for obvious reasons.

Note that the TM-733 can also be used as a "one-way" cross-band repeater.
For example, if you can receive a distant repeater with your HT, but have
difficulty getting into it, you can use the TM-733 to boost your transmitted
signal.  To set this up, just omit the part where you "change the control
to the other band by pressing [CONT SEL]."  Doing this will setup the TM-733
to repeat your signal to the other band, but will not retransmit the distant
station back to you. If this sounds ambiguous, play around with it a little 
and it will begin to make sense.


------------------------------
DTMF Paging and Squelch
------------------------------

The DTMF Paging & DTMF Squelch protocol (AAA*BBB) is compatible with
the Yaesu 530 and all Kenwood radios supporting this.  

------------------------------
DTMF Monitor 
------------------------------

There are some serious bugs in the "DTMF Monitor" feature (Page 63:
[PTT] + [DWN] + Power On).  This feature supposedly lets you hear the
DTMF tones you are transmitting.  The first problem is that it only
gives you a short tone from the internal speaker.  This is not true to
the transmitted tone that lasts as long as you hold the key.  The much
bigger problem is that it mixes the desired tone and the feedback tone
resulting in an almost indecodable DTMF tone.  Kenwood is aware of this bug.

(Updated information for Release 2.0):

Per Ricardo, a Kenwood technician, they are aware of this bug and are
working on a fix.  No details yet.


------------------------------
Front Panel
------------------------------

There are two undocumented icons on the display; one is the "heart"
symbol.  Anyone know what that's for?  It could just be a spare.  I
noticed they used the odd "spade" symbol to indicate AM receive, so
maybe these were last minute extras.  Dunno..

From looking at the schematic, it seems that the only programmable
memory is physically located in the detachable front-panel.  I think
this means that if I use my front-panel on someone else's radio, I get
all my memories and settings.  Anyone try this?

The whole front panel is connected to the rig by four wires (yep,
including the volume/squelch pots.)  According to the schematic, these
are: power, ground, data in, and data out.  I'm wondering how hard it
would be to make a PC interface for this thing and replace the whole
display and controls with a full-screen version.  It wouldn't surprise
me if many of the programming limits were also imposed by the
front panel, and not the unit.

------------------------------
Wireless Cloning
------------------------------

The advertised but undocumented Wireless Clone function is described
in App Note AAN-0008 which they will mail out on request.  (Maybe if
enough people ask for it, they will include all the functions in
future instruction manuals.)  In summary:

- Prepare the two radios for simplex operation on the same frequency.
- Turn both radios off
- Press [CALL]+[SHIFT] + [Pwr On].
- This should place the radios is clone mode with "CLonE" on the display.
- Press PTT on the "Master" radio momentarily.  This will start
  sending the programming DTMF tones.
- After all data has been transferred, the display of all radios will
  read "End", indicating success.
- If the signal is interrupted or corrupted, the "Slave" displays will
  read "Err".  Turn them off and try again.

Notes:

- Both the Master and Slave radios must have the same number of
  memory channels available for each band.  Example: You can not clone a
  stock Master to a Slave with ME-1 memory expansion.
- You can not clone between different Kenwood radio models, even if
  they seem identical.

Be careful when using the clone feature.  It has been known to wipe out
or scramble memories on the master radio during or right after clone.


------------------------------
Bugs and Problems
------------------------------

To date, I have logged two trouble reports with Kenwood.  

The first is the well-known problem with the transmitted PL (CTCSS) tone.  
The tones are filthy.  They contain many harmonics and synthesis noise.  
I'm guessing this is because they are using 7-bits from the CPU and a 
resistor net (DAC) to synthesize the tone.  The sound/intensity of the 
noise depends on the actual frequency being generated.  The PL tones also 
come out of the radio's speaker while transmitting. Weird, but not a problem.

The PL noise seems most messed up (on my radio) at 107.2 Hz, where the
noise beats with the tone.  Go simplex and ask someone to describe the
noise to you, or listen carefully to your own speaker while
transmitting.  Some repeaters do a better job than others of hiding
the noise for you.

(New information inserted into r2.0):

=============================
Transmit PL Fix 
=============================

Kenwood just released a Service Bulletin to address the transmitted PL
tone noise on the TM-733A.  (Yeah!!)  Call the Kenwood Service
Dept. (1-310-639-7140) if you want a hardcopy.  Here's a summary of
the text.  Use it at your own risk.  If you are going to get into your
radio with a hot iron, you should first get the real paper from
Kenwood with the drawing.


Kenwood Service Bulletin #ASB-1060        2 Pages
Subject: TM-733A PL Tone Distortion       August 30, 1994

Symptom:
--------
Transmitted PL tones at the receiving station have a relatively high
level of distortion.  This is easily seen when the incoming signal is
viewed on an oscilloscope.

Countermeasure:
---------------
Change the value of the "Pull-up" resistors in the PL tone encoder
circuit as shown in the accompanying chart and illustration.  This
reduces the distortion from around 9% to approximately 4%.

  Part  OLD value  NEW value
  ----  ---------  ---------
  R542  1.8k       2.7k
  R543  1.8k       3.3k
  R544  1.8k       4.7k
  R545  1.8k       6.8k
  R546  1.8k       10k
  R547  1.8k       10k
  R548  1.8k       10k

Procedure:
----------
1. Disconnect the power cable, microphone and antenna's, etc.
2. Detach the front panel and set it aside.
3. Remove the top and bottom covers.
4. Remove the speaker and speaker mounting bracket.
5. Disengage the plastic front panel from the main chassis.
6. Carefully disconnect the two ribbon cables from the Tx/Rx unit C/4.
7. Remove the two Phillips head screws that secure the Tx/Rx unit to
   the chassis.
8. Turn the circuit board over and replace the resistors using the
   parts list and illustration as a guide.
9. Reverse steps 1-7 for reassembly.


     TX-RX Unit (X57-4360-00)     Foil Side View
---------------------------------------------------------------

         
                                R  R  R   R542
                                5  5  5
                                4  4  4   R543
                                7  6  4
                                          R545
   (IC403 on component side)      R
                                  5
                                  4
                                  8       _______
                                        -|       |-
                                        -|       |-
                                        -|       |-
                                        -| IC402 |-
                                        -|       |-
                                        -|       |-
                                        -|_______|-

---------------------------------------------------------------

Caution: This modification requires advanced surface mount soldering
equipment that is rated for CMOS circuits.  It also requires
familiarity with advanced surface mount soldering techniques.  If you
do not have the proper equipment or knowledge do not attempt this
modification yourself.  Seek qualified assistance from your closest
Kenwood Service Center (Long Beach, CA, or Virginia Beach, VA).


The Service Manual specifies a test for the PL.  The technician is
simply required to verify that any one PL tone is between 500 and 1500
Hz deviation.  This is quite a wide tolerance range!  The "standard"
PL tone deviation should be 750 Hz.  Twice that strong might be too
strong and become audible.  There are no trim-pots on the PL
deviation, so I'm guessing that the deviation is pretty constant from
radio to radio.

The dirty PL is definitely found on early models, but we have had many
reports that the PL problem has been fixed in newer versions of the radio.
If you purchased your radio after September 15, 1994, (or your serial number
is greater than 55000000) it's a good chance that you may not have the PL
problem. 

------------

The other problem concerns the DTMF Confirmation Tones.  This feature
is off by default (I wonder why :), while it seems pretty useful.  To
turn it on, press [PTT] + [Down] on the microphone while powering the
radio on.  This will generate short DTMF confirmation tones whenever
you send DTMF over the air from the keypad.  Unfortunately, it mangles
the beginning of the outgoing DTMF tone!  This is serious enough that
most local repeaters can't detect the tone, or count it as two tones.

Get a receiver and listen to what you are sending out when the
Confirmation tones are enabled.  It sounds to me like they may be
mixing the confirmation tone in with the real tone and getting some
destructive interference.  Just a guess, though.

I called a Kenwood technician (Ricardo) and worked with him on the
phone to reproduce the problem there.  So, as of today, this is a
Known Problem, and they are looking into a fix. :-)

I am really curious to know what they would say if other folks called
up and complained about this problem.  Would they deny hearing about
it, or would it really be a Known Problem?  Might give some insight
into the PL-noise denial thing anyway. :-)

Personally, I'm much more concerned about the noisy PL than the DTMF
confirmation tones, since I can just shut those off and pretend that
feature doesn't exist.  If enough people call about the PL problem,
maybe they will come out with a real fix and offer it under warranty
to all the radios out there (since they're all pretty new).  My guess
is that it will involve a free TSU-8 tone decode module, but don't
hold your breath. :-)



------------------------------
External DTMF Remote Control
------------------------------

The following procedure places the 733 in External DTMF Remote Control.

Note that this mode is different than DTMF Remote Mode.  This mode 
concerns the control of the 733 with an HT, and not the microphone.

- Press Band Select and select the UHF band.
- Pick a UHF control frequency.
- Turn on the UHF DTSS function and select a tone sequence. (p. 89)
- Turn the UHF DTSS function back off.
- Press Band Select to move to the VHF band.
- Press [CONT SEL] to move control back to the UHF band.
- Turn OFF the radio, press and hold [CONT SEL] while turning the radio
  back on, then release [CONT SEL].  The S-meter scale and the DT
  indicators for the UHF band will begin flashing.  The LOCK indicator
  will turn ON, and most front-panel keys (except PWR) will be disabled.
- To begin remote control, you should key the external radio and
  press the following key sequence: "Axxx#" where "xxx" is the preset
  DTSS code selected earlier.
- If the proper code is received by the 733, the beeper will sound and
  the DT indicator will stop flashing.  The radio can now be
  remotely controlled using the function chart below.
- To return to standby mode, press "A#" on the remote radio. 
- To return the radio to normal operation, turn the radio off, then
  press and hold [CONT SEL] while turning the radio back on.



Refer to this chart when using the TM-733 in "External DTMF Control".


          1               2               3               A
       T.ALT ON         TONE ON        CTCSS ON         ENTER

          4               5               6               B
       T.ALT OFF        TONE OFF       CTCSS OFF       TONE SEL

          7               8               9               C
         CALL            VFO           MEMORY        REPEATER ON

          *               0               #               D
         DOWN        POWER LEVEL         UP          REPEATER OFF



There are no "shifted" functions.  Just one function per button.
After you hit "B" for TONE SELECT, press * or # to go up or down,
and same is true when in VFO mode or in MEMORY mode.
Tones 7, 8, and 9 mimic the three buttons at the top of the 733 mic.

Pressing "C" places the radio in cross band repeat mode.  You will
recognize this because of the dots between Kilohertz digits.
After pressing "C", put the radio back into standby mode with "A#".
The 733 will now cross band repeat.  To disable cross band repeat, place
the radio back into the External DTMF Remote Control with "Axxx#".
If you can read through the lines, the 733 is capable of operating
as a frequency agile remote base.  Now Kenwood just needs a CW IDer!


------------------------------
Assembly Mode Test
------------------------------

In the TM-733 Service Manual, it describes a test mode that I haven't
seen mentioned anywhere else.  So, here's the scoop:

Entering Assembly Mode:  [CALL] + [MUTE] + [Power On]
All LCD segments should come on.  (To exit, power off.)

Press the [VFO] key.  *This must always be done first*
The serial port is checked and "F" with "80" on the display indicates
test passed.  "1" or "2" means failure.

Different keys now show different displays, with [LOW], [SHIFT],
[TONE], and [REV] also adjusting the backlight intensity.

Set the dials to minimum, then press the [MR] key.  Each of the dials
shows the digitized level.

This looks useful for checking all the keys and dials when you suspect
a bad connection.


-------------------------snip here and print---------------------------------



Kenwood TM-733A Quick Reference Guide by Brad Killebrew N5LJV

-----------------------------------------------------------------------------

[#]                     PRESS A NUMBER, NOT THE POUND SIGN.
[KEY]                   PRESS AND RELEASE [KEY]
[KEY1]+[KEY2]           PRESS AND HOLD [KEY1] DOWN, THEN PRESS [KEY2]
[KEY1],[KEY2]           PRESS [KEY1] MOMENTARILY, THEN PRESS [KEY2]
[KEY]+[PWR]             WITH POWER OFF, PRESS AND HOLD [KEY] THEN HIT [PWR]
[KEY1]+[KEY2]+[PWR]     YOU GET THE IDEA.
[F] (1s)                PRESS AND HOLD [F] FOR ONE SECOND. "F" THEN BLINKS.
[KEY] (1s)              PRESS AND HOLD [KEY] FOR ONE SEOND.
[F],[KEY] (1s)          PRESS [F] MOMENTARILY, THEN PRESS [KEY] FOR ONE SEC.

-----------------------------------------------------------------------------

The following entries are listed in the order as they appear in the manual.

RECEIVE AUDIO SWITCHING                 [F] (1s) [CONT SEL]
AUTOMATIC SQUELCH                       [MHZ] + [PWR]
S-METER SQUELCH                         [F] (1s), [S.QSL]
SQUELCH HANG TIME                       [F]+[DIM]
RD OUTPUT SQUELCH CONTROL               [TONE]+[PWR]
VHF+VHF OPERATION                       [F],[CONT SEL]
UHF+UHF OPERATION                       [F],[CONT SEL]
TRANSMIT BAND LOCK                      [F],[BAND SEL]
BLANKING A BAND DISPLAY                 [F] (1s), [BAND SEL]
VFO TUNING LIMITS                       [F]+[C.IN],(L.FRQ)[MR],(U.FRQ)[MR]
AM/FM MODE                              [MHZ] (1s)
FREQUENCY STEP SIZE                     [VFO],[F],[STEP]
1 MHZ/10 MHZ TUNING TOGGLE              [VFO],[F]+[MHZ]
POWER OUTPUT                            [LOW]
TIME-OUT TIMER                          [F] (1s),[TOT]
WRITING MEMORY (SIMPLEX, DUPLEX)        [F],(FREQ),[MR]                 
WRITING MEMORY (ODD SPLIT)              (RX FRQ),[F],[MR] (1s),(TX FRQ)[MR]
MEMORY TO VFO TRANSFER                  [F],[VFO]
ERASING MEMORY CHANNELS                 [MR],[F]+[MR]
RECALLING MEMORY CALL CHANNEL           [CALL]
CHANGING CALL CHANNEL (SIMPLEX,DUPLEX)  [F],[C.IN]
CHANGING CALL CHANNEL (ODD SPLIT)       (RX FR),[F],[C.IN] (1s),(TX FR)[CALL]
CHANNEL DISPLAY FUNCTION                [REV]+[PRW]
INITIALIZE VFO ONE BAND                 [VFO]+[BAND SEL]+[PWR]
INITIALIZE VFO BOTH BANDS               [VFO]+[PWR]
FULL RESET (MINUS PM)                   [MR]+[PWR],[F],[MR]
FULL RESET (PLUS PM)                    [MR]+[PWR],[MR]
STORING PROGRAMMABLE MEMORY             [F],[PM],[#] 
RECALLING PROGRAMMABLE MEMORY           [PM],[#]
ERASING PROGRAMMABLE MEMORY             [F]+[PM],[#],[MR]
CANCELLING AUTOMATIC OFFET              [VFO]+[REV]+[PWR]
AUTOMATIC SIMPLEX CHECKER               [REV] (1s)
SELECTING A CTCSS TONE FREQUENCY        [F] (1s),[T.SEL],[UP]/[DOWN]
DTMF CONFIRMATION TONES                 [PTT]+[DWN]+[PWR]
STORING DTMF IN AUTOMATIC DIALER        [F]+[CALL]+[PWR],{#'s},[PF],[#]
RECALLING STORED DTMF NUMBERS           [F]+[CALL]+[PWR],[MR],[#]
TRANSMITTING STORED DTMF NUMBERS        [PTT]+[PF],[#]
SCAN RESUME TOGLE (CO, TO)              [F] (1s),[VFO]
MEMORY SCAN                             [MR] (1s)
LOCKING OUT MEMORY CHANNELS             [MR],[F] (1s),[MR]
BAND SCAN                               [VFO] (1s)
PROGRAMMABLE BAND SCAN                  [F]+[VFO],(L.FRQ),[MR],(U.FRQ),[MR]
CONFIRMING PROGRAMMABLE LIMITS          [F]+[VFO],(L.SHOWN),[MR](U.SHOWN)
CALL/VFO SCAN                           [VFO],[CALL] (1s)
CALL/MEMORY SCAN                        [MR],[CALL] (1s)
PROGRAMMABLE MEMORY SCAN                [PM]+[PWR],[PM] (1s)
AUTOMATIC BAND CHANGE (A.B.C.)          [F],[A.B.C.]
ADVNACED INTERCEPT POINT (AIP)          [F]+[A.B.C.]
MUTE                                    [MUTE]
TRANCEIVER LOCK                         [F],[MHZ]
ALL LOCK                                [F],[MHZ],[PWR],[F]+[PWR]
AUTOMATIC POWER OFF (APO)               [F] (1s),[MHZ]
BEEP LOUDNESS                           [F] (1s),[BEEP]
FREQUENCY READOUT BY BEEPS              [F]+[TONE]+[PWR],[PF]
DISPLAY DIMMER                          [F],[DIM]
AUTO DIMMER CHANGE                      [F]+[LOW]+[PWR]
DISPLAY DOMONSTRATION MODE              [CALL]+[PWR]
REMOTE CONTROL MODE                     [F]+[CONT SEL]
CTCSS                                   [TONE],TOGLE TILL "CT" APPEARS
AUTOMATIC TONE FREQUENCY ID             [TONE] (1s)
DUAL TONE SQUELCH SYSTEM (DTSS)         [F],[DTSS]
DUAL TONE SQUELCH SYSTEM (TONE SELECT)  [F] (1s),[C.SEL],[#],[SHIFT],ETC.
TONE ALERT                              [F],[T.ALT]
TONE ALERT - CHANGE TONE                [F]+[SHIFT]+[PWR]
PACKET BAUD RATE TOGLE                  [F]+[STEP]

-----------------------------------------------------------------------------

The following entries are in alphabetical order.

1 MHZ/10 MHZ TUNING TOGGLE              [VFO],[F]+[MHZ]
ADVNACED INTERCEPT POINT (AIP)          [F]+[A.B.C.]
ALL LOCK                                [F],[MHZ],[PWR],[F]+[PWR]
AM/FM MODE                              [MHZ] (1s)
AUTO DIMMER CHANGE                      [F]+[LOW]+[PWR]
AUTOMATIC BAND CHANGE (A.B.C.)          [F],[A.B.C.]
AUTOMATIC OFFET (CANCELLING)            [VFO]+[REV]+[PWR]
AUTOMATIC POWER OFF (APO)               [F] (1s),[MHZ]
AUTOMATIC SIMPLEX CHECKER               [REV] (1s)
AUTOMATIC SQUELCH                       [MHZ] + [PWR]
AUTOMATIC TONE FREQUENCY ID             [TONE] (1s)
BAND SCAN                               [VFO] (1s)
BEEP LOUDNESS                           [F] (1s),[BEEP]
BLANKING A BAND DISPLAY                 [F] (1s), [BAND SEL]
CALL CHANNEL CHANGING (ODD SPLIT)       (RX FR),[F],[C.IN] (1s),(TX FR)[CALL]
CALL CHANNEL CHANGING (SIMPLEX,DUPLEX)  [F],[C.IN]
CALL CHANNEL RECALLING                  [CALL]
CALL/MEMORY SCAN                        [MR],[CALL] (1s)
CALL/VFO SCAN                           [VFO],[CALL] (1s)
CANCELLING AUTOMATIC OFFET              [VFO]+[REV]+[PWR]
CHANGING CALL CHANNEL (ODD SPLIT)       (RX FR),[F],[C.IN] (1s),(TX FR)[CALL]
CHANGING CALL CHANNEL (SIMPLEX,DUPLEX)  [F],[C.IN]
CHANNEL DISPLAY FUNCTION                [REV]+[PRW]
CONFIRMING PROGRAMMABLE LIMITS          [F]+[VFO],(L.SHOWN),[MR](U.SHOWN)
CTCSS                                   [TONE],TOGLE TILL "CT" APPEARS
CTCSS TONE FREQUENCY (SELECTING)        [F] (1s),[T.SEL],[UP]/[DOWN]
DIMMER (AUTO CHANGE)                    [F]+[LOW]+[PWR]
DIMMER (DISPLAY)                        [F],[DIM]
DISPLAY DIMMER                          [F],[DIM]
DISPLAY DOMONSTRATION MODE              [CALL]+[PWR]
DTMF CONFIRMATION TONES                 [PTT]+[DWN]+[PWR]
DTMF IN AUTOMATIC DIALER (STORING)      [F]+[CALL]+[PWR],{#'s},[PF],[#]
DTMF NUMBERS (RECALLING STORED)         [F]+[CALL]+[PWR],[MR],[#]
DTMF NUMBERS (TRANSMITTING STORED)      [PTT]+[PF],[#]
DUAL TONE SQUELCH SYSTEM (DTSS)         [F],[DTSS]
DUAL TONE SQUELCH SYSTEM (TONE SELECT)  [F] (1s),[C.SEL],[#],[SHIFT],ETC.
ERASING MEMORY CHANNELS                 [MR],[F]+[MR]
ERASING PROGRAMMABLE MEMORY             [F]+[PM],[#],[MR]
FREQUENCY READOUT BY BEEPS              [F]+[TONE]+[PWR],[PF]
FREQUENCY STEP SIZE                     [VFO],[F],[STEP]
FULL RESET (MINUS PM)                   [MR]+[PWR],[F],[MR]
FULL RESET (PLUS PM)                    [MR]+[PWR],[MR]
INITIALIZE FULL RESET (MINUS PM)        [MR]+[PWR],[F],[MR]
INITIALIZE FULL RESET (PLUS PM)         [MR]+[PWR],[MR]
INITIALIZE VFO BOTH BANDS               [VFO]+[PWR]
INITIALIZE VFO ONE BAND                 [VFO]+[BAND SEL]+[PWR]
LOCK (ALL)                              [F],[MHZ],[PWR],[F]+[PWR]
LOCK (TRANCEIVER)                       [F],[MHZ]
LOCK (TRANSMIT BAND)                    [F],[BAND SEL]
LOCKING OUT MEMORY CHANNELS             [MR],[F] (1s),[MR]
MEMORY CHANNELS (LOCKING OUT)           [MR],[F] (1s),[MR]
MEMORY ERASING CHANNELS                 [MR],[F]+[MR]
MEMORY RECALLING CALL CHANNEL           [CALL]
MEMORY SCAN                             [MR] (1s)
MEMORY TO VFO TRANSFER                  [F],[VFO]
MEMORY WRITING (ODD SPLIT)              (RX FRQ),[F],[MR] (1s),(TX FRQ)[MR]
MEMORY WRITING (SIMPLEX, DUPLEX)        [F],(FREQ),[MR]                 
MUTE                                    [MUTE]
PACKET BAUD RATE TOGLE                  [F]+[STEP]
POWER OUTPUT                            [LOW]
PROGRAMMABLE BAND SCAN                  [F]+[VFO],(L.FRQ),[MR],(U.FRQ),[MR]
PROGRAMMABLE LIMITS (CONFIRMING)        [F]+[VFO],(L.SHOWN),[MR](U.SHOWN)
PROGRAMMABLE MEMORY (ERASING)           [F]+[PM],[#],[MR]
PROGRAMMABLE MEMORY (RECALLING)         [PM],[#]
PROGRAMMABLE MEMORY (STORING)           [F],[PM],[#] 
PROGRAMMABLE MEMORY SCAN                [PM]+[PWR],[PM] (1s)
RD OUTPUT SQUELCH CONTROL               [TONE]+[PWR]
RECALLING MEMORY CALL CHANNEL           [CALL]
RECALLING PROGRAMMABLE MEMORY           [PM],[#]
RECALLING STORED DTMF NUMBERS           [F]+[CALL]+[PWR],[MR],[#]
RECEIVE AUDIO SWITCHING                 [F] (1s) [CONT SEL]
REMOTE CONTROL MODE                     [F]+[CONT SEL]
S-METER SQUELCH                         [F] (1s), [S.QSL]
SCAN (BAND SCAN)                        [VFO] (1s)
SCAN (CALL/MEMORY)                      [MR],[CALL] (1s)
SCAN (CALL/VFO)                         [VFO],[CALL] (1s)
SCAN (PROGRAMMABLE BAND SCAN)           [F]+[VFO],(L.FRQ),[MR],(U.FRQ),[MR]
SCAN (PROGRAMMABLE MEMORY)              [PM]+[PWR],[PM] (1s)
SCAN MEMORY                             [MR] (1s)
SCAN RESUME TOGLE (CO, TO)              [F] (1s),[VFO]
SELECTING A CTCSS TONE FREQUENCY        [F] (1s),[T.SEL],[UP]/[DOWN]
SQUELCH (AUTOMATIC)                     [MHZ] + [PWR]
SQUELCH (RD OUTPUT CONTROL)             [TONE]+[PWR]
SQUELCH (S-METER)                       [F] (1s), [S.QSL]
SQUELCH HANG TIME                       [F]+[DIM]
STORING DTMF IN AUTOMATIC DIALER        [F]+[CALL]+[PWR],{#'s},[PF],[#]
STORING PROGRAMMABLE MEMORY             [F],[PM],[#] 
TIME-OUT TIMER                          [F] (1s),[TOT]
TONE ALERT                              [F],[T.ALT]
TONE ALERT - CHANGE TONE                [F]+[SHIFT]+[PWR]
TRANCEIVER LOCK                         [F],[MHZ]
TRANSMIT BAND LOCK                      [F],[BAND SEL]
TRANSMITTING STORED DTMF NUMBERS        [PTT]+[PF],[#]
UHF+UHF OPERATION                       [F],[CONT SEL]
VFO TUNING LIMITS                       [F]+[C.IN],(L.FRQ)[MR],(U.FRQ)[MR]
VHF+VHF OPERATION                       [F],[CONT SEL]
WRITING MEMORY (ODD SPLIT)              (RX FRQ),[F],[MR] (1s),(TX FRQ)[MR]
WRITING MEMORY (SIMPLEX, DUPLEX)        [F],(FREQ),[MR]                 
-----------------------------------------------------------------------------
-----------------------------------------------------------------------------

If you have additions or corrections to this file, please send it to
Brad Killebrew N5LJV at n5ljv@uh.edu, or packet n5ljv@f6cnb.#setx.tx.usa.na.

Standard Disclaimer:  The authors take absolutely no responsibility for
the material presented in this document.  The procedures contained herein 
work on the author's radios, but proceed at your own risk.

