Kenwood TR751

Here is a easy to do mod for you that are tired of the 5 KHz stepping
in the SSB/CW mode.

1. Remove the top and bottom covers of your radio, be careful not to
   damage the speaker Pcb-plug/connecting cables.

2. Remove the FOUR screws holding the FRONT-panel.

3. Carefully pull the front out of its position and fold it aside.

4. The pcb where the front panel connectors are placed is our target.

5. Locate the 3 to 4 rows of diodes in one of the pcbs corners.

6. Locate diode D16, cut it and separate the leads.

7. Check to see that your dial now is stepping in 1 KHz increments.

8. Asseble your radio again, please check that all leads are un-squeezed.

This mod make contesting and life much easier than b4..eh ?.
Please note that there MAY be other revisions that differ compared to
the radios i have been working with, so i take NO responsability
what so ever, but it SHOULD work.

These mods are based on articles from Ron (SM3MZY) and Pino (IK7ETH)



 