Special "MODIFICATION-/CONFIGURATION" Information for "PRESIDENT JAMES & PRESIDENT GEORGE" transceivers !!!

Special

"Configuration-Modifications"

President George

AM/FM/USB/LSB

@DréCB/T&R@

cbradio@vizzavi.nl

PRESIDENT GEORGE

Modification Configurations

# DIMMER key is used for BAND select

# SELECT is used to allow you go UP or DOWN "5 Kc." (together with UP/DWN channel keys

Reset "Access-Code"

# Press PWR + NB/ANL & PROGRAM and KEEP PRESSED DOWN till

Display LIT OFF

# RELEASE ONLY PWR and KEEP PRESSED NB/ANL + PROGRAM

"Code" flashes in Display, wait for "Code" disappear

# RELEASE NB/ANL + PROGRAM

# PUSH MODE one time

# PUSH M1 one time

# PUSH M3 one time

# PUSH PROGRAM one time

# PUSH PROGRAM 4 times

# PUSH PWR

Configuration Modifications

# Turn transceiver ON by pushing POWER

# Turn transceiver OFF by pushing POWER

# Press POWER and KEEP PRESSED DOWN

Transceiver goes ON and then goes OFF

# Keep POWER PRESSED and PRESS PA & DIMMER simultaneously

# RELEASE POWER after 5 secs. KEEPING PA + DIMMER pressed down; "Code" flashes in Display for 5 secs.

# "Code" disappears and Display lits up

# RELEASE now PA + DIMMER

.....now Press (your choise...)

________________

# M1

for 240 channel FM/AM/SSB 20 watt AM/FM & ± 40 watt SSB

(Internat. config.)

Display goes OFF*

# M2

for 40 channel FM 4 watt and channel 4 - 15 = AM 4 watt

(German config.)

Display goes OFF*

# M3

for 40 channel FM CEPT

("Normal" config.)

Display goes OFF*

# MODE

for 40 channel FM 4 watt

(Britain + Poland config.)

Display goes OFF*

# PROG

for 40 channel AM/FM/SSB 4 watt

(French standard config.)

Display goes OFF*

________________

* = Enter now "Your Access Code" ( 4 x PROGRAM), then press POWER

Your transceiver is modified with the new configuration!

For More "Specific-" President James- or George Information:

http://www.geocities.com/dre_cb/presiden.htm

@DréCB/T&R@