# President Herbert CB-Radio

## ALIGNMENT PROCEDURE

### CARRIER OSCILLATOR PORTION

Test equipment required:

Power Supply: 13,8 V | Oscilloscope | Dummy Load 50 ohm | Frequency Counter

Preparation alignment:

Channel: | 40

Step | Condition | Adjustment | Procedure
--- | --- | --- | ---
1 | RX Band C Channel 20 | L701 | Connect DC-Voltmeter to TP1. Adjust for 2,4Volt +/-0,1Volt
2 | TX Band C Channel 20 | L702 | Connect DC-Voltmeter to TP1. Adjust for 2,4Volt +/-0,1Volt
3 | RX Band C Channel 20 | CT701 | Connect Frequency Counter to TP 3. Adjust for 37.900MHz