VOLTAGE CHART

Realistic TRC453
Documentation Project
CBTricks.com
Voltage Chart

Symbol No. | T/RX | Base Gate | Collector Drain | Emitter Source
TR1 | RX NB ON | 0.8 | 5.3 | 0
TR2 | RX NB ON | 0.8 | 2.6 | 0
TR3 | RX NB ON | 2.6 | 6.8 | 1.9
TR4 | RX NB ON | 0.8 | 7.2 | 0.2
TR5 | RX NB ON | 0.4 | 1.3 | 0.9
TR6 | RX NB ON | 6.6 | 0 | 7.2
TR7 | RX NB ON | 0 | 0 | 0
TR8 | RX | 0.4 | 8.1 | 0
TR9 | RX SSB | 0.7 | 0 | 0
TR10 | RX | 0.7 | 0 | 0
TR11 | RX | 1.6 | 4.7 | 1
TR12 |  | 0 0.7 | 0 0 | 0 0
TR13 | RX | 2.1 | 6.8 | 1.4
TR14 | RX | 0 | 6.5 | 2.8
TR15 | RX | 1.5 | 8 | 0.7
TR16 | RX | 0.7 | 3.3 | 0
TR17 | RX | 3.3 | 6.3 | 2.6
TR18 | RX | 2.6 | 6.4 | 1.8
TR19 | RX AM SSB | 0.7 0 | 0 3 | 0 6
TR20 | RX TX | 0.7 | 5.7 | 0.5
TR21 | RX TX | 3 | 6.9 | 2.5
TR22 | RX TX | 0.7 | 4.4 | 0
TR23 | RX TX | 4.3 | 5.6 | 3.6
TR24 | RX TX | 0.4 2.9 | 0.5 6.8 | 0 2.3
TR25 | TX | 1.7 | 3.2 | 1
TR26 | TX | 0.8 | 1.7 | 0.3
TR27 | TX | 0.6 | 0 | 0
TR28 | TX | 7.5 | 1.3 | 8
TR29 | TX | 1.1 | 7.5 | 4.4
TR30 | PA | 2.4 | 4.6 | 1.8
TR31 | RX TX | 7.8 0.2 | 8 8.1 | 7.2 0.7
TR32 | RX TX | 4.9 0.8 | 7.8 0.2 | 4.7 0
TR33 | RX TX | 8 8.1 | 0 7.9 | 7.9 7.3
TR34 | RX SSB | 0 | 7.5 | 1.4
TR35 | TX | 1.3 | 7.9 | 0.6
TR36 | TX | 5.6 | 12.3 | 5.1
TR37 | TX | 13 | 5 | 12.3
TR38 | TX AM SSB | 0 0.7 | 13.1 0 | 0 0
TR538 | TX AM SSB | 0.5 0.6 | 5 13.5 | 0 0
TR539 | TX AM SSB | 0.7 0.7 | 5 13.6 | 0 0
TR544 | TX AM SSB | 13 13 | 5 13.6 | 13.8 13.9

Measurement Conditions:
Power supply voltage: 13.8V
Test equipment: Digital voltmeter
Measurement channel: 19
Unless otherwise specified, set controls as follows:
MODE: AM
SQ: MIN
ANL/NB: OFF
RF GAIN: MAX.
CLARIFIER: CENTER

Copyright © 1998,1999,2000, 2001 CBTricks.com

Disclaimer: Although the greatest care has been taken while compiling these documents,

we cannot guarantee that the instructions will work on every radio presented.